MACT Floor Comparison

Description	Number of affected sources	No. of MACT floor facilities	MACT floor "median" limit (lb HAP/ gal solids)
All facilities

(no subcategories)	157	20	0.41
All facilities

(without EGBE)	~129	16	0.25
Without 2-Pc beer/beverage facilities	96	12	0.34
Without 2-Pc beer/beverage facilities and without EGBE	~59	7	0.32