{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Background and Instructions ","Manhole Inspection","MH Summary"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Background and Instructions ","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Manhole Inspection","index":1,"n_rows":53,"n_cols":9,"rows_kept":53,"cut":false,"hidden":false,"merged":[[5,7,5,8],[8,7,8,8]]}
[]
[]
[null,null,null,null,null,null,null,null,"Manhole ID:"]
[" "]
[" "]
[" ",null,"Inspection Date:",null,"2015-06-11"," ",null,"Overall Rating (1 to 5):"]
[" ",null,"Inspector: ",null,null,null,null,null,"(1=new ... 5=failing)"]
[null,null,"Street Name:"]
[null,null,"Nearest Address #:",null,null,null,null,"Inflow Infiltration Rate:"]
[null,null,"Manhole Depth:",null,null,null,null,null,"(0=none … 5=gusher)"]
[]
["Conditions:",null,"Dry",null,"Wet",null,"Standing Water",null,"Frozen"]
[]
["MH DETAILS"]
["Location:"," ","Material:",null,"MH Cover size:",null,"MH Barrel size: ",null,"Direction Effluent:"]
["Roadway",null,"Brick",null,"22\"",null,"48\"",null,"(N, NE, E, SE, S, SW, W, NW)"]
["Gutter",null,"Block",null,"24\"",null,"60\""]
["Paved Alley",null,"Concrete",null,"30\"",null,"Other (below)",null,"# of Influents: "]
["Unpaved Alley",null,"Lined",null,"36\""]
["Easement",null,"Other",null,"Other (describe)"]
["Other (describe)"]
[]
["CONDITION"]
["Cover:",null,"Ring &Frame",null,"Cone & Riser:",null,"Barrel:",null,"Rungs:"]
["Serviceable",null,"Serviceable",null,"Serviceable",null,"Serviceable",null,"Serviceable"]
["Loose",null,"Loose",null,"Cracked/Broken",null,"Cracked/Broken",null,"Unsafe"]
["Below Grade",null,"Displaced",null,"Corroded",null,"Corroded",null,"Missing any"]
["Damaged",null,"Missing Grout",null,"Misaligned",null,"Misaligned",null,"Corroded"]
["Sealed",null,"Raise",null,"Infiltration",null,"Infiltration",null,"N/A - no rungs "]
["Holes  (# of holes)",null,"Lower",null,"Roots at Joints",null,"Roots at Joints"]
[]
["Bench:",null,"Channel:"]
["Serviceable",null,"Serviceable"]
["Cracked/Broken",null,"Obstructed"]
["Bad base joint",null,"Bad joints"]
[" ",null,"Roots at connection"]
[]
[]
["Hydraulics",null,"Indications of Surcharge?:",null,"Issues:",null,null,null,"Describe Flow:"]
[null,null,"None",null,"Grease",null,null,null,"Steady"]
[null,null,"Minor",null,"Debris",null,null," ","Pulsing"]
[null,null,"Yes,  need followup",null,"Silt",null,null,null,"Turbulent"]
[null,null,null,null,"Infiltration, if yes, note below ",null,null,null,"Surcharging"]
[null,null,null,null,"(None, Minor, Some, Excessive)",null,null,null,"Sluggish"]
[]
[null,null,"COMMENTS:"]
[]
[]
[]
[]
[]
[]
[null,null," "]

{"sheet":"MH Summary","index":2,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
["SUMMARY of Inspections:"]
[]
["DATE","MH ID","Location","Condition","I and I","COMMENTS"]
["Data Summary:"]
["2015-06-11","1-1","Main St",4,4,"Infiltration through chimney"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["x"]