{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Pb_Min_Tests","Pb_Variability","Pb_New_Sub1UPL Pooled Template ","Pb_QA_Calcs","ERT","4078_PartII"],"not_rendered":{"charts":0,"images":11,"macros":0,"external_links":0,"defined_names":18,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Pb_Min_Tests","index":0,"n_rows":747,"n_cols":59,"rows_kept":747,"cut":false,"hidden":false,"merged":[]}
["Key","primary_fuel","Pb_Min_lb_per_MWh_Rank","Reason_for_Removal","ORIS code","Plant Name","State","Unit Number","boiler_id","Unit Type","boiler_type","MWe_capacity","max_heat_input","Unit_heat_rate","Fuel types","fuel","Lead_Fuel_lb/MMBtu","Lead - ERT","Lead MW - ERT","Lead - Part II","Lead MW - Part II","Lead - min","Lead MW - min","control_group_1","control_type_1","install_date_1","control_group_2","control_type_2","install_date_2","control_group_3","control_type_3","install_date_3","control_group_4","control_type_4","install_date_4","control_group_5","control_type_5","install_date_5","control_group_6","control_type_6","install_date_6","control_group_7","control_type_7","install_date_7","control_group_8","control_type_8","install_date_8","control_group_9","control_type_9","install_date_9","control_group_10","control_type_10","install_date_10","control_group_11","control_type_11","install_date_11","control_group_12","control_type_12","install_date_12"]
[{"$f":"E2&\"_\"&I2","v":"4078_4"},"coal",1,null,4078,"Weston","WI","W4","4","Conventional Boiler","Wall firing - opposed firing",574.5,5173.07,9.0044734551784149,"subbituminous","subbituminous",2.454099454534114E-4,9.9561881881283049E-8,8.9650232254762201E-7,1.5466666666666668E-6,1.3926918944009283E-5,9.9561881881283049E-8,8.9650232254762201E-7,"NOx control","Selective Catalytic Reduction","2008-07-01","Other control","Activated carbon injection","2008-07-01","SO2 control","Dry FGD - Spray Dryer","2008-07-01","PM control","Fabric Filter, pulse","2008-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2324_1","coal",2,null,2324,"Reid Gardner","NV","1","1","Conventional Boiler","Wall firing - front firing",111,1215,10.945945945945946,"bituminous","bituminous",2.2500591115079296E-4,9.0550520926906308E-8,9.911611074431636E-7,null,null,9.0550520926906308E-8,9.911611074431636E-7,"PM control","Fabric Filter, pulse","2008-12-01","SO2 control","Wet FGD - Venturi Type","1976-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["963_34","coal",3,null,963,"Dallman","IL","34","34","Conventional Boiler","Wall firing - opposed firing",229.4,1924.9,8.3910200523103757,"bituminous","bituminous",3.1502965559980235E-4,2.2999999999999999E-7,1.9299346120313865E-6,1.36E-7,1.1411787271142112E-6,1.36E-7,1.1411787271142112E-6,"NOx control","Selective Catalytic Reduction","2009-05-01","PM control","Fabric Filter, pulse","2009-05-01","SO2 control","Wet FGD - Packed Type","2009-05-01","Other control","Wet electrostatic precipitator","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6761_101","coal",4,null,6761,"Rawhide","CO","Rawhide101","101","Conventional Boiler","Tangential firing",305,2800,9.1803278688524586,"subbituminous","subbituminous",2.3104167321457886E-4,1.3236249390726807E-7,1.2151310916077068E-6,null,null,1.3236249390726807E-7,1.2151310916077068E-6,"SO2 control","Dry FGD - Spray Dryer","1984-04-01","PM control","Fabric Filter, reverse air","1984-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["602_2","coal",5,null,602,"Brandon Shores","MD","002","2","Conventional Boiler","Wall firing - unspecified",690,6700,9.7101449275362324,"bituminous","bituminous",4.1984093149244529E-4,1.4170611592242315E-7,1.3759869227249785E-6,null,null,1.4170611592242315E-7,1.3759869227249785E-6,"NOx control","Selective Catalytic Reduction",null,"PM control","Electrostatic precipitator, hot side, unspecified",null,"Other control","Activated carbon injection",null,"Other control","Other (specify): lime injection",null,"PM control","Fabric Filter, unspecified",null,"SO2 control","Wet FGD - Unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10043_B01","coal",6,null,10043,"Logan Generating Plant","NJ","Unit1","B01","Conventional Boiler","Wall firing - opposed firing",241.7,2116,8.7546545304095993,"bituminous","bituminous",5.1281435359843493E-4,1.8498897230757785E-7,1.6195145444883523E-6,4.4100000000000008E-5,3.8608026479106339E-4,1.8498897230757785E-7,1.6195145444883523E-6,"NOx control","Selective Catalytic Reduction","1994-09-01","SO2 control","Dry FGD - Spray Dryer","1994-09-01","PM control","Fabric Filter, reverse air","1994-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["891_Boiler 9","coal",7,null,891,"Havana","IL","Boiler 9","Boiler 9","Conventional Boiler","Wall firing - unspecified",481,5030,10.457380457380458,"bituminous","bituminous",2.3538626238568642E-4,1.5554931996104345E-7,1.6266384187194357E-6,null,null,1.5554931996104345E-7,1.6266384187194357E-6,"PM control","Electrostatic precipitator, hot side, unspecified","1978-04-01","NOx control","Selective Catalytic Reduction","2003-08-01","Other control","Activated carbon injection","2009-07-01","SO2 control","Dry FGD - Spray Dryer",null,"PM control","Fabric Filter, unspecified","2009-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3845_BD21","coal",8,null,3845,"TransAlta Centralia Generation","WA","BW21CONFIG","BD21","Conventional Boiler","Tangential firing",603,7743,12.840796019900498,"subbituminous","subbituminous",3.6646426146838752E-4,1.2895774185617486E-7,1.6559200583621261E-6,null,null,1.2895774185617486E-7,1.6559200583621261E-6,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-01-01","SO2 control","Wet FGD - Spray Type","2002-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2408_E1","coal",9,null,2408,"PSEG Mercer Generating Station","NJ","MERU1E1PT1OS1-Coal","E1","Conventional Boiler","Wall firing - unspecified",343,3100,9.037900874635568,"bituminous","bituminous",9.5074331255700674E-4,1.8878896062676965E-7,1.7062559123702212E-6,5.3333333333333334E-7,4.8202137998056365E-6,1.8878896062676965E-7,1.7062559123702212E-6,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1994-05-01","NOx control","Selective Catalytic Reduction","2004-06-01","Other control","Activated carbon injection","2007-01-01","PM control","Fabric Filter, pulse","2008-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10673_BLR B","coal",10,null,10673,"AES Hawaii","HI","002","BLR B","Fluidized bed firing","Fluidized bed firing",101.5,944.2,9.3024630541871929,"bituminous","bituminous",3.515252746376491E-4,1.8823205922902722E-7,1.7510217765916011E-6,null,null,1.8823205922902722E-7,1.7510217765916011E-6,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Fabric Filter, unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1082_4","coal",11,null,1082,"Walter Scott Jr. Energy Center","IA","4","4","Conventional Boiler","Wall firing - unspecified",850,7675,9.0294117647058822,"subbituminous","subbituminous",2.620154396735339E-4,1.420508740800985E-6,1.2826358336055953E-5,1.9999999999999999E-7,1.8058823529411763E-6,1.9999999999999999E-7,1.8058823529411763E-6,"NOx control","Selective Catalytic Reduction","2007-02-01","Other control","Activated carbon injection","2007-02-01","SO2 control","Dry FGD - Circulating Dry Scrubber","2007-02-01","PM control","Fabric Filter, pulse","2007-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["113_4","coal",12,null,113,"Cholla","AZ","004","4","Conventional Boiler","Tangential firing",425,4268,10.042352941176471,"bituminous","bituminous",6.032663017808556E-4,1.8284497621474502E-7,1.8361937846694866E-6,null,null,1.8284497621474502E-7,1.8361937846694866E-6,"PM control","Fabric Filter, unspecified","2008-01-01","SO2 control","Wet FGD - Packed Type","2008-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10566_Boil 2","coal",13,null,10566,"Chambers Cogeneration LP","NJ","Boil 2","Boil 2","Conventional Boiler","Wall firing - front firing",142.5,1387,9.7333333333333325,"bituminous","bituminous",2.861435068229562E-4,1.997125060274261E-7,1.9438683920002806E-6,null,null,1.997125060274261E-7,1.9438683920002806E-6,"NOx control","Selective Catalytic Reduction","1994-03-01","SO2 control","Dry FGD - Spray Dryer","1994-03-01","PM control","Fabric Filter, reverse air","1994-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2706_1","coal",14,null,2706,"Asheville Steam Electric Plant","NC","Ash_Cfg_1d","1","Conventional Boiler","Wall firing - front firing",207,1914,9.2463768115942031,"bituminous","bituminous",3.5846887046174595E-4,4.029236022004867E-6,3.7255834522305875E-5,2.1842222222222225E-7,2.0196141706924317E-6,2.1842222222222225E-7,2.0196141706924317E-6,"NOx control","Selective Catalytic Reduction","2007-06-14","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2005-11-17","SO2 control","Wet FGD - Spray/Tray Type","2005-11-17","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2706_2","coal",15,null,2706,"Asheville Steam Electric Plant","NC","Ash_Cfg_2","2","Conventional Boiler","Wall firing - front firing",204,1902,9.3235294117647065,"bituminous","bituminous",3.404554580670135E-4,2.1983216160725487E-7,2.0496116243970527E-6,4.3100000000000003E-7,4.0184411764705884E-6,2.1983216160725487E-7,2.0496116243970527E-6,"NOx control","Selective Catalytic Reduction","2006-06-14","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1971-05-01","SO2 control","Wet FGD - Spray/Tray Type","2006-05-15","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7210_COP1","coal",16,null,7210,"Cope","SC","COP001","COP1","Conventional Boiler","Tangential firing",441,4059.1,9.2043083900226748,"bituminous","bituminous",5.3519694279551954E-4,2.3286049698252503E-7,2.1433198260811051E-6,null,null,2.3286049698252503E-7,2.1433198260811051E-6,"NOx control","Selective Catalytic Reduction","2009-01-01","SO2 control","Dry FGD - Spray Dryer","1993-04-01","PM control","Fabric Filter, unspecified","1993-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6021_C2","coal",17,null,6021,"Craig","CO","C2","C2","Conventional Boiler","Wall firing - opposed firing",456,4269,9.3618421052631575,"subbituminous","subbituminous",2.7366218384740278E-4,2.3490934304688269E-7,2.1991841786560135E-6,null,null,2.3490934304688269E-7,2.1991841786560135E-6,"PM control","Fabric Filter, pulse","2004-05-01","SO2 control","Wet FGD - Spray Type","1979-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50888_BLR1","coal",18,null,50888,"Northampton Generating Company, L.P.","PA","GEN1","BLR1","Fluidized bed firing","Fluidized bed firing",121,1146,9.4710743801652892,"coal refuse (culm or gob)","coal refuse (culm or gob)",7.8646543729002562E-3,2.4466524071860208E-7,2.3172426930869253E-6,1.0549809744514062E-6,9.9918032786885252E-6,2.4466524071860208E-7,2.3172426930869253E-6,"NOx control","Selective Noncatalytic Reduction","1995-08-01","PM control","Fabric Filter, pulse","1995-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10671_2a","coal",19,null,10671,"AES Shady Point,LLC","OK","Unit 2","2a","Fluidized bed firing","Fluidized bed firing",80,1110.4350359049981,13.880437948812476,"bituminous,  subbituminous","bituminous,  subbituminous",4.4618841124650265E-4,1.7941858859895406E-7,2.4904085859112952E-6,null,null,1.7941858859895406E-7,2.4904085859112952E-6,"PM control","Fabric Filter, pulse","1991-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10671_2b","coal",20,null,10671,"AES Shady Point,LLC","OK","Unit 2","2b","Fluidized bed firing","Fluidized bed firing",80,1110.4350359049981,13.880437948812476,"bituminous,  subbituminous","bituminous,  subbituminous",4.4618841124650265E-4,1.7941858859895406E-7,2.4904085859112952E-6,null,null,1.7941858859895406E-7,2.4904085859112952E-6,"PM control","Fabric Filter, pulse","1991-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10671_1b","coal",21,null,10671,"AES Shady Point,LLC","OK","Unit 1","1b","Fluidized bed firing","Fluidized bed firing",80,1110.4350359049981,13.880437948812476,"bituminous,  subbituminous","bituminous,  subbituminous",4.4618841124650265E-4,1.7941858859895406E-7,2.4904085859112952E-6,null,null,1.7941858859895406E-7,2.4904085859112952E-6,"PM control","Fabric Filter, pulse","1991-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10671_1A","coal",22,null,10671,"AES Shady Point,LLC","OK","Unit 1","1A","Fluidized bed firing","Fluidized bed firing",80,1110.4350359049981,13.880437948812476,"bituminous,  subbituminous","bituminous,  subbituminous",4.4618841124650265E-4,1.7941858859895406E-7,2.4904085859112952E-6,null,null,1.7941858859895406E-7,2.4904085859112952E-6,"PM control","Fabric Filter, pulse","1991-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6041_4","coal",23,null,6041,"H L Spurlock Station","KY","Unit 04","4","Fluidized bed firing","Fluidized bed firing",300,2800,9.3333333333333339,"bituminous","bituminous",5.0351108265786319E-4,3.3250851180878836E-6,3.1034127768820251E-5,2.67E-7,2.492E-6,2.67E-7,2.492E-6,"NOx control","Selective Noncatalytic Reduction","2009-04-01","SO2 control","Dry FGD - Unspecified","2009-04-01","PM control","Fabric Filter, pulse","2009-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10675_B","coal",24,null,10675,"AES Thames","CT","B","B","Fluidized bed firing","Fluidized bed firing",104,1002,9.634615384615385,"bituminous","bituminous",null,null,null,2.7066666666666666E-7,2.6077692307692307E-6,2.7066666666666666E-7,2.6077692307692307E-6,"SO2 control","Dry FGD - Circulating Dry Scrubber","1990-03-01","PM control","Fabric Filter, pulse","1990-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10673_BLR A","coal",25,null,10673,"AES Hawaii","HI","001","BLR A","Fluidized bed firing","Fluidized bed firing",101.5,1021.4,10.063054187192119,"bituminous","bituminous",4.395406436144504E-4,2.5955489457731445E-7,2.6119149686824532E-6,null,null,2.5955489457731445E-7,2.6119149686824532E-6,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Fabric Filter, unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6077_2","coal",26,null,6077,"Gerald Gentleman","NE","U2","2","Conventional Boiler","Wall firing - opposed firing",750,7538,10.050666666666666,"bituminous","bituminous",1.6588807422668179E-4,2.6401850360332862E-7,2.6535619735491881E-6,null,null,2.6401850360332862E-7,2.6535619735491881E-6,"PM control","Fabric Filter, reverse air","2001-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["56068_1","coal",27,null,56068,"Elm Road Generating Station","WI","ERGS-B1","1","Conventional Boiler","Wall firing - unspecified",677,6515,9.6233382570162487,"bituminous","bituminous",3.2042107567908847E-4,2.7918708784059832E-7,2.6867117832813857E-6,null,null,2.7918708784059832E-7,2.6867117832813857E-6,"NOx control","Selective Catalytic Reduction","2009-10-01","PM control","Fabric Filter, pulse","2009-10-01","SO2 control","Wet FGD - Spray Type","2009-10-01","Other control","Wet electrostatic precipitator","2009-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10566_Boil 1","coal",28,null,10566,"Chambers Cogeneration LP","NJ","Boil 1","Boil 1","Conventional Boiler","Wall firing - front firing",142.5,1387,9.7333333333333325,"bituminous","bituminous",2.8525088996096031E-4,2.7616506516602757E-7,2.6880066342826681E-6,null,null,2.7616506516602757E-7,2.6880066342826681E-6,"NOx control","Selective Catalytic Reduction","1994-03-01","SO2 control","Dry FGD - Spray Dryer","1994-03-01","PM control","Fabric Filter, reverse air","1994-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6639_G2","coal",29,null,6639,"R D Green","KY","2","G2","Conventional Boiler","Wall firing - opposed firing",239,2726.6,11.40836820083682,"bituminous,  Petroleum coke","bituminous,  Petroleum coke",3.4842899163277217E-4,2.3580828240058494E-7,2.6901877104327819E-6,null,null,2.3580828240058494E-7,2.6901877104327819E-6,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1981-01-01","SO2 control","Wet FGD - Spray Type","1981-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["641_5","coal",30,null,641,"Crist","FL","Unit 5","5","Conventional Boiler","Tangential firing",82,817.82999999999993,9.9735365853658529,"bituminous","bituminous",1.8702034199257133E-3,2.71535326023767E-7,2.7081675083172846E-6,null,null,2.71535326023767E-7,2.7081675083172846E-6,"NOx control","Selective Noncatalytic Reduction","2006-04-01","PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","2008-03-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-01-01","SO2 control","Wet FGD - Spray Type","2009-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["641_6","coal",31,null,641,"Crist","FL","Unit 6","6","Conventional Boiler","Wall firing - front firing",320,3193.348,9.9792124999999992,"bituminous","bituminous",1.8702034199257133E-3,2.71535326023767E-7,2.7097087196479506E-6,null,null,2.71535326023767E-7,2.7097087196479506E-6,"NOx control","Selective Noncatalytic Reduction","2005-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1994-01-01","SO2 control","Wet FGD - Spray Type","2009-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2408_E2","coal",32,null,2408,"PSEG Mercer Generating Station","NJ","MERU2E2PT2OS1-Coal","E2","Conventional Boiler","Wall firing - unspecified",343,3100,9.037900874635568,"bituminous","bituminous",6.4473909032057206E-4,3.0276816984340694E-7,2.7363887070395378E-6,5.3333333333333334E-7,4.8202137998056365E-6,3.0276816984340694E-7,2.7363887070395378E-6,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1991-08-01","NOx control","Selective Catalytic Reduction","2004-06-01","Other control","Activated carbon injection","2007-01-01","PM control","Fabric Filter, pulse","2008-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8223_4","coal",33,null,8223,"Springerville","AZ","4","4","Conventional Boiler","Wall firing - opposed firing",450,4200,9.3333333333333339,"bituminous","bituminous",1.681099761320986E-4,3.530335021164723E-7,3.2949793530870752E-6,2.9999999999999999E-7,2.7999999999999999E-6,2.9999999999999999E-7,2.7999999999999999E-6,"NOx control","Selective Catalytic Reduction","2009-12-01","SO2 control","Dry FGD - Spray Dryer","2009-12-01","PM control","Fabric Filter, pulse","2009-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["641_7","coal",34,null,641,"Crist","FL","Unit 7","7","Conventional Boiler","Wall firing - front firing",500,5279.7920000000004,10.559584000000001,"bituminous","bituminous",1.8702034199257133E-3,2.71535326023767E-7,2.867300084115354E-6,null,null,2.71535326023767E-7,2.867300084115354E-6,"NOx control","Selective Catalytic Reduction","2005-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2004-04-01","SO2 control","Wet FGD - Spray Type","2009-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["641_4","coal",35,null,641,"Crist","FL","Unit 4","4","Conventional Boiler","Tangential firing",82,868.84199999999998,10.595634146341464,"bituminous","bituminous",1.8702034199257133E-3,2.71535326023767E-7,2.8770889723553877E-6,null,null,2.71535326023767E-7,2.8770889723553877E-6,"NOx control","Selective Noncatalytic Reduction","2006-04-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","2008-03-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-01-01","SO2 control","Wet FGD - Spray Type","2009-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6139_1","coal",36,null,6139,"Welsh","TX","WE-1","1","Conventional Boiler","Wall firing - opposed firing",558,5156,9.2401433691756267,"subbituminous","subbituminous",8.0792412843355512E-5,3.1190487213511184E-7,2.8820457360728253E-6,null,null,3.1190487213511184E-7,2.8820457360728253E-6,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1977-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10672_CBC","coal",37,null,10672,"Cedar Bay Generating Company L.P.","FL","CBC1","CBC","Fluidized bed firing","Fluidized bed firing",92,1063,11.554347826086957,"bituminous","bituminous",5.6430806808640556E-4,9.3139145545448613E-7,1.0761620838566509E-5,2.5177456597964593E-7,2.9090909090909093E-6,2.5177456597964593E-7,2.9090909090909093E-6,"SO2 control","Dry FGD - Circulating Dry Scrubber","1994-01-01","NOx control","Selective Noncatalytic Reduction","1994-01-01","PM control","Fabric Filter, pulse","1994-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8223_3","coal",38,null,8223,"Springerville","AZ","3","3","Conventional Boiler","Wall firing - opposed firing",450,4200,9.3333333333333339,"subbituminous","subbituminous",1.661234697858946E-4,3.8553089423616618E-7,3.5982883462042177E-6,3.15E-7,2.9400000000000002E-6,3.15E-7,2.9400000000000002E-6,"NOx control","Selective Catalytic Reduction","2006-08-01","SO2 control","Dry FGD - Spray Dryer","2006-08-01","PM control","Fabric Filter, pulse","2006-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6016_1","coal",39,null,6016,"Duck Creek","IL","001","1","Conventional Boiler","Wall firing - unspecified",400,4500,11.25,"subbituminous","subbituminous",3.0292108196905323E-4,2.7008263987241221E-7,3.0384296985646372E-6,4.7999999999999996E-7,5.3999999999999991E-6,2.7008263987241221E-7,3.0384296985646372E-6,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Electrostatic precipitator, cold side, unspecified","2009-03-01","SO2 control","Wet FGD - Venturi Type","2009-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6137_1","coal",40,null,6137,"A. B. Brown Generating Station","IN","1Config","1","Conventional Boiler","Wall firing - opposed firing",265,2518,9.5018867924528294,"subbituminous","subbituminous",1.6797810991077613E-3,3.2146677858945694E-7,3.0545409376915189E-6,null,null,3.2146677858945694E-7,3.0545409376915189E-6,"NOx control","Selective Catalytic Reduction","2005-04-01","PM control","Fabric Filter, pulse","2004-11-01","SO2 control","Wet FGD - Spray Type","1979-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2277_1","coal",41,null,2277,"Sheldon Station","NE","U1","1","Conventional Boiler","Cyclone firing",128,1374,10.734375,"subbituminous","subbituminous",1.673543858477654E-4,2.9118697256899844E-7,3.1257101586703425E-6,null,null,2.9118697256899844E-7,3.1257101586703425E-6,"PM control","Fabric Filter, pulse","1999-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["564_2","coal",42,null,564,"Stanton Energy Center","FL","2 coal","2","Conventional Boiler","Wall firing - opposed firing",468,4286,9.1581196581196576,"coal - bituminous","bituminous",null,3.473728771952254E-7,3.1812823753391796E-6,null,null,3.473728771952254E-7,3.1812823753391796E-6,"NOx control","Selective Catalytic Reduction","1996-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1996-06-01","SO2 control","Wet FGD - Spray Type","1996-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2554_4","coal",43,null,2554,"Dunkirk Generating Plant","NY","4","4","Conventional Boiler","Tangential firing",195,1836,9.4153846153846157,"subbituminous","subbituminous",2.6520524733875415E-4,3.3841174719417797E-7,3.1862767581974913E-6,null,null,3.3841174719417797E-7,3.1862767581974913E-6,"NOx control","Selective Noncatalytic Reduction",null,"Other control","Dry sorbent injection",null,"PM control","Fabric Filter, unspecified","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7213_2","coal",44,null,7213,"Clover","VA","Unit 2","2","Conventional Boiler","Tangential firing",434,5041,11.61520737327189,"bituminous","bituminous",8.4831553288125386E-4,2.8178300385823836E-7,3.2729680240769113E-6,null,null,2.8178300385823836E-7,3.2729680240769113E-6,"NOx control","Selective Noncatalytic Reduction","2003-03-01","PM control","Fabric Filter, reverse air","2003-05-01","SO2 control","Wet FGD - Spray Type","2003-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3845_BD22","coal",45,null,3845,"TransAlta Centralia Generation","WA","BW22CONFIG","BD22","Conventional Boiler","Tangential firing",567,7743,13.656084656084657,"subbituminous","subbituminous",3.4732281316020622E-4,2.4106180302456554E-7,3.2919603894518711E-6,null,null,2.4106180302456554E-7,3.2919603894518711E-6,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1971-12-01","SO2 control","Wet FGD - Spray Type","2001-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["55479_3","coal",46,null,55479,"Wygen 1","WY","WYG1Cfg","3","Conventional Boiler","Wall firing - front firing",91,1053,11.571428571428571,"subbituminous","subbituminous",1.9616204690831555E-4,2.9382638826382022E-7,3.3999910641956339E-6,null,null,2.9382638826382022E-7,3.3999910641956339E-6,"NOx control","Selective Catalytic Reduction","2003-04-01","SO2 control","Dry FGD - Spray Dryer","2003-04-01","PM control","Fabric Filter, pulse","2003-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2554_1","coal",47,null,2554,"Dunkirk Generating Plant","NY","1","1","Conventional Boiler","Tangential firing",85,922.2,10.849411764705883,"subbituminous","subbituminous",2.3751687257385327E-4,3.1348032871416365E-7,3.4010771663553145E-6,null,null,3.1348032871416365E-7,3.4010771663553145E-6,"NOx control","Selective Noncatalytic Reduction",null,"Other control","Dry sorbent injection",null,"PM control","Fabric Filter, unspecified","2009-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2451_Unit 3","coal",48,null,2451,"San Juan","NM","Unit 3","Unit 3","Conventional Boiler","Wall firing - opposed firing",544,5758,10.584558823529411,"subbituminous","subbituminous",9.7422201709127486E-4,3.2298957698761062E-7,3.4187021770122461E-6,null,null,3.2298957698761062E-7,3.4187021770122461E-6,"Other control","Activated carbon injection","2008-04-01","PM control","Fabric Filter, pulse","2008-03-01","SO2 control","Wet FGD - Spray Type","1998-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2277_2","coal",49,null,2277,"Sheldon Station","NE","U2","2","Conventional Boiler","Cyclone firing",141,1514,10.73758865248227,"subbituminous","subbituminous",1.6726234515462637E-4,3.2129184854115127E-7,3.4498997070305178E-6,null,null,3.2129184854115127E-7,3.4498997070305178E-6,"PM control","Fabric Filter, pulse","2000-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7097_BLR1","coal",50,null,7097,"J K Spruce","TX","1","BLR1","Conventional Boiler","Tangential firing",580,6361,10.967241379310344,"bituminous","bituminous",2.5512820512820514E-4,3.1760939576808828E-7,3.4832989077255338E-6,1.6433333333333334E-6,1.8022833333333333E-5,3.1760939576808828E-7,3.4832989077255338E-6,"PM control","Fabric Filter, reverse air","1992-07-01","SO2 control","Wet FGD - Spray Type","1992-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10678_BLR1","coal",51,null,10678,"AES Warrior Run Cogeneration Facility","MD","BLR1","BLR1","Fluidized bed firing","Fluidized bed firing",202,2047,10.133663366336634,"bituminous","bituminous",7.4099320654529976E-4,3.4524017330105741E-7,3.4985476967686365E-6,null,null,3.4524017330105741E-7,3.4985476967686365E-6,"NOx control","Selective Noncatalytic Reduction","2000-02-01","PM control","Fabric Filter, pulse","2000-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["56319_0001","coal",52,null,56319,"Wygen 2","WY","WYG2Cfg","0001","Conventional Boiler","Wall firing - front firing",96,1300,13.541666666666666,"subbituminous","subbituminous",1.9592810290484708E-4,2.606800826080892E-7,3.5300427853178743E-6,null,null,2.606800826080892E-7,3.5300427853178743E-6,"NOx control","Selective Catalytic Reduction","2008-01-01","SO2 control","Dry FGD - Spray Dryer","2008-01-01","PM control","Fabric Filter, pulse","2008-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["568_BHB3","coal",53,null,568,"Bridgeport Station","CT","BHSEMU3OS2-Coal","BHB3","Conventional Boiler","Tangential firing",403,4100,10.173697270471465,"subbituminous","subbituminous",8.685464717051796E-5,3.4743131686577831E-7,3.5346610400736753E-6,null,null,3.4743131686577831E-7,3.5346610400736753E-6,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1968-08-01","Other control","Activated carbon injection","2008-07-01","PM control","Fabric Filter, pulse","2008-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6002_4","coal",54,null,6002,"James H. Miller Jr.","AL","Unit 4","4","Conventional Boiler","Wall firing - front firing",723,6976.5291176000001,9.649417866666667,"subbituminous","subbituminous",2.0118294484126496E-4,3.7468048203368662E-7,3.6154485376271346E-6,null,null,3.7468048203368662E-7,3.6154485376271346E-6,"NOx control","Selective Catalytic Reduction","2003-03-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1991-03-01","SO2 control","Wet FGD - Spray Type",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10675_A","coal",55,null,10675,"AES Thames","CT","A","A","Fluidized bed firing","Fluidized bed firing",104,1002,9.634615384615385,"bituminous","bituminous",null,null,null,3.8033333333333334E-7,3.6643653846153849E-6,3.8033333333333334E-7,3.6643653846153849E-6,"SO2 control","Dry FGD - Circulating Dry Scrubber","1990-03-01","PM control","Fabric Filter, pulse","1990-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50951_1","coal",56,null,50951,"Sunnyside Cogen Associates","UT","Config 1","1","Fluidized bed firing","Fluidized bed firing",60,700,11.666666666666666,"bituminous","bituminous",2.028326543307275E-3,3.1720547808747169E-7,3.7007305776871697E-6,null,null,3.1720547808747169E-7,3.7007305776871697E-6,"NOx control","Other (specify): Anhydrous ammonia injection","1993-01-01","SO2 control","Dry FGD - Sorbent Injection","1993-01-01","PM control","Fabric Filter, pulse","1993-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6113_1","coal",57,null,6113,"Gibson","IN","1-2007-FGDIN","1","Conventional Boiler","Wall firing - opposed firing",661,6368,9.6338880484114977,"bituminous","bituminous",1.0771736578828815E-3,3.910454337951777E-7,3.767287931025252E-6,null,null,3.910454337951777E-7,3.767287931025252E-6,"NOx control","Selective Catalytic Reduction","2005-04-01","Other control","Other (specify): Soda Ash Injection for SO3 mitigation","2004-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-01-01","SO2 control","Wet FGD - Tray Type","2007-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2451_Unit 2","coal",58,null,2451,"San Juan","NM","Unit 2","Unit 2","Conventional Boiler","Wall firing - front firing",370,3688,9.967567567567567,"subbituminous","subbituminous",9.8577064469248339E-4,3.7875687510764029E-7,3.7752847443161549E-6,null,null,3.7875687510764029E-7,3.7752847443161549E-6,"Other control","Activated carbon injection","2009-06-01","PM control","Fabric Filter, pulse","2009-04-01","SO2 control","Wet FGD - Spray Type","1998-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10672_CBA","coal",59,null,10672,"Cedar Bay Generating Company L.P.","FL","CBA1","CBA","Fluidized bed firing","Fluidized bed firing",92,1063,11.554347826086957,"bituminous","bituminous",5.9382344976583324E-4,3.2950576498679844E-7,3.8072242193583343E-6,4.2365912544651964E-7,4.8951048951048953E-6,3.2950576498679844E-7,3.8072242193583343E-6,"SO2 control","Dry FGD - Circulating Dry Scrubber","1994-01-01","NOx control","Selective Noncatalytic Reduction","1994-01-01","PM control","Fabric Filter, pulse","1994-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10672_CBB","coal",60,null,10672,"Cedar Bay Generating Company L.P.","FL","CBB1","CBB","Fluidized bed firing","Fluidized bed firing",92,1063,11.554347826086957,"bituminous","bituminous",5.7297237312918428E-4,3.3319381718707608E-7,3.8498372572811073E-6,5.3484414472502038E-7,6.1797752808988771E-6,3.3319381718707608E-7,3.8498372572811073E-6,"SO2 control","Dry FGD - Circulating Dry Scrubber","1994-01-01","NOx control","Selective Noncatalytic Reduction","1994-01-01","PM control","Fabric Filter, pulse","1994-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["130_3","coal",61,null,130,"Cross","SC","C3","3","Conventional Boiler","Tangential firing",625,6058,9.6928000000000001,"bituminous","bituminous",3.6377475127982229E-4,3.9976105448399837E-7,3.8748039489024993E-6,2.2333333333333333E-6,2.1647253333333333E-5,3.9976105448399837E-7,3.8748039489024993E-6,"NOx control","Selective Catalytic Reduction","2006-08-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2006-08-01","SO2 control","Wet FGD - Spray Type","2006-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7504_2","coal",62,null,7504,"Neil Simpson II","WY","NS2Cfg","2","Conventional Boiler","Wall firing - front firing",88,1100,12.5,"subbituminous","subbituminous",3.037139881985422E-4,3.2935247281157227E-7,4.1169059101446537E-6,null,null,3.2935247281157227E-7,4.1169059101446537E-6,"SO2 control","Dry FGD - Circulating Dry Scrubber","1995-09-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1995-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7213_1","coal",63,null,7213,"Clover","VA","Unit 1","1","Conventional Boiler","Tangential firing",431,4923,11.422273781902552,"bituminous","bituminous",7.3061912658927591E-4,3.6458288517820677E-7,4.1643655307014199E-6,null,null,3.6458288517820677E-7,4.1643655307014199E-6,"PM control","Fabric Filter, reverse air","2003-05-01","SO2 control","Wet FGD - Spray Type","2003-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2718_ES-3","coal",64,null,2718,"G G Allen","NC","3-2009","ES-3","Conventional Boiler","Tangential firing",281.5,2228,7.9147424511545292,"bituminous","bituminous",1.0162107396149949E-3,5.2982899323629236E-7,4.193460024619749E-6,null,null,5.2982899323629236E-7,4.193460024619749E-6,"NOx control","Selective Noncatalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2002-06-01","SO2 control","Wet FGD - Spray Type","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E66&\"_\"&I66","v":"2718_ES-4"},"coal",65,null,2718,"G G Allen","NC","4-2009","ES-4","Conventional Boiler","Tangential firing",297.3,2380,8.0053817692566422,"bituminous","bituminous",1.0162107396149949E-3,5.2982899323629236E-7,4.2414833632774159E-6,null,null,5.2982899323629236E-7,4.2414833632774159E-6,"NOx control","Selective Noncatalytic Reduction","2006-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1999-02-01","SO2 control","Wet FGD - Spray Type","2009-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4072_8","coal",66,null,4072,"Pulliam","WI","8","8","Conventional Boiler","Wall firing - rear firing",137.9,1510,10.949963741841914,"subbituminous","subbituminous",2.2884728988594276E-4,3.9746681774666671E-7,4.3522472429112885E-6,null,null,3.9746681774666671E-7,4.3522472429112885E-6,"Other control","Activated carbon injection",null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1964-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6181_1","coal",67,null,6181,"J T Deely","TX","1","1","Conventional Boiler","Tangential firing",450,4251,9.4466666666666672,"subbituminous","subbituminous",2.1769590533585921E-4,4.6152500892852914E-7,4.3598729176781721E-6,null,null,4.6152500892852914E-7,4.3598729176781721E-6,"PM control","Fabric Filter, reverse air","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6181_2","coal",68,null,6181,"J T Deely","TX","2","2","Conventional Boiler","Tangential firing",450,4251,9.4466666666666672,"subbituminous","subbituminous",2.1769590533585921E-4,4.6152500892852914E-7,4.3598729176781721E-6,null,null,4.6152500892852914E-7,4.3598729176781721E-6,"PM control","Fabric Filter, reverse air","2006-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["56224_BLR100","coal",69,null,56224,"TS Power Plant","NV","TSPower","BLR100","Conventional Boiler","Wall firing - opposed firing",242,2112,8.7272727272727266,"subbituminous","subbituminous",2.128207630437954E-4,8.426895592156651E-7,7.354381607700349E-6,5.0883333333333341E-7,4.440727272727273E-6,5.0883333333333341E-7,4.440727272727273E-6,"NOx control","Selective Catalytic Reduction","2008-03-01","Other control","Activated carbon injection","2008-03-01","SO2 control","Dry FGD - Spray Dryer","2008-03-01","PM control","Fabric Filter, pulse","2008-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2712_1","coal",70,null,2712,"Roxboro Steam Electric Plant","NC","Rox_Cfg_1b","1","Conventional Boiler","Wall firing - opposed firing",385,3755,9.7532467532467528,"bituminous","bituminous",4.1723900630398578E-4,4.5783404722611437E-7,4.4653684346339204E-6,9.8733333333333325E-7,9.6297056277056264E-6,4.5783404722611437E-7,4.4653684346339204E-6,"NOx control","Selective Catalytic Reduction","2002-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-01-01","SO2 control","Wet FGD - Spray/Tray Type","2008-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50976_AABO1","coal",71,null,50976,"INDIANTOWN COGENERATION L.P.","FL","001","AABO1","Conventional Boiler","Wall firing - opposed firing",361,3422,9.4792243767313025,"bituminous","bituminous",6.7127214009597258E-4,3.5016904839537267E-6,3.3193309795262196E-5,4.8999999999999997E-7,4.6448199445983376E-6,4.8999999999999997E-7,4.6448199445983376E-6,"NOx control","Selective Catalytic Reduction","1995-12-01","SO2 control","Dry FGD - Spray Dryer","1995-12-01","PM control","Fabric Filter, pulse","1995-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1393_6","coal",72,null,1393,"RS Nelson","LA","001","6","Conventional Boiler","Tangential firing",580,5761,9.9327586206896559,"bituminous","bituminous",1.96484632154106E-4,4.7786886608675327E-7,4.7465560991823896E-6,null,null,4.7786886608675327E-7,4.7465560991823896E-6,"PM control","Electrostatic precipitator, unspecified","1982-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3149_2","coal",73,null,3149,"PPL Montour","PA","U2","2","Conventional Boiler","Tangential firing",792,7239,9.1401515151515156,"bituminous","bituminous",2.8265786304700074E-4,5.2017395077343294E-7,4.7544687243041429E-6,null,null,5.2017395077343294E-7,4.7544687243041429E-6,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2000-05-01","NOx control","Selective Catalytic Reduction","2000-05-01","SO2 control","Wet FGD - Tray Type","2008-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2107_2","coal",74,null,2107,"Sioux","MO","002","2","Conventional Boiler","Cyclone firing",524,4920,9.3893129770992374,"subbituminous,  bituminous","subbituminous,  bituminous",2.5988060541981946E-4,5.1346293082042905E-7,4.8210641596116624E-6,null,null,5.1346293082042905E-7,4.8210641596116624E-6,"NOx control","Selective Noncatalytic Reduction","2007-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1997-12-01","SO2 control","Wet FGD - Unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3179_1","coal",75,null,3179,"Hatfield's Ferry Power Station","PA","001","1","Conventional Boiler","Wall firing - opposed firing",590,5700,9.6610169491525415,"bituminous","bituminous",2.6555926246496075E-4,5.110430920239814E-7,4.9371959737910064E-6,7.5999999999999992E-6,7.3423728813559313E-5,5.110430920239814E-7,4.9371959737910064E-6,"PM control","Electrostatic precipitator, cold side, unspecified","1969-01-01","SO2 control","Wet FGD - Spray Type","2009-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2712_2","coal",76,null,2712,"Roxboro Steam Electric Plant","NC","Rox_Cfg_2c","2","Conventional Boiler","Tangential firing",703,6893,9.8051209103840691,"bituminous","bituminous",5.5012667403775374E-4,5.1169052635056232E-7,5.0171874795653293E-6,5.4013333333333322E-7,5.2960726410621139E-6,5.1169052635056232E-7,5.0171874795653293E-6,"NOx control","Selective Catalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-05-01","SO2 control","Wet FGD - Spray/Tray Type","2007-04-20","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6077_1","coal",77,null,6077,"Gerald Gentleman","NE","U1","1","Conventional Boiler","Wall firing - opposed firing",715,7538,10.542657342657343,"bituminous","bituminous",1.6569142668685545E-4,4.7642562041801132E-7,5.0227920653300268E-6,null,null,4.7642562041801132E-7,5.0227920653300268E-6,"PM control","Fabric Filter, reverse air","2000-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2837_3","coal",78,null,2837,"Eastlake","OH","Unit 3","3","Conventional Boiler","Tangential firing",144,1205,8.3680555555555554,"subbituminous,  bituminous","subbituminous,  bituminous",2.2355736845351758E-4,6.390090307304471E-7,5.3472630696540884E-6,null,null,6.390090307304471E-7,5.3472630696540884E-6,"NOx control","Selective Noncatalytic Reduction","1999-10-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3140_2","coal",79,null,3140,"PPL Brunner Island","PA","U2","2","Conventional Boiler","Tangential firing",393,3790,9.6437659033078873,"bituminous","bituminous",3.9967135165937723E-4,5.5679645878876309E-7,5.3696147043496486E-6,null,null,5.5679645878876309E-7,5.3696147043496486E-6,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2009-10-01","SO2 control","Wet FGD - Tray Type","2009-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6113_2","coal",80,null,6113,"Gibson","IN","2-2007-FGDIN","2","Conventional Boiler","Wall firing - opposed firing",661,6444,9.7488653555219358,"bituminous","bituminous",1.1439315491273848E-3,5.6046079785526405E-7,5.4638568553393665E-6,null,null,5.6046079785526405E-7,5.4638568553393665E-6,"NOx control","Selective Catalytic Reduction","2001-12-01","Other control","Other (specify): Soda Ash Injection for SO3 mitigation","2004-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1991-01-01","SO2 control","Wet FGD - Tray Type","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3140_1","coal",81,null,3140,"PPL Brunner Island","PA","U1","1","Conventional Boiler","Tangential firing",330,3345,10.136363636363637,"bituminous","bituminous",3.9967135165937723E-4,5.5679645878876309E-7,5.6438913777224622E-6,null,null,5.5679645878876309E-7,5.6438913777224622E-6,"PM control","Fabric Filter, pulse","1965-01-01","SO2 control","Wet FGD - Tray Type","2009-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2828_3","coal",82,null,2828,"Cardinal","OH","CD-U3","3","Conventional Boiler","Wall firing - opposed firing",650,5275,8.115384615384615,"bituminous","bituminous",7.964484463625557E-4,7.0213283868205319E-7,5.6980780369966622E-6,null,null,7.0213283868205319E-7,5.6980780369966622E-6,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1977-09-01","NOx control","Selective Catalytic Reduction","2003-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6017_2","coal",83,null,6017,"Newton","IL","002","2","Conventional Boiler","Tangential firing",620,5500,8.870967741935484,"subbituminous","subbituminous",2.2531595785819393E-4,6.6673333457550882E-7,5.9145699034924174E-6,null,null,6.6673333457550882E-7,5.9145699034924174E-6,"Other control","Other (specify): Flue gas conditioning","2001-04-01","Other control","Activated carbon injection",null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1626_1","coal",84,null,1626,"Salem Harbor","MA","Unit 1","1","Conventional Boiler","Wall firing - front firing",81.418999999999997,981,12.0487846817082,"bituminous","bituminous",3.7878787878787879E-4,4.9694445248584524E-7,5.987576706771321E-6,null,null,4.9694445248584524E-7,5.987576706771321E-6,"NOx control","Selective Noncatalytic Reduction","1993-08-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54304_1A","coal",85,null,54304,"Birchwood Power Facility","VA","1A","1A","Conventional Boiler","Tangential firing",222,2300,10.36036036036036,"bituminous","bituminous",6.3631969971304379E-4,5.7815601570398997E-7,5.9899046672034998E-6,null,null,5.7815601570398997E-7,5.9899046672034998E-6,"NOx control","Selective Catalytic Reduction","1996-10-01","SO2 control","Dry FGD - Spray Dryer","1996-10-01","PM control","Fabric Filter, reverse air","1996-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3403_2","coal",86,null,3403,"Gallatin","TN","2","2","Conventional Boiler","Tangential firing",300,2750,9.1666666666666661,"subbituminous","subbituminous",1.8394454289863361E-4,6.5946967917925029E-7,6.0451387258097937E-6,null,null,6.5946967917925029E-7,6.0451387258097937E-6,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2727_Unit 4","coal",87,null,2727,"Marshall","NC","U4","Unit 4","Conventional Boiler","Tangential firing",700,6029.8,8.6140000000000008,"bituminous","bituminous",null,null,null,7.0460568059735639E-7,6.0694733326656285E-6,7.0460568059735639E-7,6.0694733326656285E-6,"NOx control","Selective Noncatalytic Reduction","2006-12-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2006-05-01","SO2 control","Wet FGD - Spray Type","2006-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2451_Unit 4","coal",88,null,2451,"San Juan","NM","Unit 4","Unit 4","Conventional Boiler","Wall firing - opposed firing",544,5649,10.384191176470589,"subbituminous","subbituminous",3.8709111960974366E-4,5.8652114558428191E-7,6.0905477047897216E-6,null,null,5.8652114558428191E-7,6.0905477047897216E-6,"Other control","Activated carbon injection","2008-04-01","PM control","Fabric Filter, pulse","2007-10-01","SO2 control","Wet FGD - Spray Type","1998-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4078_3","coal",89,null,4078,"Weston","WI","W3","3","Conventional Boiler","Tangential firing",365.6,3423.48,9.364004376367614,"subbituminous","subbituminous",2.5850489428127181E-4,6.5151817328818633E-7,6.10081902595361E-6,null,null,6.5151817328818633E-7,6.10081902595361E-6,"PM control","Fabric Filter, pulse","2001-05-01","Other control","Activated carbon injection",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3149_1","coal",90,null,3149,"PPL Montour","PA","U1","1","Conventional Boiler","Tangential firing",797,7239,9.0828105395232122,"bituminous","bituminous",3.029773407200152E-4,6.7769292161147249E-7,6.1553564109729601E-6,null,null,6.7769292161147249E-7,6.1553564109729601E-6,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2001-05-01","NOx control","Selective Catalytic Reduction","2001-05-01","SO2 control","Wet FGD - Tray Type","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6250_1A","coal",91,null,6250,"Mayo Electric Generating Facility","NC","May_Cfg_1b","1A","Conventional Boiler","Wall firing - opposed firing",396,3743,9.4520202020202024,"coal - bituminous","bituminous",null,null,null,6.7800000000000001E-7,6.4084696969696976E-6,6.7800000000000001E-7,6.4084696969696976E-6,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1983-10-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1983-10-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1983-10-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1983-10-01","NOx control","Selective Catalytic Reduction","2004-04-19","NOx control","Selective Catalytic Reduction","2004-04-19","SO2 control","Wet FGD - Spray/Tray Type","2009-04-09","","",null,"","",null,"","",null,"","",null,"",""]
["6250_1B","coal",92,null,6250,"Mayo Electric Generating Facility","NC","May_Cfg_1b","1B","Conventional Boiler","Wall firing - opposed firing",396,3743,9.4520202020202024,"coal - bituminous","bituminous",null,null,null,6.7800000000000001E-7,6.4084696969696976E-6,6.7800000000000001E-7,6.4084696969696976E-6,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1983-10-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1983-10-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1983-10-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1983-10-01","NOx control","Selective Catalytic Reduction","2004-04-19","NOx control","Selective Catalytic Reduction","2004-04-19","SO2 control","Wet FGD - Spray/Tray Type","2009-04-09","","",null,"","",null,"","",null,"","",null,"",""]
["708_2","coal",93,null,708,"Hammond","GA","Unit 2","2","Conventional Boiler","Wall firing - front firing",115,1138.0319999999999,9.895930434782608,"bituminous","bituminous",7.248101409646797E-4,6.4907153890291578E-7,6.4231667961805476E-6,null,null,6.4907153890291578E-7,6.4231667961805476E-6,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1969-04-01","SO2 control","Wet FGD - Spray Type","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["708_3","coal",94,null,708,"Hammond","GA","Unit 3","3","Conventional Boiler","Wall firing - front firing",115,1141.3920000000001,9.9251478260869561,"bituminous","bituminous",7.248101409646797E-4,6.4907153890291578E-7,6.4421309733171894E-6,null,null,6.4907153890291578E-7,6.4421309733171894E-6,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1968-12-01","SO2 control","Wet FGD - Spray Type","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["470_2","coal",95,null,470,"Comanche","CO","Unit 2","2","Conventional Boiler","Wall firing - front firing",365,3482,9.5397260273972595,"subbituminous","subbituminous",2.2222894976121424E-4,6.8082890473674601E-7,6.4949212227215056E-6,null,null,6.8082890473674601E-7,6.4949212227215056E-6,"Other control","Activated carbon injection",null,"SO2 control","Dry FGD - Spray Dryer","2008-07-01","PM control","Fabric Filter, reverse air","1991-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["708_1","coal",96,null,708,"Hammond","GA","Unit 1","1","Conventional Boiler","Wall firing - front firing",115,1158.752,10.076104347826087,"bituminous","bituminous",7.248101409646797E-4,6.4907153890291578E-7,6.5401125551898389E-6,null,null,6.4907153890291578E-7,6.5401125551898389E-6,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-02-01","SO2 control","Wet FGD - Spray Type","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["68029_BLR1","coal",97,null,68029,"AES Puerto Rico Cogeneration Facility","PR","Unit_1","BLR1","Fluidized bed firing","Fluidized bed firing",255,2461.4,9.652549019607843,"bituminous","bituminous",1.8801568963337041E-4,6.7875889639059044E-7,6.5517535199050955E-6,null,null,6.7875889639059044E-7,6.5517535199050955E-6,"NOx control","Selective Noncatalytic Reduction",null,"SO2 control","Dry FGD - Spray Dryer",null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["708_4","coal",98,null,708,"Hammond","GA","Unit 4","4","Conventional Boiler","Wall firing - front firing",520,5458.53,10.497173076923076,"bituminous","bituminous",7.248101409646797E-4,6.4907153890291578E-7,6.8134162831687168E-6,null,null,6.4907153890291578E-7,6.8134162831687168E-6,"NOx control","Selective Catalytic Reduction","2002-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1970-12-01","SO2 control","Wet FGD - Spray Type","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10641_B1","coal",99,null,10641,"Cambria Cogen","PA","001","B1","Fluidized bed firing","Fluidized bed firing",49,560,11.428571428571429,"coal refuse (culm or gob),  other--natural gas","coal refuse (culm or gob),  other--natural gas",3.4428084726479311E-3,6.0584906053239808E-7,6.923989263227407E-6,null,null,6.0584906053239808E-7,6.923989263227407E-6,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Fabric Filter, unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54081_2A","coal",100,null,54081,"Spruance Genco, LLC","VA","GEN2","2A","Conventional Boiler","Stoker - underfeed",28.7,375,13.066202090592334,"bituminous","bituminous",6.8748695412941291E-4,5.3829110552992893E-7,7.0334203684224158E-6,null,null,5.3829110552992893E-7,7.0334203684224158E-6,"SO2 control","Dry FGD - Spray Dryer","1992-05-01","SO2 control","Dry FGD - Spray Dryer","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54081_2B","coal",101,null,54081,"Spruance Genco, LLC","VA","GEN2","2B","Conventional Boiler","Stoker - underfeed",28.7,375,13.066202090592334,"bituminous","bituminous",6.8748695412941291E-4,5.3829110552992893E-7,7.0334203684224158E-6,null,null,5.3829110552992893E-7,7.0334203684224158E-6,"SO2 control","Dry FGD - Spray Dryer","1992-05-01","SO2 control","Dry FGD - Spray Dryer","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1554_2","coal",102,null,1554,"Herbert A. Wagner","MD","002","2","Conventional Boiler","Wall firing - unspecified",145,1488,10.262068965517241,"bituminous","bituminous",3.3169317344294534E-3,7.3207396406551275E-7,7.5125935070998823E-6,null,null,7.3207396406551275E-7,7.5125935070998823E-6,"NOx control","Selective Noncatalytic Reduction",null,"Other control","Activated carbon injection",null,"PM control","Electrostatic precipitator, cold side, unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10849_BLR1","coal",103,null,10849,"Silver Bay Power","MN","GEN1","BLR1","Conventional Boiler","Wall firing - front firing",45,371.91187187999998,8.2647082639999994,"subbituminous","subbituminous",2.0085470085470084E-4,9.2109919298513827E-7,7.6126161122280024E-6,null,null,9.2109919298513827E-7,7.6126161122280024E-6,"PM control","Fabric Filter, reverse air","1980-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6065_1","coal",104,null,6065,"Iatan","MO","1","1","Conventional Boiler","Wall firing - opposed firing",726,7800,10.743801652892563,"coal - subbituminous","subbituminous",null,null,null,7.1999999999999999E-7,7.7355371900826453E-6,7.1999999999999999E-7,7.7355371900826453E-6,"NOx control","Selective Catalytic Reduction","2009-02-01","Other control","Activated carbon injection","2009-10-01","PM control","Fabric Filter, pulse","2009-02-01","SO2 control","Wet FGD - Spray Type","2009-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54144_BRBR1","coal",105,null,54144,"Piney Creek Project","PA","BRBRI","BRBR1","Fluidized bed firing","Fluidized bed firing",36,450,12.5,"bituminous,  synfuel","bituminous,  synfuel",3.1270817216152544E-3,1.4284361374527188E-6,1.7855451718158986E-5,6.2054054054054056E-7,7.7567567567567564E-6,6.2054054054054056E-7,7.7567567567567564E-6,"NOx control","Selective Noncatalytic Reduction","2002-08-01","PM control","Fabric Filter, pulse","1992-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["60_1","coal",106,null,60,"Whelan Energy Center Unit 1 (WEC1)","NE","1","1","Conventional Boiler","Tangential firing",83.6,845.1,10.10885167464115,"subbituminous","subbituminous",2.5250369101582703E-4,7.7806250610520388E-7,7.8653184678170794E-6,null,null,7.7806250610520388E-7,7.8653184678170794E-6,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6021_C1","coal",107,null,6021,"Craig","CO","C1","C1","Conventional Boiler","Wall firing - opposed firing",456,4028,8.8333333333333339,"subbituminous","subbituminous",3.4001101530869385E-4,9.2527968033395115E-7,8.1733038429499029E-6,null,null,9.2527968033395115E-7,8.1733038429499029E-6,"PM control","Fabric Filter, pulse","2003-11-01","SO2 control","Wet FGD - Spray Type","1980-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3287_MCM2","coal",108,null,3287,"McMeekin","SC","MCM002","MCM2","Conventional Boiler","Tangential firing",132,1101.3,8.3431818181818187,"bituminous","bituminous",5.6883489198317303E-4,1.019174697928726E-6,8.5031598093098942E-6,null,null,1.019174697928726E-6,8.5031598093098942E-6,"PM control","Fabric Filter, unspecified","1992-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["130_4","coal",109,null,130,"Cross","SC","C4","4","Conventional Boiler","Tangential firing",625,6798,10.876799999999999,"bituminous","bituminous",3.0425260003525469E-4,7.8335387757409349E-7,8.5203834555978998E-6,2.0666666666666666E-6,2.2478719999999997E-5,7.8335387757409349E-7,8.5203834555978998E-6,"NOx control","Selective Catalytic Reduction","2008-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2008-05-01","SO2 control","Wet FGD - Spray Type","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2712_3A","coal",110,null,2712,"Roxboro Steam Electric Plant","NC","Rox_Cfg_3b","3A","Conventional Boiler","Wall firing - rear firing",370.5,3460,9.3387314439946021,"coal - bituminous","bituminous",null,null,null,9.3899999999999992E-7,8.7690688259109301E-6,9.3899999999999992E-7,8.7690688259109301E-6,"NOx control","Selective Catalytic Reduction","2003-04-22","NOx control","Selective Catalytic Reduction","2003-04-22","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-11-01","SO2 control","Wet FGD - Spray/Tray Type","2008-05-08","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2712_3B","coal",111,null,2712,"Roxboro Steam Electric Plant","NC","Rox_Cfg_3b","3B","Conventional Boiler","Wall firing - rear firing",370.5,3460,9.3387314439946021,"coal - bituminous","bituminous",null,null,null,9.3899999999999992E-7,8.7690688259109301E-6,9.3899999999999992E-7,8.7690688259109301E-6,"NOx control","Selective Catalytic Reduction","2003-04-22","NOx control","Selective Catalytic Reduction","2003-04-22","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-11-01","SO2 control","Wet FGD - Spray/Tray Type","2008-05-08","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2712_4B","coal",112,null,2712,"Roxboro Steam Electric Plant","NC","Rox_Cfg_4c","4B","Conventional Boiler","Wall firing - opposed firing",372.5,3469,9.3127516778523489,"coal - bituminous","bituminous",null,null,null,9.5933333333333348E-7,8.9340331096196885E-6,9.5933333333333348E-7,8.9340331096196885E-6,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","NOx control","Selective Catalytic Reduction","2001-07-12","NOx control","Selective Catalytic Reduction","2001-07-12","Other control","Dry sorbent injection","2008-07-07","SO2 control","Wet FGD - Spray/Tray Type","2007-11-27"]
["2712_4A","coal",113,null,2712,"Roxboro Steam Electric Plant","NC","Rox_Cfg_4c","4A","Conventional Boiler","Wall firing - opposed firing",372.5,3469,9.3127516778523489,"coal - bituminous","bituminous",null,null,null,9.5933333333333348E-7,8.9340331096196885E-6,9.5933333333333348E-7,8.9340331096196885E-6,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-09-01","NOx control","Selective Catalytic Reduction","2001-07-12","NOx control","Selective Catalytic Reduction","2001-07-12","Other control","Dry sorbent injection","2008-07-07","SO2 control","Wet FGD - Spray/Tray Type","2007-11-27"]
["10774_2","coal",114,null,10774,"Southampton Power Station","VA","Unit 1 & 2","2","Conventional Boiler","Stoker - spreader",34,447,13.147058823529411,"bituminous","bituminous",6.5338864707859153E-4,6.9036769385771128E-7,9.0255423505809603E-6,null,null,6.9036769385771128E-7,9.0255423505809603E-6,"PM control","Multiple cyclone","1992-03-01","PM control","Multiple cyclone","1992-03-01","SO2 control","Dry FGD - Spray Dryer","1992-03-01","SO2 control","Dry FGD - Spray Dryer","1992-03-01","PM control","Fabric Filter, pulse","1992-03-01","PM control","Fabric Filter, pulse","1992-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10774_1","coal",115,null,10774,"Southampton Power Station","VA","Unit 1 & 2","1","Conventional Boiler","Stoker - spreader",34,442,13,"bituminous","bituminous",6.5338864707859153E-4,6.9036769385771128E-7,9.0255423505809603E-6,null,null,6.9036769385771128E-7,9.0255423505809603E-6,"PM control","Multiple cyclone","1992-03-01","PM control","Multiple cyclone","1992-03-01","SO2 control","Dry FGD - Spray Dryer","1992-03-01","SO2 control","Dry FGD - Spray Dryer","1992-03-01","PM control","Fabric Filter, pulse","1992-03-01","PM control","Fabric Filter, pulse","1992-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["525_1","coal",116,null,525,"Hayden","CO","Unit 1","1","Conventional Boiler","Wall firing - front firing",202,1963,9.717821782178218,"bituminous","bituminous",4.2430787773521726E-4,9.5925031741717829E-7,9.3218236291580253E-6,null,null,9.5925031741717829E-7,9.3218236291580253E-6,"SO2 control","Dry FGD - Spray Dryer","1998-12-01","PM control","Fabric Filter, reverse air","1998-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6019_1","coal",117,null,6019,"W H Zimmer","OH","1","1","Conventional Boiler","Wall firing - opposed firing",1408,12656,8.9886363636363633,"bituminous,  bituminous,  bituminous","bituminous,  bituminous,  bituminous",3.5863307512454089E-4,1.047136355655361E-6,9.4123279241294374E-6,null,null,1.047136355655361E-6,9.4123279241294374E-6,"Other control","Other (specify): Magnesium Hydroxide Injection",null,"NOx control","Selective Catalytic Reduction","2004-01-01","Other control","Dry sorbent injection","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1991-03-01","SO2 control","Wet FGD - Spray Type","2004-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6018_2","coal",118,null,6018,"East Bend Station","KY","2","2","Conventional Boiler","Wall firing - front firing",650.72463770000002,6313,9.7014922046188872,"bituminous","bituminous",5.0717057809055268E-4,9.8002396679652739E-7,9.5076948742161902E-6,null,null,9.8002396679652739E-7,9.5076948742161902E-6,"Other control","Dry sorbent injection","2005-01-01","PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1981-01-01","NOx control","Selective Catalytic Reduction","2002-01-01","SO2 control","Wet FGD - Spray Type","1981-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["113_3","coal",119,null,113,"Cholla","AZ","003","3","Conventional Boiler","Tangential firing",305,2929,9.6032786885245898,"bituminous","bituminous",7.5419976810574448E-4,1.0103634506813589E-6,9.7028017935924586E-6,null,null,1.0103634506813589E-6,9.7028017935924586E-6,"PM control","Fabric Filter, unspecified","2009-01-01","SO2 control","Wet FGD - Unspecified","2009-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2837_1","coal",120,null,2837,"Eastlake","OH","Unit 1","1","Conventional Boiler","Tangential firing",144,1205,8.3680555555555554,"subbituminous,  bituminous","subbituminous,  bituminous",1.539279435510362E-4,1.1756126235598438E-6,9.8375917457611926E-6,null,null,1.1756126235598438E-6,9.8375917457611926E-6,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6096_NC2","coal",121,null,6096,"Nebraska City","NE","NC2","NC2","Conventional Boiler","Wall firing - front firing",682,6920.2539999999999,10.147,"bituminous","bituminous",1.6820727557840284E-4,9.7180856152046086E-7,9.8609414737481172E-6,null,null,9.7180856152046086E-7,9.8609414737481172E-6,"NOx control","Selective Catalytic Reduction","2009-05-01","Other control","Activated carbon injection","2009-05-01","SO2 control","Dry FGD - Spray Dryer","2009-05-01","PM control","Fabric Filter, pulse","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1374_1374-2","coal",122,null,1374,"Elmer Smith Station","KY","Unit001","1374-2","Conventional Boiler","Tangential firing",291.5,2317,7.9485420240137223,"bituminous,  petroleum coke","bituminous,  petroleum coke",6.999135608079034E-4,1.1955054238653571E-6,9.9163745732093853E-6,null,null,1.1955054238653571E-6,9.9163745732093853E-6,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1993-12-01","SO2 control","Wet FGD - Spray Type","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1374_1374","coal",123,null,1374,"Elmer Smith Station","KY","Unit001","1374","Conventional Boiler","Cyclone firing",153,1370,8.9542483660130721,"bituminous,  petroleum coke","bituminous,  petroleum coke",6.999135608079034E-4,1.1955054238653571E-6,9.9163745732093853E-6,null,null,1.1955054238653571E-6,9.9163745732093853E-6,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1993-12-01","SO2 control","Wet FGD - Spray Type","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["525_2","coal",124,null,525,"Hayden","CO","Unit 2","2","Conventional Boiler","Tangential firing",285,2712,9.5157894736842099,"bituminous","bituminous",4.3787446208073223E-4,1.0650137604971454E-6,1.0134446731467572E-5,null,null,1.0650137604971454E-6,1.0134446731467572E-5,"SO2 control","Dry FGD - Spray Dryer","1999-06-01","PM control","Fabric Filter, reverse air","1999-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["68029_BLR2","coal",125,null,68029,"AES Puerto Rico Cogeneration Facility","PR","Unit_2","BLR2","Fluidized bed firing","Fluidized bed firing",255,2461.4,9.652549019607843,"bituminous","bituminous",2.0490149103699027E-4,1.0570025819818536E-6,1.02027692364319E-5,null,null,1.0570025819818536E-6,1.02027692364319E-5,"NOx control","Selective Noncatalytic Reduction",null,"SO2 control","Dry FGD - Spray Dryer",null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54081_1A","coal",126,null,54081,"Spruance Genco, LLC","VA","GEN1","1A","Conventional Boiler","Stoker - underfeed",28.7,375,13.066202090592334,"bituminous","bituminous",5.012524736105478E-4,7.8881170481050949E-7,1.0306773146478782E-5,null,null,7.8881170481050949E-7,1.0306773146478782E-5,"SO2 control","Dry FGD - Spray Dryer","1992-05-01","SO2 control","Dry FGD - Spray Dryer","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54081_1B","coal",127,null,54081,"Spruance Genco, LLC","VA","GEN1","1B","Conventional Boiler","Stoker - underfeed",28.7,375,13.066202090592334,"bituminous","bituminous",5.012524736105478E-4,7.8881170481050949E-7,1.0306773146478782E-5,null,null,7.8881170481050949E-7,1.0306773146478782E-5,"SO2 control","Dry FGD - Spray Dryer","1992-05-01","SO2 control","Dry FGD - Spray Dryer","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2451_Unit 1","coal",128,null,2451,"San Juan","NM","Unit 1","Unit 1","Conventional Boiler","Wall firing - front firing",370,3707,10.018918918918919,"subbituminous","subbituminous",8.8883563042060801E-4,1.050454516286137E-6,1.0524418626682999E-5,null,null,1.050454516286137E-6,1.0524418626682999E-5,"Other control","Activated carbon injection","2009-06-01","PM control","Fabric Filter, pulse","2008-10-01","SO2 control","Wet FGD - Spray Type","1998-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E130&\"_\"&I130","v":"1167_8"},"coal",129,null,1167,"Muscatine #1","IA","8","8","Conventional Boiler","Cyclone firing",75,823,10.973333333333333,"subbituminous","subbituminous",1.7432395412849398E-4,9.6745845370690893E-7,1.0616244098677147E-5,null,null,9.6745845370690893E-7,1.0616244098677147E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1999-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10641_B2","coal",130,null,10641,"Cambria Cogen","PA","002","B2","Fluidized bed firing","Fluidized bed firing",49,560,11.428571428571429,"coal refuse (culm or gob),  other--natural gas","coal refuse (culm or gob),  other--natural gas",3.1798075375294261E-3,9.4512168009160147E-7,1.0801390629618303E-5,null,null,9.4512168009160147E-7,1.0801390629618303E-5,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Fabric Filter, unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3138_3","coal",131,null,3138,"New Castle Plant","PA","NC3-2","3","Conventional Boiler","Wall firing - front firing",98,1025,10.459183673469388,"coal - bituminous","bituminous",null,null,null,1.05275E-6,1.1010905612244898E-5,1.05275E-6,1.1010905612244898E-5,"NOx control","Selective Noncatalytic Reduction","2005-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1047_4","coal",132,null,1047,"Lansing","IA","Unit 4","4","Conventional Boiler","Turbo",264.2,2626,9.939439818319455,"coal - subbituminous","subbituminous",null,null,null,1.11E-6,1.1032778198334594E-5,1.11E-6,1.1032778198334594E-5,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1977-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["492_5","coal",133,null,492,"Martin Drake","CO","Unit 5 - Coal","5","Conventional Boiler","Wall firing - front firing",55,570,10.363636363636363,"subbituminous","subbituminous",3.5938853826671563E-4,1.0689663026403658E-6,1.1078378045545609E-5,null,null,1.0689663026403658E-6,1.1078378045545609E-5,"PM control","Fabric Filter, reverse air","1998-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3287_MCM1","coal",134,null,3287,"McMeekin","SC","MCM001","MCM1","Conventional Boiler","Tangential firing",135,1143.5,8.4703703703703699,"bituminous","bituminous",6.3398106847782426E-4,1.3180789707597687E-6,1.1164617059731818E-5,null,null,1.3180789707597687E-6,1.1164617059731818E-5,"PM control","Fabric Filter, unspecified","1993-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54755_BLR2","coal",135,null,54755,"Roanoke Valley II","NC","Boiler 2","BLR2","Conventional Boiler","Wall firing - front firing",50,560,11.2,"bituminous","bituminous",9.584907710857817E-4,1.0049072339287526E-6,1.1254961020002027E-5,null,null,1.0049072339287526E-6,1.1254961020002027E-5,"NOx control","Selective Noncatalytic Reduction","1995-06-01","SO2 control","Dry FGD - Spray Dryer","1995-06-01","PM control","Fabric Filter, pulse","1995-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["55749_PC1","coal",136,null,55749,"Hardin Generator Project","MT","PC1","PC1","Conventional Boiler","Wall firing - unspecified",119,1304,10.957983193277311,"bituminous","bituminous",3.7981485725632714E-4,1.0483657962510146E-6,1.1487974775725404E-5,null,null,1.0483657962510146E-6,1.1487974775725404E-5,"NOx control","Selective Catalytic Reduction","2006-04-01","Other control","Activated carbon injection",null,"SO2 control","Dry FGD - Spray Dryer","2006-04-01","PM control","Fabric Filter, pulse","2006-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2716_1","coal",137,null,2716,"W.H. Weatherspoon Plant","NC","Wea_Cfg_1","1","Conventional Boiler","Wall firing - front firing",53,472,8.9056603773584904,"bituminous","bituminous",7.5046935312249243E-4,1.309452517917355E-6,1.1661539404848898E-5,null,null,1.309452517917355E-6,1.1661539404848898E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2716_2","coal",138,null,2716,"W.H. Weatherspoon Plant","NC","Wea_Cfg_1","2","Conventional Boiler","Wall firing - front firing",53,472,8.9056603773584904,"bituminous","bituminous",7.5046935312249243E-4,1.309452517917355E-6,1.1661539404848898E-5,null,null,1.309452517917355E-6,1.1661539404848898E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["130_1","coal",139,null,130,"Cross","SC","C1","1","Conventional Boiler","Wall firing - opposed firing",610,6502,10.659016393442624,"bituminous","bituminous",3.1307384117060244E-4,1.1159465294259819E-6,1.1894892351356942E-5,null,null,1.1159465294259819E-6,1.1894892351356942E-5,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1995-05-01","SO2 control","Wet FGD - Spray Type","1995-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["988_4","coal",140,null,988,"Tanners Creek","IN","TC-4","4","Conventional Boiler","Cyclone firing",579.70000000000005,4990,8.6079006382611691,"subbituminous,  bituminous","subbituminous,  bituminous",2.6936958453934335E-4,1.4722685497631998E-6,1.2673141389198493E-5,null,null,1.4722685497631998E-6,1.2673141389198493E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3775_1","coal",141,null,3775,"Clinch River","VA","CR-1","1","Conventional Boiler","Vertical firing",230,2100.9,9.1343478260869571,"bituminous","bituminous",6.4868397096564691E-4,1.4002783098567695E-6,1.2790629135556902E-5,null,null,1.4002783098567695E-6,1.2790629135556902E-5,"NOx control","Selective Noncatalytic Reduction","2009-01-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1975-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50974_#2 CFB Boiler","coal",142,null,50974,"Scrubgrass Generating Company L.P.","PA","Gen 1","#2 CFB Boiler","Fluidized bed firing","Fluidized bed firing",48.5,600,12.371134020618557,"coal refuse (culm or gob)","coal refuse (culm or gob)",8.2038822684265041E-3,6.4562840428628393E-6,8.3199536634830405E-5,9.9999999999999995E-7,1.2886597938144331E-5,9.9999999999999995E-7,1.2886597938144331E-5,"NOx control","Selective Noncatalytic Reduction","1999-06-01","NOx control","Selective Noncatalytic Reduction","1999-06-01","PM control","Fabric Filter, pulse","1993-06-01","PM control","Fabric Filter, pulse","1993-06-01","SO2 control","Dry FGD - Circulating Dry Scrubber","1993-06-01","SO2 control","Dry FGD - Circulating Dry Scrubber","1993-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50974_#1 CFB boiler","coal",143,null,50974,"Scrubgrass Generating Company L.P.","PA","Gen 1","#1 CFB boiler","Fluidized bed firing","Fluidized bed firing",48.5,650,13.402061855670103,"coal refuse (culm or gob)","coal refuse (culm or gob)",8.2038822684265041E-3,6.4562840428628393E-6,8.3199536634830405E-5,9.9999999999999995E-7,1.2886597938144331E-5,9.9999999999999995E-7,1.2886597938144331E-5,"NOx control","Selective Noncatalytic Reduction","1999-06-01","NOx control","Selective Noncatalytic Reduction","1999-06-01","PM control","Fabric Filter, pulse","1993-06-01","PM control","Fabric Filter, pulse","1993-06-01","SO2 control","Dry FGD - Circulating Dry Scrubber","1993-06-01","SO2 control","Dry FGD - Circulating Dry Scrubber","1993-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6113_4","coal",144,null,6113,"Gibson","IN","4","4","Conventional Boiler","Wall firing - opposed firing",661,6265,9.4780635400907709,"bituminous","bituminous",null,null,null,1.3776140099482376E-6,1.3057113120008636E-5,1.3776140099482376E-6,1.3057113120008636E-5,"NOx control","Selective Catalytic Reduction","2003-04-01","Other control","Other (specify): Soda Ash Injection for SO3 mitigation","2004-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","SO2 control","Wet FGD - Tray Type","1994-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1008_2","coal",145,null,1008,"R. Gallagher","IN","2-2007","2","Conventional Boiler","Wall firing - front firing",150,1460,9.7333333333333325,"coal - bituminous","bituminous",null,null,null,1.3927829050448491E-6,1.3556420275769863E-5,1.3927829050448491E-6,1.3556420275769863E-5,"PM control","Fabric Filter, shake and deflate","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3118_2","coal",146,null,3118,"Conemaugh","PA","CON-2","2","Conventional Boiler","Tangential firing",936,8985,9.5993589743589745,"bituminous","bituminous",null,null,null,1.4863333333333333E-6,1.4267847222222222E-5,1.4863333333333333E-6,1.4267847222222222E-5,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-05-01","SO2 control","Wet FGD - Spray Type","1995-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["527_1","coal",147,null,527,"Nucla","CO","001","1","Fluidized bed firing","Fluidized bed firing",110,1032,9.3818181818181809,"bituminous","bituminous",1.0538392101452484E-3,1.5908094863380294E-6,1.4924685362734965E-5,null,null,1.5908094863380294E-6,1.4924685362734965E-5,"NOx control","Selective Noncatalytic Reduction","2006-07-01","PM control","Fabric Filter, shake and deflate","1987-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2378_2","coal",148,null,2378,"BL England","NJ","2 Coal w or w/o TDF","2","Conventional Boiler","Cyclone firing",167.3,1600,9.5636580992229518,"bituminous","bituminous",null,null,null,1.583297376866492E-6,1.514211478174768E-5,1.583297376866492E-6,1.514211478174768E-5,"NOx control","Selective Noncatalytic Reduction","1998-06-01","Other control","Activated carbon injection","2007-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-01-01","SO2 control","Wet FGD - Spray Type","1994-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["981_3","coal",149,null,981,"State Line","IN","Unit 3","3","Conventional Boiler","Tangential firing",216,2380,11.018518518518519,"bituminous","bituminous",4.2016806722689078E-4,1.4338753820887386E-6,1.5799182450792581E-5,null,null,1.4338753820887386E-6,1.5799182450792581E-5,"PM control","Fabric Filter, pulse","1999-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54081_4B","coal",150,null,54081,"Spruance Genco, LLC","VA","GEN4","4B","Conventional Boiler","Stoker - underfeed",28.7,375,13.066202090592334,"bituminous","bituminous",6.0531889546371119E-4,1.2123341791702846E-6,1.5840603386371314E-5,2.4519555386500998E-6,3.2037746585149387E-5,1.2123341791702846E-6,1.5840603386371314E-5,"SO2 control","Dry FGD - Spray Dryer","1992-05-01","SO2 control","Dry FGD - Spray Dryer","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54081_4A","coal",151,null,54081,"Spruance Genco, LLC","VA","GEN4","4A","Conventional Boiler","Stoker - underfeed",28.7,375,13.066202090592334,"bituminous","bituminous",6.0531889546371119E-4,1.2123341791702846E-6,1.5840603386371314E-5,2.4519555386500998E-6,3.2037746585149387E-5,1.2123341791702846E-6,1.5840603386371314E-5,"SO2 control","Dry FGD - Spray Dryer","1992-05-01","SO2 control","Dry FGD - Spray Dryer","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1710_Unit 2","coal",152,null,1710,"Consumers Energy - J.H. Campbell","MI","JHC2-Conf","Unit 2","Conventional Boiler","Wall firing - front firing",374,3392,9.0695187165775408,"subbituminous,  bituminous","subbituminous,  bituminous",4.1608311054779171E-4,1.8067271635940434E-6,1.6386145825965231E-5,null,null,1.8067271635940434E-6,1.6386145825965231E-5,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1978-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1710_Unit 1","coal",153,null,1710,"Consumers Energy - J.H. Campbell","MI","JHC1-Conf","Unit 1","Conventional Boiler","Tangential firing",274,2561,9.3467153284671536,"subbituminous","subbituminous",1.6620121410363675E-4,1.8067271635940434E-6,1.6886964474322429E-5,null,null,1.8067271635940434E-6,1.6886964474322429E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2001-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3138_5","coal",154,null,3138,"New Castle Plant","PA","NC5-2","5","Conventional Boiler","Wall firing - front firing",143.30000000000001,1441,10.055826936496858,"coal - bituminous","bituminous",null,null,null,1.7600000000000001E-6,1.7698255408234471E-5,1.7600000000000001E-6,1.7698255408234471E-5,"NOx control","Selective Noncatalytic Reduction","2005-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["642_1","coal",155,null,642,"Scholz","FL","Unit 1","1","Conventional Boiler","Wall firing - front firing",49,581.09100000000001,11.859,"bituminous","bituminous",8.3800480431662149E-4,1.5356232218508671E-6,1.8210955787929434E-5,null,null,1.5356232218508671E-6,1.8210955787929434E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["887_1","coal",156,null,887,"Joppa Steam","IL","1","1","Conventional Boiler","Tangential firing",183.3,1800,9.8199672667757767,"subbituminous","subbituminous",2.1179373645490752E-4,1.8555982397516794E-6,1.822191397464824E-5,null,null,1.8555982397516794E-6,1.822191397464824E-5,"Other control","Activated carbon injection","2009-07-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4042_3","coal",157,null,4042,"Valley","WI","VAPP-B3","3","Conventional Boiler","Wall firing - front firing",72,868,12.055555555555555,"bituminous","bituminous",3.8001779602251225E-4,1.6038555418423378E-6,1.933536958776596E-5,null,null,1.6038555418423378E-6,1.933536958776596E-5,"PM control","Fabric Filter, pulse","1995-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["642_2","coal",158,null,642,"Scholz","FL","Unit 2","2","Conventional Boiler","Wall firing - front firing",49,644.74199999999996,13.157999999999999,"bituminous","bituminous",8.3800480431662149E-4,1.5356232218508671E-6,2.0205730353113708E-5,null,null,1.5356232218508671E-6,2.0205730353113708E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10075_2","coal",159,null,10075,"Taconite Harbor Energy Center","MN","THEC2","2","Conventional Boiler","Tangential firing",79.2,913,11.527777777777777,"bituminous","bituminous",1.637593414396971E-4,1.7912658325922976E-6,2.0649314459050096E-5,null,null,1.7912658325922976E-6,2.0649314459050096E-5,"NOx control","","2007-01-01","Other control","Dry sorbent injection","2007-01-01","PM control","Electrostatic precipitator, cold side, unspecified","2007-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2094_3","coal",160,null,2094,"Sibley","MO","3","3","Conventional Boiler","Cyclone firing",419,4094.1,9.7711217183770884,"subbituminous,  bituminous","subbituminous,  bituminous",2.9354780230140062E-4,2.1273413422549101E-6,2.078651119170842E-5,null,null,2.1273413422549101E-6,2.078651119170842E-5,"NOx control","Selective Catalytic Reduction","2009-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1993-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3280_CAN3","coal",161,null,3280,"Canadys Steam","SC","CAN003","CAN3","Conventional Boiler","Wall firing - unspecified",185,1824.5,9.8621621621621625,"bituminous","bituminous",6.2453246891418506E-4,2.1182549662128098E-6,2.0890573977596062E-5,null,null,2.1182549662128098E-6,2.0890573977596062E-5,"PM control","Fabric Filter, unspecified","1998-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10075_1","coal",162,null,10075,"Taconite Harbor Energy Center","MN","THEC1","1","Conventional Boiler","Tangential firing",83,847,10.204819277108435,"bituminous","bituminous",1.8783066759046798E-4,2.0593890833251133E-6,2.1015693416582784E-5,null,null,2.0593890833251133E-6,2.1015693416582784E-5,"NOx control","Selective Noncatalytic Reduction","2008-01-01","Other control","Dry sorbent injection","2008-01-01","PM control","Electrostatic precipitator, cold side, unspecified","2008-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4041_7","coal",163,null,4041,"South Oak Creek","WI","OCPP-B7","7","Conventional Boiler","Tangential firing",320,2856,8.9250000000000007,"subbituminous","subbituminous",1.7461149397476577E-4,2.4226607006905536E-6,2.1622246753663195E-5,null,null,2.4226607006905536E-6,2.1622246753663195E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1992-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["884_4","coal",164,null,884,"Will County","IL","WC4CONFIG","4","Conventional Boiler","Tangential firing",542,5254.5300000000007,9.6947047970479723,"subbituminous","subbituminous",2.5739275373470736E-4,2.25319708890173E-6,2.1844080626470127E-5,null,null,2.25319708890173E-6,2.1844080626470127E-5,"Other control","Activated carbon injection","2009-07-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1963-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6664_101","coal",165,null,6664,"Louisa","IA","101","101","Conventional Boiler","Wall firing - unspecified",805,8624,10.71304347826087,"subbituminous","subbituminous",2.4431339511373211E-4,2.0583016067842347E-6,2.2050674604853716E-5,1.06E-5,1.1355826086956522E-4,2.0583016067842347E-6,2.2050674604853716E-5,"SO2 control","Dry FGD - Circulating Dry Scrubber","2007-12-01","PM control","Fabric Filter, pulse","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["47_4","coal",166,null,47,"Colbert","AL","4","4","Conventional Boiler","Wall firing - front firing",200,2121,10.605,"subbituminous,  bituminous","subbituminous,  bituminous",2.6332074891308611E-4,2.1675268213358195E-6,2.2986621940266367E-5,null,null,2.1675268213358195E-6,2.2986621940266367E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1991-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2094_1","coal",167,null,2094,"Sibley","MO","1","1","Conventional Boiler","Cyclone firing",55,609.6,11.083636363636364,"subbituminous,  bituminous","subbituminous,  bituminous",2.9354780230140062E-4,2.1273413422549101E-6,2.3578677858883513E-5,null,null,2.1273413422549101E-6,2.3578677858883513E-5,"NOx control","Selective Noncatalytic Reduction","2008-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2079_5A","coal",168,null,2079,"Hawthorn","MO","5A","5A","Conventional Boiler","Wall firing - opposed firing",594,6600,11.111111111111111,"subbituminous,  bituminous","subbituminous,  bituminous",1.919444716111297E-4,2.1790715658586759E-6,2.4211906287318621E-5,null,null,2.1790715658586759E-6,2.4211906287318621E-5,"NOx control","Selective Catalytic Reduction","2001-05-01","SO2 control","Dry FGD - Spray Dryer","2001-05-01","PM control","Fabric Filter, pulse","2001-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3942_2","coal",169,null,3942,"Albright Power Station","WV","Unit_2","2","Conventional Boiler","Wall firing - unspecified",81,643,7.9382716049382713,"bituminous","bituminous",9.2612332811794519E-4,3.0663068802690411E-6,2.4341176839666584E-5,null,null,3.0663068802690411E-6,2.4341176839666584E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54081_3B","coal",170,null,54081,"Spruance Genco, LLC","VA","GEN3","3B","Conventional Boiler","Stoker - underfeed",28.7,375,13.066202090592334,"bituminous","bituminous",5.2263340221341361E-4,1.9920333437026558E-6,2.6028310240017279E-5,null,null,1.9920333437026558E-6,2.6028310240017279E-5,"SO2 control","Dry FGD - Spray Dryer","1992-05-01","SO2 control","Dry FGD - Spray Dryer","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54081_3A","coal",171,null,54081,"Spruance Genco, LLC","VA","GEN3","3A","Conventional Boiler","Stoker - underfeed",28.7,375,13.066202090592334,"bituminous","bituminous",5.2263340221341361E-4,1.9920333437026558E-6,2.6028310240017279E-5,null,null,1.9920333437026558E-6,2.6028310240017279E-5,"SO2 control","Dry FGD - Spray Dryer","1992-05-01","SO2 control","Dry FGD - Spray Dryer","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","PM control","Fabric Filter, pulse","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2094_2","coal",172,null,2094,"Sibley","MO","2","2","Conventional Boiler","Cyclone firing",51,627.29999999999995,12.299999999999999,"subbituminous,  bituminous","subbituminous,  bituminous",2.9354780230140062E-4,2.1273413422549101E-6,2.6166298509735393E-5,null,null,2.1273413422549101E-6,2.6166298509735393E-5,"NOx control","Selective Noncatalytic Reduction","2008-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["47_3","coal",173,null,47,"Colbert","AL","3","3","Conventional Boiler","Wall firing - front firing",200,2121,10.605,"other--subbituminous/bituminous blend","other--subbituminous/bituminous blend",2.897279363832673E-4,2.4785016287040809E-6,2.628450977240678E-5,null,null,2.4785016287040809E-6,2.628450977240678E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3118_1","coal",174,null,3118,"Conemaugh","PA","CON-1","1","Conventional Boiler","Tangential firing",936,8985,9.5993589743589745,"bituminous","bituminous",null,null,null,2.8066666666666663E-6,2.6942200854700853E-5,2.8066666666666663E-6,2.6942200854700853E-5,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1970-05-01","SO2 control","Wet FGD - Spray Type","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3131_4","coal",175,null,3131,"Shawville","PA","SHAW4-2","4","Conventional Boiler","Tangential firing",188,1794,9.5425531914893611,"bituminous","bituminous",9.0428011831353045E-4,5.8664903656051964E-5,5.598129636114746E-4,2.8700000000000001E-6,2.7387127659574467E-5,2.8700000000000001E-6,2.7387127659574467E-5,"NOx control","Selective Noncatalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1960-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3131_3","coal",176,null,3131,"Shawville","PA","SHAW3-2","3","Conventional Boiler","Tangential firing",188,1794,9.5425531914893611,"bituminous","bituminous",9.0428011831353045E-4,5.8664903656051964E-5,5.598129636114746E-4,2.8700000000000001E-6,2.7387127659574467E-5,2.8700000000000001E-6,2.7387127659574467E-5,"NOx control","Selective Noncatalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1959-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3161_2","coal",177,null,3161,"Eddystone Generating Station","PA","Unit 2","2","Conventional Boiler","Tangential firing",339,2808,8.283185840707965,"bituminous","bituminous",3.3197336803979883E-4,3.6615082462631156E-6,3.0328953261082092E-5,3.3133333333333331E-6,2.7444955752212389E-5,3.3133333333333331E-6,2.7444955752212389E-5,"NOx control","Selective Noncatalytic Reduction","2003-06-01","PM control","Multiple cyclone","1960-11-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1960-11-01","PM control","PM scrubber - Venturi","1982-12-01","SO2 control","Wet FGD - Spray Type","1982-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10151_BLR1A","coal",178,null,10151,"Grant Town Power Plant","WV","GEN1","BLR1A","Fluidized bed firing","Fluidized bed firing",47.5,675,14.210526315789474,"coal refuse (culm or gob)","coal refuse (culm or gob)",1.4988118706093371E-3,2.062359144540091E-6,2.9307208896096031E-5,null,null,2.062359144540091E-6,2.9307208896096031E-5,"NOx control","Selective Noncatalytic Reduction","2005-05-01","NOx control","Selective Noncatalytic Reduction","2005-05-01","SO2 control","Dry FGD - Circulating Dry Scrubber","1992-07-01","SO2 control","Dry FGD - Circulating Dry Scrubber","1992-07-01","PM control","Fabric Filter, pulse","1992-07-01","PM control","Fabric Filter, pulse","2005-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10151_BLR1B","coal",179,null,10151,"Grant Town Power Plant","WV","GEN1","BLR1B","Fluidized bed firing","Fluidized bed firing",47.5,675,14.210526315789474,"coal refuse (culm or gob)","coal refuse (culm or gob)",1.4988118706093371E-3,2.062359144540091E-6,2.9307208896096031E-5,null,null,2.062359144540091E-6,2.9307208896096031E-5,"NOx control","Selective Noncatalytic Reduction","2005-05-01","NOx control","Selective Noncatalytic Reduction","2005-05-01","SO2 control","Dry FGD - Circulating Dry Scrubber","1992-07-01","SO2 control","Dry FGD - Circulating Dry Scrubber","1992-07-01","PM control","Fabric Filter, pulse","1992-07-01","PM control","Fabric Filter, pulse","2005-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["892_Unit 1","coal",180,null,892,"Hennepin Power Station","IL","001","Unit 1","Conventional Boiler","Tangential firing",75,776,10.346666666666666,"subbituminous","subbituminous",2.1649547543042225E-4,2.8624993210329861E-6,2.9617326308287961E-5,null,null,2.8624993210329861E-6,2.9617326308287961E-5,"PM control","Electrostatic precipitator, cold side, unspecified","1972-08-01","Other control","Activated carbon injection","2009-12-01","PM control","Fabric Filter, unspecified","2008-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50776_BLR2","coal",181,null,50776,"PANTHER CREEK ENERGY FACILITY","PA","BG2","BLR2","Fluidized bed firing","Fluidized bed firing",46.5,600,12.903225806451612,"coal refuse (culm or gob)","coal refuse (culm or gob)",2.7160184071992051E-3,2.3007973966742339E-6,2.9687708344183661E-5,null,null,2.3007973966742339E-6,2.9687708344183661E-5,"NOx control","Selective Noncatalytic Reduction","1992-10-01","PM control","Fabric Filter, pulse","1992-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50776_BLR1","coal",182,null,50776,"PANTHER CREEK ENERGY FACILITY","PA","BG1","BLR1","Fluidized bed firing","Fluidized bed firing",46.5,600,12.903225806451612,"coal refuse (culm or gob)","coal refuse (culm or gob)",2.7160184071992051E-3,2.3007973966742339E-6,2.9687708344183661E-5,null,null,2.3007973966742339E-6,2.9687708344183661E-5,"NOx control","Selective Noncatalytic Reduction","1992-10-01","PM control","Fabric Filter, pulse","1992-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["492_7","coal",183,null,492,"Martin Drake","CO","Unit 7 - Coal","7","Conventional Boiler","Wall firing - front firing",141,1475,10.460992907801419,"subbituminous,  bituminous","subbituminous,  bituminous",5.0290447878846112E-4,2.8679845098899186E-6,3.0001965617642767E-5,null,null,2.8679845098899186E-6,3.0001965617642767E-5,"PM control","Fabric Filter, reverse air","1993-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2403_U2","coal",184,null,2403,"PSEG Hudson Generating Station","NJ","HUDU2E2PT2OS1-Coal","U2","Conventional Boiler","Wall firing - opposed firing",659.7,6600,10.004547521600728,"natural gas","subbituminous",null,null,null,3.0333333333333337E-6,3.0347127482188877E-5,3.0333333333333337E-6,3.0347127482188877E-5,"NOx control","Selective Noncatalytic Reduction","1999-03-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1968-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["892_Unit 2","coal",185,null,892,"Hennepin Power Station","IL","002","Unit 2","Conventional Boiler","Tangential firing",234,2500,10.683760683760683,"subbituminous","subbituminous",2.1649547543042225E-4,2.8624993210329861E-6,3.0582257703343866E-5,null,null,2.8624993210329861E-6,3.0582257703343866E-5,"PM control","Electrostatic precipitator, cold side, unspecified","1974-06-01","Other control","Activated carbon injection","2009-06-01","PM control","Fabric Filter, unspecified","2008-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3152_4","coal",186,null,3152,"Sunbury Generation LP","PA","Boiler 4","4","Conventional Boiler","Wall firing - front firing",128,1360,10.625,"bituminous","bituminous",5.0125224619414579E-4,2.9645248059149453E-6,3.1498076062846298E-5,null,null,2.9645248059149453E-6,3.1498076062846298E-5,"Other control","Other (specify): SO3 injection","1980-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1970-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["864_5","coal",187,null,864,"Meredosia","IL","005","5","Conventional Boiler","Tangential firing",204,2784,13.647058823529411,"subbituminous","subbituminous",2.0224437697361435E-4,2.3292066533144144E-6,3.1786820209937888E-5,null,null,2.3292066533144144E-6,3.1786820209937888E-5,"Other control","Activated carbon injection","2009-08-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1992-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10603_031","coal",188,null,10603,"Ebensburg Power Company","PA","EPC01","031","Fluidized bed firing","Fluidized bed firing",58,830,14.310344827586206,"coal refuse (culm or gob)","coal refuse (culm or gob)",9.4723153875628848E-3,7.259847987365687E-6,1.0389092809506069E-4,2.2699999999999999E-6,3.2484482758620686E-5,2.2699999999999999E-6,3.2484482758620686E-5,"PM control","Fabric Filter, pulse","1990-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["52007_BLR1","coal",189,null,52007,"Mecklenburg Power Station","VA","Unit 1 & 2","BLR1","Conventional Boiler","Wall firing - front firing",76,916,12.052631578947368,"bituminous","bituminous",1.0178947139883542E-3,2.8561467909399166E-6,3.4461665885419782E-5,null,null,2.8561467909399166E-6,3.4461665885419782E-5,"SO2 control","Dry FGD - Spray Dryer","1992-11-01","SO2 control","Dry FGD - Spray Dryer","1992-11-01","PM control","Fabric Filter, pulse","1992-11-01","PM control","Fabric Filter, pulse","1992-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["52007_BLR2","coal",190,null,52007,"Mecklenburg Power Station","VA","Unit 1 & 2","BLR2","Conventional Boiler","Wall firing - front firing",76,918,12.078947368421053,"bituminous","bituminous",1.0178947139883542E-3,2.8561467909399166E-6,3.4461665885419782E-5,null,null,2.8561467909399166E-6,3.4461665885419782E-5,"SO2 control","Dry FGD - Spray Dryer","1992-11-01","SO2 control","Dry FGD - Spray Dryer","1992-11-01","PM control","Fabric Filter, pulse","1992-11-01","PM control","Fabric Filter, pulse","1992-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6041_1","coal",191,null,6041,"H L Spurlock Station","KY","Unit 01","1","Conventional Boiler","Wall firing - opposed firing",344,3641,10.584302325581396,"bituminous","bituminous",1.1468597460813125E-3,3.3462022493329321E-6,3.5417216249480254E-5,null,null,3.3462022493329321E-6,3.5417216249480254E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2003-05-01","NOx control","Selective Catalytic Reduction","2003-05-01","SO2 control","Wet FGD - Unspecified","2009-04-01","Other control","Wet electrostatic precipitator","2009-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7343_4","coal",192,null,7343,"George Neal South","IA","4","4","Conventional Boiler","Wall firing - unspecified",682,6900,10.117302052785924,"","Subbituminous",null,null,null,3.63E-6,3.6725806451612905E-5,3.63E-6,3.6725806451612905E-5,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1989-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E194&\"_\"&I194","v":"6098_001"},"coal",193,null,6098,"Big Stone","SD","001","001","Conventional Boiler","Cyclone firing",495,5309,10.725252525252525,"subbituminous","subbituminous",1.7162820148382068E-4,3.4554553423216483E-6,3.7060631136132588E-5,null,null,3.4554553423216483E-6,3.7060631136132588E-5,"PM control","Fabric Filter, pulse","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10771_10771-01","coal",194,null,10771,"Hopewell","VA","1 & 2","10771-01","Conventional Boiler","Stoker - spreader",34,433,12.735294117647058,"bituminous","bituminous",9.2946254525201892E-4,2.9669976307573095E-6,3.7305631974963229E-5,null,null,2.9669976307573095E-6,3.7305631974963229E-5,"NOx control","Selective Noncatalytic Reduction","1992-04-01","NOx control","Selective Noncatalytic Reduction","1992-04-01","PM control","Multiple cyclone","1992-04-01","PM control","Multiple cyclone","1992-04-01","SO2 control","Dry FGD - Spray Dryer","1992-04-01","SO2 control","Dry FGD - Spray Dryer","1992-04-01","PM control","Fabric Filter, pulse","1992-04-01","PM control","Fabric Filter, pulse","1992-04-01","","",null,"","",null,"","",null,"",""]
["10771_10771-02","coal",195,null,10771,"Hopewell","VA","1 & 2","10771-02","Conventional Boiler","Stoker - underfeed",34,422,12.411764705882353,"bituminous","bituminous",9.2946254525201892E-4,2.9669976307573095E-6,3.7305631974963229E-5,null,null,2.9669976307573095E-6,3.7305631974963229E-5,"NOx control","Selective Noncatalytic Reduction","1992-04-01","NOx control","Selective Noncatalytic Reduction","1992-04-01","PM control","Multiple cyclone","1992-04-01","PM control","Multiple cyclone","1992-04-01","SO2 control","Dry FGD - Spray Dryer","1992-04-01","SO2 control","Dry FGD - Spray Dryer","1992-04-01","PM control","Fabric Filter, pulse","1992-04-01","PM control","Fabric Filter, pulse","1992-04-01","","",null,"","",null,"","",null,"",""]
["10743_CFB1","coal",196,null,10743,"Morgantown Energy Facility","WV","Unit 1&2","CFB1","Fluidized bed firing","Fluidized bed firing",29,457,15.758620689655173,"bituminous","bituminous",2.4342312966015483E-3,2.3840985353435697E-6,3.7405683916597392E-5,null,null,2.3840985353435697E-6,3.7405683916597392E-5,"PM control","Fabric Filter, pulse","1992-01-01","PM control","Fabric Filter, pulse","1992-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10743_CFB2","coal",197,null,10743,"Morgantown Energy Facility","WV","Unit 1&2","CFB2","Fluidized bed firing","Fluidized bed firing",29,453,15.620689655172415,"bituminous","bituminous",2.4342312966015483E-3,2.3840985353435697E-6,3.7405683916597392E-5,null,null,2.3840985353435697E-6,3.7405683916597392E-5,"PM control","Fabric Filter, pulse","1992-01-01","PM control","Fabric Filter, pulse","1992-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8023_1","coal",198,null,8023,"Columbia","WI","Unit 1","1","Conventional Boiler","Tangential firing",590.29999999999995,6090,10.316788073860749,"coal - subbituminous","subbituminous",null,null,null,3.63E-6,3.7449940708114521E-5,3.63E-6,3.7449940708114521E-5,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1975-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["897_Unit 2","coal",199,null,897,"Vermilion","IL","002","Unit 2","Conventional Boiler","Tangential firing",110,1076,9.7818181818181813,"subbituminous","subbituminous",2.0438320429345998E-4,3.8822407629961354E-6,3.7975373281671288E-5,null,null,3.8822407629961354E-6,3.7975373281671288E-5,"PM control","Electrostatic precipitator, unspecified","1974-01-01","Other control","Activated carbon injection","2007-05-01","PM control","Fabric Filter, unspecified","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3131_2","coal",200,null,3131,"Shawville","PA","SHAW2-2","2","Conventional Boiler","Wall firing - front firing",125,1349,10.792,"coal - bituminous","bituminous",null,null,null,3.6299999999999995E-6,3.9174959999999994E-5,3.6299999999999995E-6,3.9174959999999994E-5,"NOx control","Selective Noncatalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1954-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1976-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1104_1","coal",201,null,1104,"Burlington","IA","Unit 1","1","Conventional Boiler","Tangential firing",212.02,2228,10.508442599754739,"coal - subbituminous","subbituminous",null,null,null,3.7799999999999998E-6,3.9721913027072913E-5,3.7799999999999998E-6,3.9721913027072913E-5,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1968-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3251_1","coal",202,null,3251,"HB Robinson / Darlington Electric Power Plant","SC","Rob_Cfg_1","1","Conventional Boiler","Tangential firing",187,1733,9.2673796791443852,"bituminous","bituminous",3.922691345841754E-4,4.3432084446855689E-6,4.0250161682567334E-5,null,null,4.3432084446855689E-6,4.0250161682567334E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["883_8","coal",203,null,883,"Waukegan","IL","WK8CONFIG","8","Conventional Boiler","Tangential firing",383,3960.8919999999998,10.3417545691906,"subbituminous","subbituminous",1.6709497815768987E-4,4.0178028391780748E-6,4.155113087017682E-5,null,null,4.0178028391780748E-6,4.155113087017682E-5,"Other control","Activated carbon injection","2008-07-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1962-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1241_2","coal",204,null,1241,"La Cygne","KS","2","2","Conventional Boiler","Wall firing - opposed firing",685,7700,11.240875912408759,"subbituminous","subbituminous",2.2020847810794752E-4,3.7716108820817475E-6,4.2396209915371468E-5,null,null,3.7716108820817475E-6,4.2396209915371468E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6254_1","coal",205,null,6254,"Ottumwa","IA","Unit 1","1","Conventional Boiler","Tangential firing",765.1,7990,10.443079336034504,"coal - subbituminous","subbituminous",null,null,null,4.2200000000000003E-6,4.4069794798065613E-5,4.2200000000000003E-6,4.4069794798065613E-5,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1981-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["897_Unit 1","coal",206,null,897,"Vermilion","IL","001","Unit 1","Conventional Boiler","Tangential firing",72,831,11.541666666666666,"subbituminous","subbituminous",2.0438320429345998E-4,3.8822407629961354E-6,4.4807528806247061E-5,null,null,3.8822407629961354E-6,4.4807528806247061E-5,"PM control","Electrostatic precipitator, unspecified","1973-06-01","Other control","Activated carbon injection","2007-05-01","PM control","Fabric Filter, unspecified","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6076_3","coal",207,null,6076,"Colstrip","MT","Unit3","3","Conventional Boiler","Tangential firing",805,7573,9.4074534161490675,"subbituminous","subbituminous",4.881423081599895E-4,4.7693884159197935E-6,4.4867799346286451E-5,null,null,4.7693884159197935E-6,4.4867799346286451E-5,"Other control","Activated carbon injection","2009-12-01","SO2 control","Wet FGD - Venturi Type","1984-01-01","PM control","PM scrubber - Venturi","1984-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54035_BLR1","coal",208,null,54035,"Roanoke Valley I","NC","Boiler 1","BLR1","Conventional Boiler","Wall firing - front firing",182,1700,9.3406593406593412,"bituminous","bituminous",1.0722023925150094E-3,4.8313112516349732E-6,4.5127632570216785E-5,null,null,4.8313112516349732E-6,4.5127632570216785E-5,"SO2 control","Dry FGD - Spray Dryer","1994-05-01","PM control","Fabric Filter, reverse air","1994-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1295_2","coal",209,null,1295,"Quindaro","KS","Unit 2","2","Conventional Boiler","Wall firing - front firing",119.8,1394,11.636060100166945,"bituminous","bituminous",1.6692534286367401E-4,3.9253782581095174E-6,4.5675937327250978E-5,null,null,3.9253782581095174E-6,4.5675937327250978E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1986-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2708_5","coal",210,null,2708,"Cape Fear Steam Electric Plant","NC","Cap_Cfg_5b","5","Conventional Boiler","Tangential firing",153,1242,8.117647058823529,"bituminous","bituminous",2.2646512412512857E-4,5.8286094317893928E-6,4.7314594210996246E-5,null,null,5.8286094317893928E-6,4.7314594210996246E-5,"NOx control","Selective Noncatalytic Reduction","2006-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1943_002","coal",211,null,1943,"Hoot Lake","MN","2","002","Conventional Boiler","Tangential firing",60.7,747.2,12.309719934102143,"subbituminous","subbituminous",9.6037829540181272E-5,4.1259433369263917E-6,5.0789206941538718E-5,null,null,4.1259433369263917E-6,5.0789206941538718E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1250_3","coal",212,null,1250,"Lawrence Energy Center","KS","3","3","Conventional Boiler","Tangential firing",58,645,11.120689655172415,"bituminous","bituminous",1.856075398471904E-4,4.5987053383581816E-6,5.1140774883465988E-5,null,null,4.5987053383581816E-6,5.1140774883465988E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4042_1","coal",213,null,4042,"Valley","WI","VAPP-B1","1","Conventional Boiler","Wall firing - front firing",72,868,12.055555555555555,"bituminous","bituminous",4.0747668997767752E-4,4.4693143810003982E-6,5.3880067815393687E-5,null,null,4.4693143810003982E-6,5.3880067815393687E-5,"PM control","Fabric Filter, pulse","1994-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["976_123","coal",214,null,976,"Marion Generating Station","IL","123","123","Fluidized bed firing","Fluidized bed firing",120,1250,10.416666666666666,"bituminous","bituminous",3.2672493308915974E-3,5.3423748489929336E-6,5.5649738010343052E-5,null,null,5.3423748489929336E-6,5.5649738010343052E-5,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Fabric Filter, unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1048_2","coal",215,null,1048,"ML Kapp","IA","Unit 2","2","Conventional Boiler","Tangential firing",229,2332,10.183406113537117,"coal - subbituminous","subbituminous",null,null,null,5.6799999999999998E-6,5.7841746724890821E-5,5.6799999999999998E-6,5.7841746724890821E-5,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["990_60","coal",216,null,990,"Harding Street","IN","60s","60","Conventional Boiler","Tangential firing",112,1017,9.0803571428571423,"bituminous","bituminous",1.0142335043668304E-3,6.9040925332370265E-6,6.2691625949125499E-5,null,null,6.9040925332370265E-6,6.2691625949125499E-5,"NOx control","Selective Noncatalytic Reduction","2004-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1363_4","coal",217,null,1363,"Cane Run","KY","CR4","4","Conventional Boiler","Wall firing - front firing",168,2310,13.75,"bituminous","bituminous",1.1626851555755246E-3,4.7725956106824678E-6,6.5623189646883936E-5,null,null,4.7725956106824678E-6,6.5623189646883936E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1963-06-01","SO2 control","Wet FGD - Spray Type","1976-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["874_5","coal",218,null,874,"Joliet 9","IL","JOL5 CONFIG","5","Conventional Boiler","Cyclone firing",326,3572.3780000000002,10.95821472392638,"subbituminous","subbituminous",1.6513458377099516E-4,6.3055967418929415E-6,6.9098083060153436E-5,null,null,6.3055967418929415E-6,6.9098083060153436E-5,"Other control","Activated carbon injection","2009-07-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1966-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2364_2","coal",219,null,2364,"Merrimack Station","NH","mk2","2","Conventional Boiler","Cyclone firing",337,3017,8.9525222551928785,"bituminous","bituminous",2.2283470526217105E-4,7.7833454714828164E-6,6.9680573553304619E-5,null,null,7.7833454714828164E-6,6.9680573553304619E-5,"NOx control","Selective Catalytic Reduction","1995-05-01","Other control","Activated carbon injection",null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1999-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1968-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["991_6","coal",220,null,991,"Eagle Valley","IN","6","6","Conventional Boiler","Tangential firing",105,1017,9.6857142857142851,"bituminous","bituminous",1.1630825459019256E-3,7.2803140045094539E-6,7.0515041357962992E-5,null,null,7.2803140045094539E-6,7.0515041357962992E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1971-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3131_1","coal",221,null,3131,"Shawville","PA","SHAW1-2","1","Conventional Boiler","Wall firing - front firing",125,1349,10.792,"coal - bituminous","bituminous",null,null,null,6.6000000000000003E-6,7.1227200000000001E-5,6.6000000000000003E-6,7.1227200000000001E-5,"NOx control","Selective Noncatalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1954-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1976-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3130_1","coal",222,null,3130,"Seward","PA","SEW-1","1","Fluidized bed firing","Fluidized bed firing",292.5,3100,10.598290598290598,"coal refuse (culm or gob)","coal refuse (culm or gob)",5.0911526958715902E-3,6.9533030922302547E-6,7.3693126789448854E-5,null,null,6.9533030922302547E-6,7.3693126789448854E-5,"NOx control","Selective Noncatalytic Reduction","2004-03-01","PM control","Fabric Filter, pulse","2004-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3130_2","coal",223,null,3130,"Seward","PA","SEW-1","2","Fluidized bed firing","Fluidized bed firing",292.5,3100,10.598290598290598,"coal refuse (culm or gob)","coal refuse (culm or gob)",5.0911526958715902E-3,6.9533030922302547E-6,7.3693126789448854E-5,null,null,6.9533030922302547E-6,7.3693126789448854E-5,"NOx control","Selective Noncatalytic Reduction","2004-03-01","PM control","Fabric Filter, pulse","2004-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1091_2","coal",224,null,1091,"George Neal North","IA","2","2","Conventional Boiler","Wall firing - unspecified",325,3081,9.48,"","Subbituminous",null,null,null,7.8820000000000001E-6,7.4721360000000003E-5,7.8820000000000001E-6,7.4721360000000003E-5,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1977-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7253_3","coal",225,null,7253,"Richard Gorsuch","OH","UNIT3","3","Conventional Boiler","Radiant",53.3,553,10.375234521575985,"bituminous","bituminous",9.0809249464341346E-4,7.2109415365698141E-6,7.4815209563285312E-5,null,null,7.2109415365698141E-6,7.4815209563285312E-5,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["990_70","coal",226,null,990,"Harding Street","IN","70ss","70","Conventional Boiler","Tangential firing",463,4123,8.9049676025917925,"bituminous","bituminous",4.9664366736336212E-4,8.5785717832559354E-6,7.6391903806402204E-5,null,null,8.5785717832559354E-6,7.6391903806402204E-5,"NOx control","Selective Catalytic Reduction","2005-12-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1978-12-01","SO2 control","Wet FGD - Spray Type","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1010_6","coal",227,null,1010,"Wabash River","IN","6","6","Conventional Boiler","Tangential firing",342,3059.0605,8.9446213450292404,"bituminous","bituminous",1.3971631192692972E-3,9.3567572274526789E-6,8.3692650416929853E-5,null,null,9.3567572274526789E-6,8.3692650416929853E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1993-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["628_1","coal",228,null,628,"Crystal River Power Plant","FL","CryR_Cfg_1","1","Conventional Boiler","Tangential firing",400,3837,9.5924999999999994,"bituminous","bituminous",5.4674376211710445E-7,9.6333375001473353E-6,9.2407789970163311E-5,null,null,9.6333375001473353E-6,9.2407789970163311E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["997_12","coal",229,null,997,"Michigan City","IN","12","12","Conventional Boiler","Cyclone firing",495,4650,9.3939393939393945,"subbituminous","subbituminous",1.3367673149344578E-4,9.9384180481309079E-6,9.3360896815775207E-5,null,null,9.9384180481309079E-6,9.3360896815775207E-5,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1992-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1385_3","coal",230,null,1385,"Dale Station","KY","03","3","Conventional Boiler","Wall firing - front firing",80,944,11.8,"bituminous","bituminous",3.4573771436457887E-4,7.9858090548354225E-6,9.4232546847057994E-5,null,null,7.9858090548354225E-6,9.4232546847057994E-5,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1010_4","coal",231,null,1010,"Wabash River","IN","4","4","Conventional Boiler","Wall firing - front firing",90,923.69500000000005,10.263277777777779,"bituminous","bituminous",1.3971631192692972E-3,9.3567572274526789E-6,9.6030998524576703E-5,null,null,9.3567572274526789E-6,9.6030998524576703E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1993-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1363_5","coal",232,null,1363,"Cane Run","KY","CR5","5","Conventional Boiler","Wall firing - front firing",181,2182,12.05524861878453,"bituminous","bituminous",1.1993387969581599E-3,7.9696261345471283E-6,9.6075824450728367E-5,null,null,7.9696261345471283E-6,9.6075824450728367E-5,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1966-03-01","SO2 control","Wet FGD - Spray Type","1978-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2840_3","coal",233,null,2840,"Conesville","OH","CV-3","3","Conventional Boiler","Wall firing - front firing",165,1862,11.284848484848485,"bituminous","bituminous",5.9415473970421612E-4,8.9236214152106476E-6,1.0070171560680137E-4,null,null,8.9236214152106476E-6,1.0070171560680137E-4,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1091_3","coal",234,null,1091,"George Neal North","IA","3","3","Conventional Boiler","Wall firing - unspecified",531,5021,9.4557438794726938,"","Subbituminous",null,null,null,1.112E-5,1.0514787193973636E-4,1.112E-5,1.0514787193973636E-4,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1073_4","coal",235,null,1073,"Prairie Creek","IA","Unit 4","4","Conventional Boiler","Wall firing - front firing",148.30000000000001,1611,10.863115306810519,"subbituminous","subbituminous",null,null,null,1.0200000000000001E-5,1.108037761294673E-4,1.0200000000000001E-5,1.108037761294673E-4,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1974-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2161_5","coal",236,null,2161,"James River Power Station","MO","Unit_5_JRPS","5","Conventional Boiler","Wall firing - front firing",105,1010,9.6190476190476186,"subbituminous","subbituminous",1.9935745246492983E-4,1.1602750101604313E-5,1.1160740573924147E-4,null,null,1.1602750101604313E-5,1.1160740573924147E-4,"NOx control","Selective Noncatalytic Reduction","2009-03-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1994-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3115_2","coal",237,null,3115,"Titus","PA","TI-2","2","Conventional Boiler","Tangential firing",86.2,900,10.440835266821345,"coal - bituminous","bituminous",null,null,null,1.1583333333333333E-5,1.2093967517401391E-4,1.1583333333333333E-5,1.2093967517401391E-4,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1082_3","coal",238,null,1082,"Walter Scott Jr. Energy Center","IA","3","3","Conventional Boiler","Wall firing - unspecified",765,7700,10.065359477124183,"","Subbituminous",null,null,null,1.2300000000000001E-5,1.2380392156862745E-4,1.2300000000000001E-5,1.2380392156862745E-4,"SO2 control","Dry FGD - Circulating Dry Scrubber","2009-05-01","PM control","Fabric Filter, pulse","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1167_9","coal",239,null,1167,"Muscatine #1","IA","9","9","Conventional Boiler","Tangential firing",175.5,1837,10.467236467236468,"coal - subbituminous","subbituminous",null,null,null,1.3732896876394519E-5,1.4374547898539448E-4,1.3732896876394519E-5,1.4374547898539448E-4,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1983-05-01","SO2 control","Wet FGD - Spray Type","1983-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1218_2","coal",240,null,1218,"Fair Station","IA","U2","2","Conventional Boiler","Wall firing - front firing",44,465,10.568181818181818,"bituminous","bituminous",1.0122903621786739E-3,1.406595960705729E-5,1.4865161857458272E-4,null,null,1.406595960705729E-5,1.4865161857458272E-4,"Other control","Other (specify): Flue gas conditioning for opacity control","2006-04-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1974-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10143_AAB01","coal",241,null,10143,"Colver Power Project","PA","AAB01","AAB01","Fluidized bed firing","Fluidized bed firing",131,1204,9.1908396946564892,"coal refuse (culm or gob)","coal refuse (culm or gob)",4.3412334774048239E-3,1.7142462641593176E-5,1.575536261105205E-4,null,null,1.7142462641593176E-5,1.575536261105205E-4,"NOx control","Selective Noncatalytic Reduction","1995-05-01","PM control","Fabric Filter, pulse","1995-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6041_3","coal",242,null,6041,"H L Spurlock Station","KY","Unit 03","3","Fluidized bed firing","Fluidized bed firing",300,2500,8.3333333333333339,"bituminous","bituminous",7.2831821949882834E-4,1.9948050917260171E-5,1.6623375764383477E-4,null,null,1.9948050917260171E-5,1.6623375764383477E-4,"NOx control","Selective Noncatalytic Reduction","2005-03-01","SO2 control","Dry FGD - Unspecified","2005-03-01","PM control","Fabric Filter, pulse","2005-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1091_1","coal",243,null,1091,"George Neal North","IA","1","1","Conventional Boiler","Cyclone firing",145,1363,9.4,"","Subbituminous",null,null,null,1.8600000000000001E-5,1.7484000000000003E-4,1.8600000000000001E-5,1.7484000000000003E-4,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3942_1","coal",244,null,3942,"Albright Power Station","WV","Unit_1","1","Conventional Boiler","Wall firing - unspecified",81,786,9.7037037037037042,"bituminous","bituminous",5.4696197064041711E-4,1.8070963647676376E-5,1.7535527687745226E-4,null,null,1.8070963647676376E-5,1.7535527687745226E-4,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2732_7","coal",245,null,2732,"Riverbend","NC","7","7","Conventional Boiler","Tangential firing",99.5,1059,10.643216080402009,"bituminous","bituminous",7.233030339198988E-4,1.8077179878870228E-5,1.9239933157511125E-4,null,null,1.8077179878870228E-5,1.9239933157511125E-4,"NOx control","Selective Noncatalytic Reduction","2007-02-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3295_URQ3","coal",246,null,3295,"Urquhart","SC","URQ003","URQ3","Conventional Boiler","Tangential firing",103,1048,10.174757281553399,"bituminous","bituminous",7.0045925329337809E-4,2.0752044690123493E-5,2.1114701781795557E-4,null,null,2.0752044690123493E-5,2.1114701781795557E-4,"PM control","Electrostatic precipitator, cold side, unspecified","1969-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2098_6","coal",247,null,2098,"Lake Road","MO","6","6","Conventional Boiler","Cyclone firing",99,980,9.8989898989898997,"subbituminous,  bituminous","subbituminous,  bituminous",3.0358965692459387E-4,2.1752342087897486E-5,2.1532621460747009E-4,null,null,2.1752342087897486E-5,2.1532621460747009E-4,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1995-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6085_14","coal",248,null,6085,"R.M. Schahfer","IN","R.M.0014","14","Conventional Boiler","Cyclone firing",468,4650,9.9358974358974361,"subbituminous","subbituminous",1.9016467134193033E-4,2.268628043318657E-5,2.2540855558614861E-4,null,null,2.268628043318657E-5,2.2540855558614861E-4,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3098_4","coal",249,null,3098,"Elrama Power Plant","PA","ELR4-2","4","Conventional Boiler","Wall firing - front firing",185,1921,10.383783783783784,"bituminous","bituminous",2.8778031548439047E-4,3.700713554373244E-5,3.8427409394329741E-4,null,null,3.700713554373244E-5,3.8427409394329741E-4,"NOx control","Selective Noncatalytic Reduction","2001-07-01","PM control","Multiple cyclone","1960-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1960-11-01","SO2 control","Wet FGD - Venturi Type","1975-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3098_3","coal",250,null,3098,"Elrama Power Plant","PA","ELR3-2","3","Conventional Boiler","Vertical firing",125,1303,10.423999999999999,"bituminous","bituminous",2.8778031548439047E-4,3.700713554373244E-5,3.8576238090786693E-4,null,null,3.700713554373244E-5,3.8576238090786693E-4,"NOx control","Selective Noncatalytic Reduction","2001-07-01","PM control","Multiple cyclone","1954-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1954-11-01","SO2 control","Wet FGD - Venturi Type","1975-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1218_1","coal",251,null,1218,"Fair Station","IA","U1","1","Conventional Boiler","Wall firing - front firing",24.5,330,13.469387755102041,"coal - bituminous","bituminous",null,null,null,2.9E-5,3.906122448979592E-4,2.9E-5,3.906122448979592E-4,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3098_2","coal",252,null,3098,"Elrama Power Plant","PA","ELR2-2","2","Conventional Boiler","Vertical firing",100,1254,12.54,"bituminous","bituminous",2.8778031548439047E-4,3.700713554373244E-5,4.6406947971840476E-4,null,null,3.700713554373244E-5,4.6406947971840476E-4,"NOx control","Selective Noncatalytic Reduction","2001-07-01","PM control","Multiple cyclone","1953-03-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1953-03-01","SO2 control","Wet FGD - Venturi Type","1975-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3098_1","coal",253,null,3098,"Elrama Power Plant","PA","ELR1-2","1","Conventional Boiler","Vertical firing",100,1254,12.54,"bituminous","bituminous",2.8778031548439047E-4,3.700713554373244E-5,4.6406947971840476E-4,null,null,3.700713554373244E-5,4.6406947971840476E-4,"NOx control","Selective Noncatalytic Reduction","2001-07-01","PM control","Multiple cyclone","1952-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1952-06-01","SO2 control","Wet FGD - Venturi Type","1975-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2848_H-5","coal",254,null,2848,"O H Hutchings","OH","H-5","H-5","Conventional Boiler","Tangential firing",63,641,10.174603174603174,"coal - bituminous","bituminous",null,null,null,5.7199999999999994E-5,5.8198730158730153E-4,5.7199999999999994E-5,5.8198730158730153E-4,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2161_4","coal",255,null,2161,"James River Power Station","MO","Unit_4_JRPS","4","Conventional Boiler","Wall firing - front firing",60,600,10,"subbituminous","subbituminous",2.0184348644446991E-4,2.8104613840999014E-3,2.8104613840999014E-2,null,null,2.8104613840999014E-3,2.8104613840999014E-2,"NOx control","Selective Noncatalytic Reduction","2007-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10773_1","coal",null,null,10773,"Altavista Power Station","VA","U1 & 2","1","Conventional Boiler","Stoker - spreader",34.5,442,12.811594202898551,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","1992-02-01","NOx control","Selective Noncatalytic Reduction","1992-02-01","PM control","Multiple cyclone","1992-02-01","PM control","Multiple cyclone","1992-02-01","SO2 control","Dry FGD - Spray Dryer","1992-02-01","SO2 control","Dry FGD - Spray Dryer","1992-02-01","PM control","Fabric Filter, pulse","1992-02-01","PM control","Fabric Filter, pulse","1992-02-01","","",null,"","",null,"","",null,"",""]
[{"$f":"E258&\"_\"&I258","v":"10769_C-E CONTRACT 24687"},"coal",null,null,10769,"Rio Bravo Poso","CA","Config 1","C-E CONTRACT 24687","Fluidized bed firing","Fluidized bed firing",36,407.93,11.331388888888888,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","1990-03-01","PM control","Fabric Filter, reverse air","1990-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10773_2","coal",null,null,10773,"Altavista Power Station","VA","U1 & 2","2","Conventional Boiler","Stoker - spreader",34.5,447,12.956521739130435,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","1992-02-01","NOx control","Selective Noncatalytic Reduction","1992-02-01","PM control","Multiple cyclone","1992-02-01","PM control","Multiple cyclone","1992-02-01","SO2 control","Dry FGD - Spray Dryer","1992-02-01","SO2 control","Dry FGD - Spray Dryer","1992-02-01","PM control","Fabric Filter, pulse","1992-02-01","PM control","Fabric Filter, pulse","1992-02-01","","",null,"","",null,"","",null,"",""]
["50879_50879","coal",null,null,50879,"Wheelabrator Frackville Energy Co.","PA","1","50879","Fluidized bed firing","Fluidized bed firing",45,590,13.111111111111111,"coal refuse (culm or gob)","coal refuse (culm or gob)",null,null,null,null,null,null,null,"PM control","Fabric Filter, unspecified","1988-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8224_1","coal",null,null,8224,"North Valmy","NV","1","1","Conventional Boiler","Wall firing - opposed firing",243.5,2560,10.513347022587268,"","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1981-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10768_S-1715-3-13","coal",null,null,10768,"Rio Bravo Jasmin","CA","Config 1","S-1715-3-13","Fluidized bed firing","Fluidized bed firing",36,412.16,11.44888888888889,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","1990-03-01","PM control","Fabric Filter, reverse air","1990-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8102_1","coal",null,null,8102,"General James M. Gavin","OH","GA-1","1","Conventional Boiler","Wall firing - opposed firing",1320,11936,9.0424242424242429,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2000-01-01","Other control","Dry sorbent injection","2001-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-04-01","SO2 control","Wet FGD - Spray Type","1994-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8224_2","coal",null,null,8224,"North Valmy","NV","2","2","Conventional Boiler","Wall firing - front firing",270.2,2881,10.662472242783124,"","subbituminous, bituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","1985-05-01","PM control","Fabric Filter, reverse air","1985-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10343_SG-101","coal",null,null,10343,"Foster Wheeler Mt Carmel Cogen","PA","SG-101","SG-101","Fluidized bed firing","Fluidized bed firing",43,505,11.744186046511627,"coal refuse (culm or gob)","coal refuse (culm or gob)",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1990-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8102_2","coal",null,null,8102,"General James M. Gavin","OH","GA-2","2","Conventional Boiler","Wall firing - opposed firing",1320,11936,9.0424242424242429,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2000-01-01","Other control","Dry sorbent injection","2001-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-03-01","SO2 control","Wet FGD - Spray Type","1995-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50835_2","coal",null,null,50835,"TES Filer City Station","MI","TES2-Conf","2","Conventional Boiler","Stoker - spreader",32.200000000000003,408,12.670807453416147,"other--Fuel Type 1 - Coal/Coke/TDF\nFuel Type 2 - Wood Chip","other--Fuel Type 1 - Coal/Coke/TDF\nFuel Type 2 - Wood Chip",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","1990-06-01","PM control","Fabric Filter, pulse","1990-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50835_1","coal",null,null,50835,"TES Filer City Station","MI","TES1-Conf","1","Conventional Boiler","Stoker - spreader",32.200000000000003,408,12.670807453416147,"other--Fuel Type 1 - Coal/Coke/TDF\nFuel Type 2 - Wood Chips","other--Fuel Type 1 - Coal/Coke/TDF\nFuel Type 2 - Wood Chips",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","1990-06-01","PM control","Fabric Filter, pulse","1990-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["54634_1","coal",null,null,54634,"St. Nicholas Cogen Project","PA","1","1","Fluidized bed firing","Fluidized bed firing",99.2,1300,13.104838709677418,"coal refuse (culm or gob)","coal refuse (culm or gob)",null,null,null,null,null,null,null,"PM control","Fabric Filter, pulse","1990-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50611_031","coal",null,null,50611,"WPS Westwood Generation, LLC","PA","001","031","Fluidized bed firing","Fluidized bed firing",36,615,17.083333333333332,"coal refuse (culm or gob)","coal refuse (culm or gob)",null,null,null,null,null,null,null,"PM control","Fabric Filter, pulse","1987-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["889_Unit 1","coal",null,null,889,"Baldwin Energy Complex","IL","001","Unit 1","Conventional Boiler","Cyclone firing",626,5892,9.4121405750798726,"","Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2001-12-01","PM control","Electrostatic precipitator, cold side, unspecified","1970-07-01","Other control","Activated carbon injection","2009-06-01","SO2 control","Dry FGD - Spray Dryer",null,"PM control","Fabric Filter, pulse",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["889_Unit 2","coal",null,null,889,"Baldwin Energy Complex","IL","002","Unit 2","Conventional Boiler","Cyclone firing",628,5996,9.5477707006369421,"","Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2001-12-01","PM control","Electrostatic precipitator, cold side, unspecified","1973-05-01","Other control","Activated carbon injection","2009-06-01","SO2 control","Dry FGD - Spray Dryer",null,"PM control","Fabric Filter, pulse",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["889_Unit 3","coal",null,null,889,"Baldwin Energy Complex","IL","003","Unit 3","Conventional Boiler","Tangential firing",622,6031,9.6961414790996781,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1975-01-01","Other control","Activated carbon injection","2009-06-01","SO2 control","Dry FGD - Spray Dryer",null,"PM control","Fabric Filter, pulse",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["983_5","coal",null,null,983,"Clifty Creek","IN","Unit 5","5","Conventional Boiler","Wall firing - front firing",215,2176.5099999999998,10.123302325581394,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-11-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1978-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["981_4","coal",null,null,981,"State Line","IN","Unit 4","4","Conventional Boiler","Cyclone firing",344,3478,10.11046511627907,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1962-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["983_1","coal",null,null,983,"Clifty Creek","IN","Unit 1","1","Conventional Boiler","Wall firing - front firing",215,2305.8420000000001,10.724846511627907,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-07-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["983_2","coal",null,null,983,"Clifty Creek","IN","Unit 2","2","Conventional Boiler","Wall firing - front firing",215,2247.252,10.45233488372093,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-04-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["988_1","coal",null,null,988,"Tanners Creek","IN","TC-1","1","Conventional Boiler","Vertical firing",152.5,1391,9.1213114754098363,"","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["988_2","coal",null,null,988,"Tanners Creek","IN","TC-2","2","Conventional Boiler","Vertical firing",152.5,1391,9.1213114754098363,"","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["988_3","coal",null,null,988,"Tanners Creek","IN","TC-3","3","Conventional Boiler","Vertical firing",215.4,1844,8.5608170844939639,"","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["990_50","coal",null,null,990,"Harding Street","IN","50s","50","Conventional Boiler","Tangential firing",112,1017,9.0803571428571423,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2004-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1968-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["963_33","coal",null,null,963,"Dallman","IL","33","33","Conventional Boiler","Tangential firing",208,2089.8000000000002,10.047115384615385,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-06-01","SO2 control","Wet FGD - Spray Type","1980-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["709_4","coal",null,null,709,"Harllee Branch","GA","Unit 4","4","Conventional Boiler","Cell burner",520,4874.2980000000007,9.3736500000000014,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-03-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1969-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["710_MB1","coal",null,null,710,"Jack McDonough","GA","MB1","MB1","Conventional Boiler","Tangential firing",270,2490.9899999999998,9.2258888888888873,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["728_Y4BR","coal",null,null,728,"Yates","GA","Y4BR","Y4BR","Conventional Boiler","Tangential firing",138,1421.82,10.30304347826087,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1970-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["728_Y5BR","coal",null,null,728,"Yates","GA","Y5BR","Y5BR","Conventional Boiler","Tangential firing",145,1440.692,9.9358068965517248,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1968-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["728_Y7BR","coal",null,null,728,"Yates","GA","Y7BR","Y7BR","Conventional Boiler","Tangential firing",361,3437.8199999999997,9.5230470914127423,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["983_6","coal",null,null,983,"Clifty Creek","IN","Unit 6","6","Conventional Boiler","Wall firing - front firing",215,2206.0219999999999,10.260567441860465,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1977-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["898_Unit 4","coal",null,null,898,"Wood River","IL","4","Unit 4","Conventional Boiler","Tangential firing",97,1181,12.175257731958762,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1954-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["898_Unit 5","coal",null,null,898,"Wood River","IL","5","Unit 5","Conventional Boiler","Tangential firing",391,4123,10.544757033248082,"","Subbituminous",null,null,null,null,null,null,null,"Other control","Activated carbon injection","2009-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2002-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["983_3","coal",null,null,983,"Clifty Creek","IN","Unit 3","3","Conventional Boiler","Wall firing - front firing",215,2233.7980000000002,10.389758139534885,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["983_4","coal",null,null,983,"Clifty Creek","IN","Unit 4","4","Conventional Boiler","Wall firing - front firing",215,2224.4670000000001,10.346358139534884,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-01-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["991_4","coal",null,null,991,"Eagle Valley","IN","4","4","Conventional Boiler","Tangential firing",60,741,12.35,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1973-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["728_Y6BR","coal",null,null,728,"Yates","GA","Y6BR","Y6BR","Conventional Boiler","Tangential firing",363,3492.8960000000002,9.6223030303030317,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1008_1","coal",null,null,1008,"R. Gallagher","IN","1-2007","1","Conventional Boiler","Wall firing - front firing",150,1460,9.7333333333333325,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, shake and deflate","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1010_2","coal",null,null,1010,"Wabash River","IN","2","2","Conventional Boiler","Wall firing - front firing",90,923.69500000000005,10.263277777777779,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1994-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1010_3","coal",null,null,1010,"Wabash River","IN","3","3","Conventional Boiler","Wall firing - front firing",90,923.69500000000005,10.263277777777779,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1994-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1010_5","coal",null,null,1010,"Wabash River","IN","5","5","Conventional Boiler","Wall firing - front firing",103,1079.0931,10.476632038834952,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1994-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1040_1","coal",null,null,1040,"Whitewater Valley","IN","001","1","Conventional Boiler","Wall firing - unspecified",36,385,10.694444444444445,"","Bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2004-03-01","PM control","Electrostatic precipitator, unspecified","1974-01-11","PM control","Fabric Filter, unspecified","2009-01-06","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1040_2","coal",null,null,1040,"Whitewater Valley","IN","002","2","Conventional Boiler","Tangential firing",69,730,10.579710144927537,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2003-09-01","PM control","Electrostatic precipitator, unspecified","1973-05-16","PM control","Fabric Filter, unspecified","2009-01-06","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2527_6","coal",null,null,2527,"AES Greenidge","NY","Unit 4","6","Conventional Boiler","Tangential firing",112,1117,9.9732142857142865,"coal - bituminous, petroleum coke","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2007-05-01","NOx control","Selective Noncatalytic Reduction","2007-05-01","Other control","Activated carbon injection","2007-05-01","SO2 control","Dry FGD - Circulating Dry Scrubber","2007-05-01","PM control","Fabric Filter, pulse","2006-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1043_2SG1","coal",null,null,1043,"Frank E. Ratts","IN","2SG1conf1","2SG1","Conventional Boiler","Wall firing - front firing",131,1142,8.7175572519083975,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["995_7","coal",null,null,995,"Bailly","IN","7","7","Conventional Boiler","Cyclone firing",176,1638,9.3068181818181817,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2008-03-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-06-01","SO2 control","Wet FGD - Packed Type","1992-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1058_2","coal",null,null,1058,"Sixth Street","IA","Unit 2","2","Conventional Boiler","Wall firing - front firing",13.3,304,22.857142857142858,"coal - subbituminous","natural gas, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1968-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1058_3","coal",null,null,1058,"Sixth Street","IA","Unit 3","3","Conventional Boiler","Wall firing - front firing",13.9,304,21.870503597122301,"coal - subbituminous","natural gas, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1969-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1058_4","coal",null,null,1058,"Sixth Street","IA","Unit 4","4","Conventional Boiler","Wall firing - front firing",14.8,304,20.54054054054054,"coal - subbituminous","natural gas, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1969-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1058_5","coal",null,null,1058,"Sixth Street","IA","Unit 5","5","Conventional Boiler","Wall firing - front firing",32.299999999999997,389,12.043343653250774,"coal - subbituminous","natural gas, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1082_1","coal",null,null,1082,"Walter Scott Jr. Energy Center","IA","1","1","Conventional Boiler","Wall firing - unspecified",45,656,14.577777777777778,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1082_2","coal",null,null,1082,"Walter Scott Jr. Energy Center","IA","2","2","Conventional Boiler","Tangential firing",94,935,9.9468085106382986,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1131_7","coal",null,null,1131,"Streeter Station","IA","7","7","Conventional Boiler","Wall firing - front firing",38.4,473,12.317708333333334,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1043_1SG1","coal",null,null,1043,"Frank E. Ratts","IN","1SG1conf1","1SG1","Conventional Boiler","Wall firing - front firing",130,1142,8.7846153846153854,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1046_1","coal",null,null,1046,"Dubuque","IA","Unit 1","1","Conventional Boiler","Wall firing - front firing",37.6,605.79999999999995,16.111702127659573,"coal - bituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["994_2","coal",null,null,994,"AES Petersburg","IN","2ss","2","Conventional Boiler","Tangential firing",445,4144,9.3123595505617978,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-12-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1969-12-01","SO2 control","Wet FGD - Spray Type","1996-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["995_8","coal",null,null,995,"Bailly","IN","8","8","Conventional Boiler","Cyclone firing",352,3374,9.5852272727272734,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2006-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1981-02-01","SO2 control","Wet FGD - Packed Type","1992-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1001_2","coal",null,null,1001,"Cayuga","IN","2-2008-FGDIN","2","Conventional Boiler","Tangential firing",525,5040,9.6,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2006-01-01","SO2 control","Wet FGD - Spray Type","2008-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1004_7-1","coal",null,null,1004,"Edwardsport","IN","7-1","7-1","Conventional Boiler","Wall firing - front firing",42.75,510,11.929824561403509,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1008_3","coal",null,null,1008,"R. Gallagher","IN","3-2008","3","Conventional Boiler","Wall firing - front firing",150,1460,9.7333333333333325,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, shake and deflate","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1004_8-1","coal",null,null,1004,"Edwardsport","IN","8-1","8-1","Conventional Boiler","Wall firing - front firing",42.75,510,11.929824561403509,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["991_3","coal",null,null,991,"Eagle Valley","IN","3","3","Conventional Boiler","Tangential firing",46,524,11.391304347826088,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1975-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1046_5","coal",null,null,1046,"Dubuque","IA","Unit 5","5","Conventional Boiler","Wall firing - front firing",29.2,337.3,11.551369863013699,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1047_3","coal",null,null,1047,"Lansing","IA","Unit 3","3","Conventional Boiler","Wall firing - front firing",31.9,452.9,14.197492163009404,"coal - bituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E322&\"_\"&I322","v":"991_5"},"coal",null,null,991,"Eagle Valley","IN","5","5","Conventional Boiler","Tangential firing",66,741,11.227272727272727,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["994_1","coal",null,null,994,"AES Petersburg","IN","1s","1","Conventional Boiler","Tangential firing",255,2200,8.6274509803921564,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1967-12-01","SO2 control","Wet FGD - Spray Type","1996-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["994_3","coal",null,null,994,"AES Petersburg","IN","3ss","3","Conventional Boiler","Tangential firing",580,5540,9.5517241379310338,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-12-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1977-12-01","SO2 control","Wet FGD - Spray Type","1977-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3_1","coal",null,null,3,"Barry","AL","Unit 1","1","Conventional Boiler","Tangential firing",145,1380.8842005000001,9.5233393137931035,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2006-05-01","PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1976-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1008_4","coal",null,null,1008,"R. Gallagher","IN","4-2008","4","Conventional Boiler","Wall firing - front firing",150,1460,9.7333333333333325,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, shake and deflate","2008-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["59_1","coal",null,null,59,"Platte","NE","1","1","Conventional Boiler","Tangential firing",110,1048,9.5272727272727273,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1982-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50_2","coal",null,null,50,"Widows Creek","AL","2","2","Conventional Boiler","Wall firing - front firing",140.6,1528,10.867709815078237,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50_3","coal",null,null,50,"Widows Creek","AL","3","3","Conventional Boiler","Wall firing - front firing",140.6,1528,10.867709815078237,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50_4","coal",null,null,50,"Widows Creek","AL","4","4","Conventional Boiler","Wall firing - front firing",140.6,1528,10.867709815078237,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50_5","coal",null,null,50,"Widows Creek","AL","5","5","Conventional Boiler","Wall firing - front firing",140.6,1589,11.301564722617355,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50_6","coal",null,null,50,"Widows Creek","AL","6","6","Conventional Boiler","Wall firing - front firing",140.6,1589,11.301564722617355,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50_7","coal",null,null,50,"Widows Creek","AL","7","7","Conventional Boiler","Tangential firing",575,5681,9.8800000000000008,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","Other control","Other (specify): Sodium bisulfite to control opacity","2003-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1981-12-01","SO2 control","Wet FGD - Venturi Type","1981-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50_8","coal",null,null,50,"Widows Creek","AL","8","8","Conventional Boiler","Tangential firing",550,5839,10.616363636363637,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","Other control","Other (specify): Hydrated lime to control opacity","2004-05-01","PM control","PM scrubber - Venturi","1978-01-01","SO2 control","Wet FGD - Venturi Type","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["645_3","coal",null,null,645,"Big Bend","FL","BB03_SCR_iso","3","Conventional Boiler","Wall firing - opposed firing",400,4115,10.2875,"coal - bituminous, petroleum coke","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2008-07-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1976-05-01","SO2 control","Wet FGD - Packed Type","2008-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["56_3","coal",null,null,56,"Charles R. Lowman","AL","3D","3","Conventional Boiler","Wall firing - opposed firing",258,2500,9.6899224806201545,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-06-01","NOx control","Selective Catalytic Reduction","2007-12-01","SO2 control","Wet FGD - Spray Type","1980-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["87_1","coal",null,null,87,"Escalante","NM","1","1","Conventional Boiler","Tangential firing",260,2366,9.1,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1984-01-01","SO2 control","Wet FGD - Spray Type","1984-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["108_SGU1","coal",null,null,108,"HOLCOMB","KS","SGU1","SGU1","Conventional Boiler","Wall firing - opposed firing",387,3389,8.7571059431524549,"","subbituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","1983-08-01","PM control","Fabric Filter, reverse air","1983-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["113_1","coal",null,null,113,"Cholla","AZ","001","1","Conventional Boiler","Tangential firing",131,1270,9.6946564885496187,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, unspecified","2007-01-01","SO2 control","Wet FGD - Venturi Type","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["113_2","coal",null,null,113,"Cholla","AZ","002","2","Conventional Boiler","Tangential firing",305,2938,9.6327868852459009,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","PM scrubber - Venturi","1978-01-01","SO2 control","Wet FGD - Venturi Type","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["56_2","coal",null,null,56,"Charles R. Lowman","AL","2","2","Conventional Boiler","Wall firing - opposed firing",258,2500,9.6899224806201545,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-06-01","NOx control","Selective Catalytic Reduction","2007-12-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10_1","coal",null,null,10,"Greene County","AL","Unit 1","1","Conventional Boiler","Wall firing - opposed firing",272,2452.6240000000003,9.0170000000000012,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1975-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3_2","coal",null,null,3,"Barry","AL","Unit 2","2","Conventional Boiler","Tangential firing",145,1372.7464499600001,9.4672168962758629,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2006-07-01","PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1976-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3_3","coal",null,null,3,"Barry","AL","Unit 3","3","Conventional Boiler","Tangential firing",263,2434.4651799059998,9.2565215966007592,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2006-07-01","PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3_4","coal",null,null,3,"Barry","AL","Unit 4","4","Conventional Boiler","Tangential firing",376,3512.6520801700003,9.3421597876861711,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2006-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1985-01-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1976-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7_1","coal",null,null,7,"Gadsden","AL","Unit 1","1","Conventional Boiler","Tangential firing",68,792.06151999999997,11.647963529411765,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1964-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7_2","coal",null,null,7,"Gadsden","AL","Unit 2","2","Conventional Boiler","Tangential firing",70,847.83672006000006,12.111953143714286,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1964-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8_10","coal",null,null,8,"Gorgas","AL","Unit 10","10","Conventional Boiler","Tangential firing",720,6523.7939999700002,9.0608249999583332,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-10-01","SO2 control","Wet FGD - Spray Type","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8_6","coal",null,null,8,"Gorgas","AL","Unit 6","6","Conventional Boiler","Wall firing - front firing",110,1291.84600032,11.744054548363637,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8_7","coal",null,null,8,"Gorgas","AL","Unit 7","7","Conventional Boiler","Wall firing - front firing",110,1218.3293700299998,11.075721545727271,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["50_1","coal",null,null,50,"Widows Creek","AL","1","1","Conventional Boiler","Wall firing - front firing",140.6,1528,10.867709815078237,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8_9","coal",null,null,8,"Gorgas","AL","Unit 9","9","Conventional Boiler","Tangential firing",185,1738.6247499249998,9.3979716212162145,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1972-06-01","SO2 control","Wet FGD - Spray Type","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["47_5","coal",null,null,47,"Colbert","AL","5","5","Conventional Boiler","Wall firing - opposed firing",550,5547,10.085454545454546,"coal - bituminous, coal - subbituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10_2","coal",null,null,10,"Greene County","AL","Unit 2","2","Conventional Boiler","Wall firing - opposed firing",260,2392.8209999999999,9.2031576923076912,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1975-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["26_1","coal",null,null,26,"E. C. Gaston","AL","Unit 1","1","Conventional Boiler","Wall firing - front firing",270,2430.236240102,9.0008749633407401,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1974-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["26_2","coal",null,null,26,"E. C. Gaston","AL","Unit 2","2","Conventional Boiler","Wall firing - front firing",270,2511.8462400000003,9.3031342222222229,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1975-04-01","PM control","Fabric Filter, pulse","1999-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["26_3","coal",null,null,26,"E. C. Gaston","AL","Unit 3","3","Conventional Boiler","Wall firing - front firing",270,2462.7794800699999,9.1214054817407408,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1973-12-01","PM control","Fabric Filter, pulse","1996-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["26_4","coal",null,null,26,"E. C. Gaston","AL","Unit 4","4","Conventional Boiler","Wall firing - front firing",270,2468.3519999999999,9.1420444444444442,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1972-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["47_1","coal",null,null,47,"Colbert","AL","1","1","Conventional Boiler","Wall firing - front firing",200,2121,10.605,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["47_2","coal",null,null,47,"Colbert","AL","2","2","Conventional Boiler","Wall firing - front firing",200,2121,10.605,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8_8","coal",null,null,8,"Gorgas","AL","Unit 8","8","Conventional Boiler","Tangential firing",175,1600.8972500399998,9.1479842859428562,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1972-06-01","SO2 control","Wet FGD - Spray Type","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["709_2","coal",null,null,709,"Harllee Branch","GA","Unit 2","2","Conventional Boiler","Wall firing - front firing",332,3091.7249999999999,9.31242469879518,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1967-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1977-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["130_2","coal",null,null,130,"Cross","SC","C2","2","Conventional Boiler","Tangential firing",595,6011,10.102521008403361,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-05-01","SO2 control","Wet FGD - Spray Type","1984-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["643_1","coal",null,null,643,"Lansing Smith","FL","Unit 1","1","Conventional Boiler","Tangential firing",172,1728.2159999999999,10.047767441860465,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-06-01","PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","2007-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["645_1","coal",null,null,645,"Big Bend","FL","BB01_pre-SCR","1","Conventional Boiler","Wall firing - opposed firing",410,4037,9.8463414634146336,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1970-10-01","SO2 control","Wet FGD - Packed Type","1999-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["645_4","coal",null,null,645,"Big Bend","FL","BB04_SCR_iso","4","Conventional Boiler","Tangential firing",465,4330,9.3118279569892479,"coal - bituminous, petroleum coke, coal refuse","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2007-06-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1985-02-01","SO2 control","Wet FGD - Packed Type","2008-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["663_B-2","coal",null,null,663,"Deerhaven Generating Station","FL","001","B-2","Conventional Boiler","Wall firing - unspecified",235,2428,10.331914893617022,"","Bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, unspecified","1987-10-01","NOx control","Selective Catalytic Reduction","2009-05-01","SO2 control","Dry FGD - Unspecified","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["593_4","coal",null,null,593,"Edge Moor","DE","4","4","Conventional Boiler","Tangential firing",182,1900,10.43956043956044,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-05-01","SO2 control","Dry FGD - Sorbent Injection","2009-01-01","Other control","Activated carbon injection",null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1983-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["709_1","coal",null,null,709,"Harllee Branch","GA","Unit 1","1","Conventional Boiler","Cell burner",267,2542.694,9.5231985018726597,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1965-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["593_3","coal",null,null,593,"Edge Moor","DE","3","3","Conventional Boiler","Tangential firing",92,991,10.771739130434783,"","oil - other, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-05-01","SO2 control","Dry FGD - Sorbent Injection","2009-01-01","Other control","Activated carbon injection",null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1983-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["709_3","coal",null,null,709,"Harllee Branch","GA","Unit 3","3","Conventional Boiler","Cell burner",513,4825.8289999999997,9.4070740740740728,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1981-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1968-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["727_3","coal",null,null,727,"Mitchell","GA","Unit 3","3","Conventional Boiler","Tangential firing",164,855,5.2134146341463419,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["728_Y2BR","coal",null,null,728,"Yates","GA","Y2BR","Y2BR","Conventional Boiler","Tangential firing",105,1171.8,11.16,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1968-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["728_Y3BR","coal",null,null,728,"Yates","GA","Y3BR","Y3BR","Conventional Boiler","Tangential firing",105,1250.704,11.911466666666666,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1969-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["733_1","coal",null,null,733,"Kraft","GA","Unit 1","1","Conventional Boiler","Tangential firing",50,547.53600000000006,10.95072,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["733_2","coal",null,null,733,"Kraft","GA","Unit 2","2","Conventional Boiler","Tangential firing",54,532.58400000000006,9.8626666666666676,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["733_3","coal",null,null,733,"Kraft","GA","Unit 3","3","Conventional Boiler","Tangential firing",107,1052.3340000000001,9.8348971962616822,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1004_7-2","coal",null,null,1004,"Edwardsport","IN","7-2","7-2","Conventional Boiler","Wall firing - front firing",42.75,510,11.929824561403509,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["136_1","coal",null,null,136,"Seminole Generating Station","FL","Unit 1","1","Conventional Boiler","Wall firing - opposed firing",694,7172,10.334293948126801,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2009-02-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-01-01","Other control","Dry sorbent injection","2009-02-01","SO2 control","Wet FGD - Spray Type","1984-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["136_2","coal",null,null,136,"Seminole Generating Station","FL","Unit 2","2","Conventional Boiler","Wall firing - opposed firing",694,7172,10.334293948126801,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2009-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-12-01","Other control","Dry sorbent injection","2009-04-01","SO2 control","Wet FGD - Spray Type","1984-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["160_2","coal",null,null,160,"Apache Station","AZ","ST2","2","Conventional Boiler","Turbo",204,1932.521,9.4731421568627443,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-06-01","SO2 control","Wet FGD - Spray Type","1978-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["160_3","coal",null,null,160,"Apache Station","AZ","ST3","3","Conventional Boiler","Turbo",204,1932.521,9.4731421568627443,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-06-01","SO2 control","Wet FGD - Spray Type","1978-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["207_PPBoiler1","coal",null,null,207,"St Johns River Power Park","FL","PPUnit1Configuration","PPBoiler1","Conventional Boiler","Wall firing - opposed firing",660,6144,9.3090909090909086,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2009-07-01","NOx control","Other (specify): Ammonia Injection for SO3 Mitigation","2009-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1988-03-01","SO2 control","Wet FGD - Spray/Tray Type","1986-12-01","SO2 control","Wet FGD - Spray Type","1986-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["207_PPBoiler2","coal",null,null,207,"St Johns River Power Park","FL","PPUnit2Configuration","PPBoiler2","Conventional Boiler","Wall firing - opposed firing",660,6144,9.3090909090909086,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2009-03-01","NOx control","Other (specify): Ammonia Injection for SO3 Mitigation","2009-03-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1986-12-01","SO2 control","Wet FGD - Spray/Tray Type","1988-03-01","SO2 control","Wet FGD - Spray Type","1988-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["508_4","coal",null,null,508,"Lamar Plant","CO","001","4","Fluidized bed firing","Fluidized bed firing",44,509.8,11.586363636363636,"","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Fabric Filter, unspecified","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E386&\"_\"&I386","v":"564_1"},"coal",null,null,564,"Stanton Energy Center","FL","1 coal","1","Conventional Boiler","Wall firing - opposed firing",468,4286,9.1581196581196576,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1987-05-01","SO2 control","Wet FGD - Spray Type","1987-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["628_2","coal",null,null,628,"Crystal River Power Plant","FL","CryR_Cfg_2","2","Conventional Boiler","Tangential firing",515,4161,8.0796116504854361,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["628_4","coal",null,null,628,"Crystal River Power Plant","FL","CryR_Cfg_4","4","Conventional Boiler","Wall firing - opposed firing",769,7613,9.8998699609882959,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["492_6","coal",null,null,492,"Martin Drake","CO","Unit 6 - Coal","6","Conventional Boiler","Wall firing - front firing",85,930,10.941176470588236,"","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1978-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1745_9A","coal",null,null,1745,"Trenton Channel Power Plant","MI","TC9A-Config","9A","Conventional Boiler","Tangential firing",540,4045,7.4907407407407405,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1969-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1695_4","coal",null,null,1695,"B.C. Cobb","MI","BCCobb4-Conf","4","Conventional Boiler","Tangential firing",167,1656,9.9161676646706578,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2000-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1702_1","coal",null,null,1702,"D.E. Karn","MI","DEK1-Conf","1","Conventional Boiler","Tangential firing",275,2445,8.8909090909090907,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1959-12-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1976-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1702_2","coal",null,null,1702,"D.E. Karn","MI","DEK2-Conf","2","Conventional Boiler","Wall firing - front firing",281,2587,9.2064056939501775,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1959-12-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1976-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1720_8","coal",null,null,1720,"J.C. Weadock","MI","JCW8-Conf","8","Conventional Boiler","Tangential firing",166.5,1475,8.8588588588588593,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1733_1","coal",null,null,1733,"Monroe Power Plant","MI","MN1-Config","1","Conventional Boiler","Wall firing - opposed firing",810,7140,8.8148148148148149,"","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1733_2","coal",null,null,1733,"Monroe Power Plant","MI","MN2-Config","2","Conventional Boiler","Wall firing - opposed firing",815,7140,8.7607361963190176,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1743_2","coal",null,null,1743,"St Clair Power Plant","MI","SC2-Config","2","Conventional Boiler","Wall firing - front firing",163,1750,10.736196319018404,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1743_3","coal",null,null,1743,"St Clair Power Plant","MI","SC3-Config","3","Conventional Boiler","Wall firing - front firing",174,1765,10.14367816091954,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1897_3","coal",null,null,1897,"Hibbard Energy Center","MN","HREC3","3","Conventional Boiler","Stoker - spreader",35,518,14.8,"","",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1949-01-01","PM control","Electrostatic precipitator, unspecified","1987-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1743_6","coal",null,null,1743,"St Clair Power Plant","MI","SC6-Config","6","Conventional Boiler","Tangential firing",331,3045,9.1993957703927496,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1893_4","coal",null,null,1893,"Boswell Energy Center","MN","BEC4","4","Conventional Boiler","Tangential firing",587.5,5947,10.122553191489361,"","Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction",null,"PM control","PM scrubber - Venturi","1980-01-01","SO2 control","Wet FGD - Unspecified","1980-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1831_EUBoiler1","coal",null,null,1831,"Otto E. Eckert Station","MI","001","EUBoiler1","Conventional Boiler","Wall firing - front firing",40,509,12.725,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1831_EUBoiler2","coal",null,null,1831,"Otto E. Eckert Station","MI","002","EUBoiler2","Conventional Boiler","Tangential firing",38,522,13.736842105263158,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1831_EUBoiler3","coal",null,null,1831,"Otto E. Eckert Station","MI","003","EUBoiler3","Conventional Boiler","Tangential firing",40,522,13.05,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1831_EUBoiler4","coal",null,null,1831,"Otto E. Eckert Station","MI","004","EUBoiler4","Conventional Boiler","Wall firing - front firing",72,807,11.208333333333334,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1891_1","coal",null,null,1891,"Laskin Energy Center","MN","LEC1","1","Conventional Boiler","Tangential firing",60,725,12.083333333333334,"coal - bituminous, coal - subbituminous","natural gas, subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","PM scrubber - wet","1971-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1891_2","coal",null,null,1891,"Laskin Energy Center","MN","LEC2","2","Conventional Boiler","Tangential firing",55,660,12,"coal - bituminous, coal - subbituminous","natural gas, subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","PM scrubber - wet","1971-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1893_1","coal",null,null,1893,"Boswell Energy Center","MN","BEC1","1","Conventional Boiler","Wall firing - front firing",73,750,10.273972602739725,"","Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-01-01","PM control","Fabric Filter, unspecified","1977-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1893_2","coal",null,null,1893,"Boswell Energy Center","MN","BEC2","2","Conventional Boiler","Wall firing - front firing",72,750,10.416666666666666,"","Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Fabric Filter, unspecified","1977-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1904_3","coal",null,null,1904,"Black Dog","MN","Boiler 3","3","Conventional Boiler","Wall firing - front firing",96,985,10.260416666666666,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1956-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1743_4","coal",null,null,1743,"St Clair Power Plant","MI","SC4-Config","4","Conventional Boiler","Wall firing - front firing",157,1692,10.777070063694268,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["994_4","coal",null,null,994,"AES Petersburg","IN","4s","4","Conventional Boiler","Tangential firing",584,5550,9.5034246575342465,"bituminous,  No.2 Fuel Oil (distillate)","bituminous,  No.2 Fuel Oil (distillate)",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1986-12-01","SO2 control","Wet FGD - Spray Type","1986-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1695_5","coal",null,null,1695,"B.C. Cobb","MI","BCCobb5-Conf","5","Conventional Boiler","Tangential firing",167.5,1623,9.6895522388059696,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2000-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1710_Unit 3","coal",null,null,1710,"Consumers Energy - J.H. Campbell","MI","JHC3-Conf","Unit 3","Conventional Boiler","Wall firing - front firing",869,8199,9.4349827387802065,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2007-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1720_7","coal",null,null,1720,"J.C. Weadock","MI","JCW7-Conf","7","Conventional Boiler","Tangential firing",166,1560,9.3975903614457827,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1731_1","coal",null,null,1731,"Harbor Beach Power Plant","MI","HB1-Config","1","Conventional Boiler","Wall firing - front firing",110,1181,10.736363636363636,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1968-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1733_4","coal",null,null,1733,"Monroe Power Plant","MI","MN4-Config","4","Conventional Boiler","Wall firing - opposed firing",815,7140,8.7607361963190176,"","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1974-01-01","SO2 control","Wet FGD - Unspecified","2009-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1740_2","coal",null,null,1740,"River Rouge Power Plant","MI","RR2-Config","2","Conventional Boiler","Tangential firing",269,2317,8.6133828996282524,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1897_4","coal",null,null,1897,"Hibbard Energy Center","MN","HREC4","4","Conventional Boiler","Stoker - spreader",36,471,13.083333333333334,"","",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1951-01-01","PM control","Electrostatic precipitator, unspecified","1987-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1743_1","coal",null,null,1743,"St Clair Power Plant","MI","SC1-Config","1","Conventional Boiler","Wall firing - front firing",161,1753,10.888198757763975,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1745_16","coal",null,null,1745,"Trenton Channel Power Plant","MI","TC16-Config","16","Conventional Boiler","Tangential firing",58,603,10.396551724137931,"","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1948-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1966-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1745_17","coal",null,null,1745,"Trenton Channel Power Plant","MI","TC16-Config","17","Conventional Boiler","Tangential firing",58,603,10.396551724137931,"","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1948-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1966-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1745_18","coal",null,null,1745,"Trenton Channel Power Plant","MI","TC16-Config","18","Conventional Boiler","Tangential firing",58,603,10.396551724137931,"","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1948-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1966-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1745_19","coal",null,null,1745,"Trenton Channel Power Plant","MI","TC16-Config","19","Conventional Boiler","Tangential firing",58,603,10.396551724137931,"","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1948-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1966-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1825_3","coal",null,null,1825,"Grand Haven City of J.B. Sims","MI","001","3","Conventional Boiler","Wall firing - unspecified",79.7,755,9.473023839397742,"","Bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Electrostatic precipitator, unspecified","1983-08-01","SO2 control","Wet FGD - Tray Type","1983-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1831_EUBoiler5","coal",null,null,1831,"Otto E. Eckert Station","MI","005","EUBoiler5","Conventional Boiler","Wall firing - front firing",71,807,11.366197183098592,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1831_EUBoiler6","coal",null,null,1831,"Otto E. Eckert Station","MI","006","EUBoiler6","Conventional Boiler","Wall firing - front firing",71,807,11.366197183098592,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1832_EU001","coal",null,null,1832,"Erickson Station","MI","001","EU001","Conventional Boiler","Wall firing - front firing",165,1668,10.109090909090909,"bituminous","bituminous",1.4684080163781838E-4,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1998-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1893_3","coal",null,null,1893,"Boswell Energy Center","MN","BEC3","3","Conventional Boiler","Tangential firing",371.3,4115,11.08268246700781,"subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction",null,"SO2 control","Wet FGD - Spray Type","2009-01-01","Other control","Activated carbon injection",null,"PM control","Fabric Filter, unspecified","2009-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1239_39","coal",null,null,1239,"Riverton","KS","039","39","Conventional Boiler","Wall firing - unspecified",40,426,10.65,"","petroleum coke, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2324_3","coal",null,null,2324,"Reid Gardner","NV","3","3","Conventional Boiler","Wall firing - front firing",111,1237,11.144144144144144,"coal - bituminous, other non-fossil fuel (specify)","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, pulse","2009-02-01","SO2 control","Wet FGD - Venturi Type","1976-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2104_4","coal",null,null,2104,"Meramec","MO","004","4","Conventional Boiler","Wall firing - unspecified",362,3782,10.447513812154696,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1980-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2167_1","coal",null,null,2167,"New Madrid","MO","con1","1","Conventional Boiler","Cyclone firing",600,6000,10,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-02-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2167_2","coal",null,null,2167,"New Madrid","MO","con2","2","Conventional Boiler","Cyclone firing",600,6000,10,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2000-02-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2187_2","coal",null,null,2187,"JE Corette Plant","MT","Corette1","2","Conventional Boiler","Tangential firing",163,1750,10.736196319018404,"","subbituminous",null,null,null,null,null,null,null,"Other control","Activated carbon injection","2009-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1968-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1904_4","coal",null,null,1904,"Black Dog","MN","Boiler 4","4","Conventional Boiler","Wall firing - front firing",178,1735,9.7471910112359552,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1960-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2324_2","coal",null,null,2324,"Reid Gardner","NV","2","2","Conventional Boiler","Wall firing - front firing",111,1215,10.945945945945946,"","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, pulse","2009-04-01","SO2 control","Wet FGD - Venturi Type","1976-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2104_1","coal",null,null,2104,"Meramec","MO","001","1","Conventional Boiler","Tangential firing",128,1566,12.234375,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1979-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2324_4","coal",null,null,2324,"Reid Gardner","NV","4","4","Conventional Boiler","Wall firing - front firing",281,2956,10.519572953736654,"","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, pulse","1983-07-01","SO2 control","Wet FGD - Venturi Type","1983-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2442_1","coal",null,null,2442,"Four Corners","NM","001","1","Conventional Boiler","Wall firing - unspecified",199,1707.7,8.5814070351758804,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Other (specify): PM scrubber - Venturi with FGD","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2442_2","coal",null,null,2442,"Four Corners","NM","002","2","Conventional Boiler","Wall firing - unspecified",197,1707.7,8.6685279187817255,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Other (specify): PM scrubber - Venturi with FGD","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2442_3","coal",null,null,2442,"Four Corners","NM","003","3","Conventional Boiler","Wall firing - unspecified",256,2189.6,8.5531249999999996,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Other (specify): PM scrubber - Venturi with FGD","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2442_4","coal",null,null,2442,"Four Corners","NM","004","4","Conventional Boiler","Cell burner",825,7520,9.1151515151515152,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, unspecified","1982-01-01","SO2 control","Wet FGD - Tray Type","1985-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2442_5","coal",null,null,2442,"Four Corners","NM","005","5","Conventional Boiler","Cell burner",825,7520,9.1151515151515152,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, unspecified","1982-01-01","SO2 control","Wet FGD - Tray Type","1985-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2291_NO4","coal",null,null,2291,"North Omaha","NE","NO4","NO4","Conventional Boiler","Tangential firing",138.19999999999999,1471.0007999999998,10.644,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1976-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1740_3","coal",null,null,1740,"River Rouge Power Plant","MI","RR3-Config","3","Conventional Boiler","Wall firing - front firing",293,2679,9.1433447098976117,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1943_003","coal",null,null,1943,"Hoot Lake","MN","3","003","Conventional Boiler","Wall firing - front firing",83.5,978.7,11.720958083832336,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2049_4","coal",null,null,2049,"Jack Watson","MS","Unit 4","4","Conventional Boiler","Wall firing - front firing",250,2226.86,8.9074400000000011,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1968-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2103_1","coal",null,null,2103,"Labadie","MO","001","1","Conventional Boiler","Tangential firing",630,6183,9.8142857142857149,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"Other control","Other (specify): FGC SO3 Injection","1992-11-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1983-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E450&\"_\"&I450","v":"2103_2"},"coal",null,null,2103,"Labadie","MO","002","2","Conventional Boiler","Tangential firing",623,6183,9.924558587479936,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"Other control","Other (specify): FGC SO3 Injection","1992-11-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1982-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2103_3","coal",null,null,2103,"Labadie","MO","003","3","Conventional Boiler","Tangential firing",633,6107,9.6477093206951032,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"Other control","Other (specify): FGC SO3 Injection","1992-11-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1983-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2103_4","coal",null,null,2103,"Labadie","MO","004","4","Conventional Boiler","Tangential firing",633,6107,9.6477093206951032,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"Other control","Other (specify): FGC SO3 Injection","1992-11-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1983-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2104_3","coal",null,null,2104,"Meramec","MO","003","3","Conventional Boiler","Wall firing - unspecified",282,3172,11.24822695035461,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1980-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2169_2","coal",null,null,2169,"Chamois Power Plant","MO","Unit 2","2","Conventional Boiler","Cyclone firing",50,563,11.26,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2104_2","coal",null,null,2104,"Meramec","MO","002","2","Conventional Boiler","Tangential firing",128,1566,12.234375,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1979-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2291_NO5","coal",null,null,2291,"North Omaha","NE","NO5","NO5","Conventional Boiler","Wall firing - front firing",224,2348.64,10.484999999999999,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1976-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2384_8","coal",null,null,2384,"Deepwater","NJ","Coal-firing","8","Conventional Boiler","Wall firing - front firing",87,820,9.4252873563218387,"","bituminous",null,null,null,null,null,null,null,"Other control","Other (specify): Hydrated lime injection to control HCl","2008-09-01","NOx control","Selective Noncatalytic Reduction","2008-09-01","PM control","Fabric Filter, reverse air","1981-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2049_5","coal",null,null,2049,"Jack Watson","MS","Unit 5","5","Conventional Boiler","Wall firing - front firing",500,4752.8599999999997,9.5057200000000002,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1973-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1915_Boiler 1","coal",null,null,1915,"Allen S King","MN","Unit 1","Boiler 1","Conventional Boiler","Cyclone firing",580,4730,8.1551724137931032,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2007-04-01","SO2 control","Dry FGD - Spray Dryer","2007-04-01","Other control","Activated carbon injection",null,"PM control","Fabric Filter, pulse","2007-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2161_3","coal",null,null,2161,"James River Power Station","MO","Unit_3_JRPS","3","Conventional Boiler","Wall firing - front firing",44,496,11.272727272727273,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2007-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1378_2","coal",null,null,1378,"Paradise","KY","2","2","Conventional Boiler","Cyclone firing",704,6959,9.8849431818181817,"coal - bituminous, coal - subbituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2000-05-01","PM control","PM scrubber - Venturi","1983-12-01","SO2 control","Wet FGD - Venturi Type","1983-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1353_BSU2","coal",null,null,1353,"Big Sandy","KY","BSU-2","BSU2","Conventional Boiler","Wall firing - opposed firing",800,7914,9.8925000000000001,"","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1356_1","coal",null,null,1356,"Ghent","KY","GH1","1","Conventional Boiler","Tangential firing",520,6286,12.088461538461539,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","Other control","Other (specify): Sorbent injection for SO3 reduction","2008-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-12-01","Other control","Other (specify): Sorbent injection for SO3 reduction","2008-06-01","SO2 control","Wet FGD - Spray Type","1994-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1356_2","coal",null,null,1356,"Ghent","KY","GH2","2","Conventional Boiler","Tangential firing",510,5705,11.186274509803921,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1977-03-01","SO2 control","Wet FGD - Spray Type","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1357_5","coal",null,null,1357,"Green River","KY","GR04","5","Conventional Boiler","Wall firing - front firing",102,1374,13.470588235294118,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1975-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1361_5","coal",null,null,1361,"Tyrone","KY","TY3","5","Conventional Boiler","Wall firing - front firing",75,995,13.266666666666667,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1364_4","coal",null,null,1364,"Mill Creek","KY","MC4","4","Conventional Boiler","Wall firing - opposed firing",517,5805,11.228239845261122,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-07-01","SO2 control","Wet FGD - Spray Type","1982-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1250_4","coal",null,null,1250,"Lawrence Energy Center","KS","4","4","Conventional Boiler","Tangential firing",126,1276,10.126984126984127,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","PM scrubber - Venturi","1976-01-01","PM control","PM scrubber - Venturi","1976-01-01","SO2 control","Wet FGD - Spray Type","1976-01-01","SO2 control","Wet FGD - Spray Type","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1378_1","coal",null,null,1378,"Paradise","KY","1","1","Conventional Boiler","Cyclone firing",704,6959,9.8849431818181817,"coal - bituminous, coal - subbituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2001-05-01","PM control","PM scrubber - Venturi","1983-09-01","SO2 control","Wet FGD - Venturi Type","1983-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1378_3","coal",null,null,1378,"Paradise","KY","3","3","Conventional Boiler","Cyclone firing",1150.2,11457,9.9608763693270728,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1981-06-01","SO2 control","Wet FGD - Spray Type","2006-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_1","coal",null,null,1379,"Shawnee","KY","1","1","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1981-06-01","PM control","Fabric Filter, reverse air","1981-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_6","coal",null,null,1379,"Shawnee","KY","6","6","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1980-02-01","PM control","Fabric Filter, reverse air","1980-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_7","coal",null,null,1379,"Shawnee","KY","7","7","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1980-07-01","PM control","Fabric Filter, reverse air","1980-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_8","coal",null,null,1379,"Shawnee","KY","8","8","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1981-02-01","PM control","Fabric Filter, reverse air","1981-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_9","coal",null,null,1379,"Shawnee","KY","9","9","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1981-04-01","PM control","Fabric Filter, reverse air","1981-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1743_7","coal",null,null,1743,"St Clair Power Plant","MI","SC7-Config","7","Conventional Boiler","Tangential firing",465,4547,9.7784946236559147,"","bituminous, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1969-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1382_H2","coal",null,null,1382,"HMP&L Station Two Henderson","KY","2","H2","Conventional Boiler","Wall firing - rear firing",173.1,1866.2,10.781051415366841,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-04-01","SO2 control","Wet FGD - Tray Type","1995-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1239_40","coal",null,null,1239,"Riverton","KS","040","40","Conventional Boiler","Tangential firing",58,600,10.344827586206897,"","petroleum coke, subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1252_10","coal",null,null,1252,"Tecumseh Energy Center","KS","10","10","Conventional Boiler","Tangential firing",145,1423,9.8137931034482762,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1252_9","coal",null,null,1252,"Tecumseh Energy Center","KS","9","9","Conventional Boiler","Tangential firing",82,846,10.317073170731707,"subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1295_1","coal",null,null,1295,"Quindaro","KS","Unit 1","1","Conventional Boiler","Cyclone firing",77,782,10.155844155844155,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1991-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1356_3","coal",null,null,1356,"Ghent","KY","GH3","3","Conventional Boiler","Wall firing - opposed firing",525,5868,11.177142857142858,"bituminous","bituminous",null,null,null,null,null,null,null,"Other control","Other (specify): Sorbent injection for SO3 reduction","2008-06-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1981-05-01","NOx control","Selective Catalytic Reduction","2004-05-01","Other control","Other (specify): Sorbent injection for SO3 reduction","2008-06-01","SO2 control","Wet FGD - Spray Type","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1356_4","coal",null,null,1356,"Ghent","KY","GH4","4","Conventional Boiler","Wall firing - opposed firing",525,5967,11.365714285714287,"bituminous","bituminous",null,null,null,null,null,null,null,"Other control","Other (specify): Sorbent injection for SO3 reduction","2008-06-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1984-06-01","NOx control","Selective Catalytic Reduction","2004-05-01","Other control","Other (specify): Sorbent injection for SO3 reduction","2008-06-01","SO2 control","Wet FGD - Spray Type","2008-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1357_4","coal",null,null,1357,"Green River","KY","GR03","4","Conventional Boiler","Wall firing - front firing",72,1047,14.541666666666666,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1363_6","coal",null,null,1363,"Cane Run","KY","CR6","6","Conventional Boiler","Tangential firing",261,3017,11.559386973180077,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1969-05-01","SO2 control","Wet FGD - Spray Type","1979-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1364_1","coal",null,null,1364,"Mill Creek","KY","MC1","1","Conventional Boiler","Tangential firing",330,3723,11.281818181818181,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-07-01","SO2 control","Wet FGD - Spray Type","1980-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1353_BSU1","coal",null,null,1353,"Big Sandy","KY","BSU-1","BSU1","Conventional Boiler","Wall firing - opposed firing",280.5,2512,8.9554367201426022,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1969-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1364_3","coal",null,null,1364,"Mill Creek","KY","MC3","3","Conventional Boiler","Wall firing - opposed firing",422,4896,11.601895734597157,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-06-01","SO2 control","Wet FGD - Spray Type","1978-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1383_R1","coal",null,null,1383,"Robert A Reid","KY","1","R1","Conventional Boiler","Wall firing - front firing",72,616.6,8.56388888888889,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Single cyclone","1966-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1966-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1077_1","coal",null,null,1077,"Sutherland","IA","Unit 1","1","Conventional Boiler","Wall firing - front firing",31,401.5,12.951612903225806,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1077_2","coal",null,null,1077,"Sutherland","IA","Unit 2","2","Conventional Boiler","Wall firing - front firing",30.9,375.6,12.155339805825244,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1364_2","coal",null,null,1364,"Mill Creek","KY","MC2","2","Conventional Boiler","Tangential firing",330,3788,11.478787878787879,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-06-01","SO2 control","Wet FGD - Spray Type","1981-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1384_2","coal",null,null,1384,"Cooper Station.","KY","Unit 02","2","Conventional Boiler","Wall firing - front firing",240,2418,10.074999999999999,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_10","coal",null,null,1379,"Shawnee","KY","10","10","Fluidized bed firing","Fluidized bed firing",175,1800,10.285714285714286,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1981-07-01","PM control","Fabric Filter, reverse air","1981-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_2","coal",null,null,1379,"Shawnee","KY","2","2","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1981-03-01","PM control","Fabric Filter, reverse air","1981-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_3","coal",null,null,1379,"Shawnee","KY","3","3","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1980-11-01","PM control","Fabric Filter, reverse air","1980-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_4","coal",null,null,1379,"Shawnee","KY","4","4","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1980-05-01","PM control","Fabric Filter, reverse air","1980-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1379_5","coal",null,null,1379,"Shawnee","KY","5","5","Conventional Boiler","Wall firing - front firing",175,1691,9.6628571428571437,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1979-11-01","PM control","Fabric Filter, reverse air","1979-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1381_C1","coal",null,null,1381,"Kenneth C Coleman","KY","4","C1","Conventional Boiler","Wall firing - front firing",157.6,1623,10.298223350253808,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1971-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-08-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-07-01","SO2 control","Wet FGD - Tray Type","2006-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1619_2","coal",null,null,1619,"Brayton Point","MA","BP2","2","Conventional Boiler","Tangential firing",259,2458,9.4903474903474905,"coal - bituminous","subbituminous",null,null,null,null,null,null,null,"Other control","Other (specify): passes a split stream  of flue gas over a vanadium catalyst to generate SO3 from the SO2 in the gas which enhances ESP performance.","1995-03-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1981-07-01","Other control","Activated carbon injection","2008-12-01","SO2 control","Dry FGD - Spray Dryer","2008-06-01","PM control","Fabric Filter, pulse","2007-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1382_H1","coal",null,null,1382,"HMP&L Station Two Henderson","KY","1","H1","Conventional Boiler","Wall firing - rear firing",166.1,1799,10.830824804334739,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-10-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-06-01","SO2 control","Wet FGD - Tray Type","1995-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1381_C2","coal",null,null,1381,"Kenneth C Coleman","KY","4","C2","Conventional Boiler","Wall firing - front firing",146,1632,11.178082191780822,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1971-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-08-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-07-01","SO2 control","Wet FGD - Tray Type","2006-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1385_1","coal",null,null,1385,"Dale Station","KY","01","1","Conventional Boiler","Wall firing - front firing",24,278,11.583333333333334,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1385_2","coal",null,null,1385,"Dale Station","KY","02","2","Conventional Boiler","Wall firing - front firing",24,278,11.583333333333334,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1606_1","coal",null,null,1606,"Mount Tom","MA","1 current","1","Conventional Boiler","Wall firing - front firing",155,1480,9.5483870967741939,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2006-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-09-01","SO2 control","Dry FGD - Circulating Dry Scrubber","2009-12-01","PM control","Fabric Filter, pulse","2009-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1619_1","coal",null,null,1619,"Brayton Point","MA","BP1","1","Conventional Boiler","Tangential firing",258,2528,9.7984496124031004,"coal - bituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2006-10-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1981-03-01","Other control","Activated carbon injection","2007-12-01","SO2 control","Dry FGD - Spray Dryer","2008-07-01","PM control","Fabric Filter, pulse","2008-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1626_2","coal",null,null,1626,"Salem Harbor","MA","Unit 2","2","Conventional Boiler","Wall firing - front firing",78.763000000000005,1014,12.87406523367571,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","1992-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1626_3","coal",null,null,1626,"Salem Harbor","MA","Unit 3","3","Conventional Boiler","Wall firing - front firing",151.751,1783,11.749510711626282,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","1993-08-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1381_C3","coal",null,null,1381,"Kenneth C Coleman","KY","4","C3","Conventional Boiler","Wall firing - rear firing",165,1660,10.060606060606061,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1971-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-08-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-07-01","SO2 control","Wet FGD - Tray Type","2006-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["1384_1","coal",null,null,1384,"Cooper Station.","KY","Unit 01","1","Conventional Boiler","Wall firing - front firing",124,1381,11.137096774193548,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3403_4","coal",null,null,3403,"Gallatin","TN","4","4","Conventional Boiler","Tangential firing",327.60000000000002,3032,9.2551892551892543,"coal - subbituminous, coal - bituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3138_4","coal",null,null,3138,"New Castle Plant","PA","NC4-2","4","Conventional Boiler","Wall firing - front firing",114,1025,8.9912280701754383,"coal - subbituminous, coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2005-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3264_3","coal",null,null,3264,"W. S. Lee","SC","3","3","Conventional Boiler","Tangential firing",182.1,2252,12.366831411312466,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1971-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E514&\"_\"&I514","v":"3280_CAN1"},"coal",null,null,3280,"Canadys Steam","SC","CAN001","CAN1","Conventional Boiler","Tangential firing",121,1141.5,9.4338842975206614,"","Bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3280_CAN2","coal",null,null,3280,"Canadys Steam","SC","CAN002","CAN2","Conventional Boiler","Tangential firing",123,1175.7,9.5585365853658537,"","Bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3317_1","coal",null,null,3317,"Dolphus M Grainger","SC","G1","1","Conventional Boiler","Wall firing - front firing",87,940,10.804597701149426,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1966-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3317_2","coal",null,null,3317,"Dolphus M Grainger","SC","G2","2","Conventional Boiler","Wall firing - front firing",87,972,11.172413793103448,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1966-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3393_3","coal",null,null,3393,"Allen Steam Plant","TN","3","3","Conventional Boiler","Cyclone firing",330,3064,9.2848484848484851,"coal - subbituminous, coal - bituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_9","coal",null,null,3406,"Johnsonville","TN","9","9","Conventional Boiler","Wall firing - front firing",172.8,1734,10.034722222222221,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3152_2A","coal",null,null,3152,"Sunbury Generation LP","PA","Boiler 2A","2A","Conventional Boiler","Arch firing",40,525,13.125,"coal - bituminous","petroleum coke, bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1970-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2872_4","coal",null,null,2872,"Muskingum River","OH","MR-4","4","Conventional Boiler","Cyclone firing",237.5,2150,9.0526315789473681,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2952_5","coal",null,null,2952,"Muskogee","OK","MK5 Config","5","Conventional Boiler","Tangential firing",415,5373.0016000000005,12.946991807228917,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1978-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2952_6","coal",null,null,2952,"Muskogee","OK","MK6 Config","6","Conventional Boiler","Tangential firing",371,5214.8899999999994,14.056307277628031,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1984-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3122_2","coal",null,null,3122,"Homer City Station","PA","HC2CONFIG","2","Conventional Boiler","Wall firing - opposed firing",655,5690.5520000000006,8.687865648854963,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2000-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1970-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3122_3","coal",null,null,3122,"Homer City Station","PA","HC3CONFIG","3","Conventional Boiler","Wall firing - opposed firing",680,6175,9.0808823529411757,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2001-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1977-12-01","SO2 control","Wet FGD - Spray Type","2001-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3122_1","coal",null,null,3122,"Homer City Station","PA","HC1CONFIG","1","Conventional Boiler","Wall firing - opposed firing",655,5898.6799999999994,9.0056183206106866,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2001-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1969-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3405_1","coal",null,null,3405,"John Sevier","TN","1","1","Conventional Boiler","Tangential firing",200,1967,9.8350000000000009,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2007-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2872_5","coal",null,null,2872,"Muskingum River","OH","MR-5","5","Conventional Boiler","Cyclone firing",615.20000000000005,5550,9.0214564369310786,"","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2005-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2876_1","coal",null,null,2876,"Kyger Creek","OH","Unit 1","1","Conventional Boiler","Wall firing - front firing",214,2111.4100000000003,9.8664018691588797,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-10-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1980-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2876_2","coal",null,null,2876,"Kyger Creek","OH","Unit 2","2","Conventional Boiler","Wall firing - front firing",213,2135.931,10.027845070422535,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-12-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1980-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2963_3313","coal",null,null,2963,"Northeastern","OK","NE-3","3313","Conventional Boiler","Tangential firing",490,4775,9.7448979591836729,"subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2963_3314","coal",null,null,2963,"Northeastern","OK","NE-4","3314","Conventional Boiler","Tangential firing",490,4775,9.7448979591836729,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3113_1","coal",null,null,3113,"Portland","PA","POR-1","1","Conventional Boiler","Tangential firing",172,1719,9.9941860465116275,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1989-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3113_2","coal",null,null,3113,"Portland","PA","POR-2","2","Conventional Boiler","Tangential firing",255,2542,9.9686274509803923,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1987-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2535_1","coal",null,null,2535,"AES Cayuga, LLC","NY","Unit_1","1","Conventional Boiler","Tangential firing",164,1462,8.9146341463414629,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction",null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning",null,"SO2 control","Wet FGD - Spray Type","1995-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3399_1","coal",null,null,3399,"Cumberland","TN","1","1","Conventional Boiler","Wall firing - opposed firing",1300,14130,10.86923076923077,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","Other control","Other (specify): Hydrated Lime for Opacity","2006-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-06-01","SO2 control","Wet FGD - Spray Type","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_4","coal",null,null,3406,"Johnsonville","TN","4","4","Conventional Boiler","Tangential firing",125,1405,11.24,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2007-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_5","coal",null,null,3406,"Johnsonville","TN","5","5","Conventional Boiler","Tangential firing",147,1566,10.653061224489797,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_6","coal",null,null,3406,"Johnsonville","TN","6","6","Conventional Boiler","Tangential firing",147,1566,10.653061224489797,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_2","coal",null,null,3407,"Kingston","TN","2","2","Conventional Boiler","Tangential firing",175,1641,9.3771428571428572,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_3","coal",null,null,3407,"Kingston","TN","3","3","Conventional Boiler","Tangential firing",175,1641,9.3771428571428572,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_4","coal",null,null,3407,"Kingston","TN","4","4","Conventional Boiler","Tangential firing",175,1641,9.3771428571428572,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_5","coal",null,null,3407,"Kingston","TN","5","5","Conventional Boiler","Tangential firing",200,2056,10.28,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_10","coal",null,null,3406,"Johnsonville","TN","10","10","Conventional Boiler","Wall firing - front firing",172.8,1734,10.034722222222221,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3776_52","coal",null,null,3776,"Glen Lyn","VA","GL-5","52","Conventional Boiler","Tangential firing",50,572,11.44,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_1","coal",null,null,3406,"Johnsonville","TN","1","1","Conventional Boiler","Tangential firing",125,1405,11.24,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2005-07-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3788_4","coal",null,null,3788,"Potomac River","VA","4","4","Conventional Boiler","Tangential firing",108,961,8.8981481481481488,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Sorbent Injection","2006-05-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-10-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1956-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3936_2","coal",null,null,3936,"Kanawha River","WV","KR-2","2","Conventional Boiler","Vertical firing",219.6,1950,8.8797814207650276,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1969-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3938_11","coal",null,null,3938,"Philip Sporn","WV","SP-1","11","Conventional Boiler","Vertical firing",152.5,1311,8.5967213114754095,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1980-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3938_21","coal",null,null,3938,"Philip Sporn","WV","SP-2","21","Conventional Boiler","Vertical firing",152.5,1311,8.5967213114754095,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1980-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3938_31","coal",null,null,3938,"Philip Sporn","WV","SP-3","31","Conventional Boiler","Vertical firing",152.5,1311,8.5967213114754095,"","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-01-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_7","coal",null,null,3406,"Johnsonville","TN","7","7","Conventional Boiler","Wall firing - front firing",172.8,1734,10.034722222222221,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1989-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_8","coal",null,null,3406,"Johnsonville","TN","8","8","Conventional Boiler","Wall firing - front firing",172.8,1734,10.034722222222221,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3776_51","coal",null,null,3776,"Glen Lyn","VA","GL-5","51","Conventional Boiler","Tangential firing",50,572,11.44,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3297_WAT1","coal",null,null,3297,"Wateree","SC","WAT001","WAT1","Conventional Boiler","Wall firing - unspecified",383,3329.7,8.69373368146214,"","Bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Fabric Filter, unspecified","2001-05-01","SO2 control","Wet FGD - Unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3140_3","coal",null,null,3140,"PPL Brunner Island","PA","U3","3","Conventional Boiler","Tangential firing",780,7239,9.2807692307692307,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2007-06-01","SO2 control","Wet FGD - Tray Type","2009-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3178_1","coal",null,null,3178,"Armstrong Power Station","PA","Unit 1","1","Conventional Boiler","Wall firing - unspecified",184,1749,9.5054347826086953,"","Bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3178_2","coal",null,null,3178,"Armstrong Power Station","PA","Unit 2","2","Conventional Boiler","Wall firing - unspecified",183,1706,9.3224043715846996,"","Bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3181_33","coal",null,null,3181,"Mitchell Power Station","PA","033","33","Conventional Boiler","Tangential firing",289,2563,8.8685121107266429,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1971-01-01","SO2 control","Wet FGD - Spray Type","1983-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3264_1","coal",null,null,3264,"W. S. Lee","SC","1","1","Conventional Boiler","Tangential firing",105.9,1215,11.473087818696884,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1969-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3264_2","coal",null,null,3264,"W. S. Lee","SC","2","2","Conventional Boiler","Tangential firing",105.8,1215,11.483931947069944,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/ flue gas conditioning","1969-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3406_2","coal",null,null,3406,"Johnsonville","TN","2","2","Conventional Boiler","Tangential firing",125,1405,11.24,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2008-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2876_5","coal",null,null,2876,"Kyger Creek","OH","Unit 5","5","Conventional Boiler","Wall firing - front firing",213,2129.6379999999999,9.9983004694835671,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1980-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3297_WAT2","coal",null,null,3297,"Wateree","SC","WAT002","WAT2","Conventional Boiler","Wall firing - unspecified",380,3305.1,8.6976315789473677,"","Bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-04-01","PM control","Fabric Filter, unspecified","2001-07-01","SO2 control","Wet FGD - Unspecified",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3319_3","coal",null,null,3319,"Jefferies","SC","J3","3","Conventional Boiler","Wall firing - front firing",164,1780,10.853658536585366,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3319_4","coal",null,null,3319,"Jefferies","SC","J4","4","Conventional Boiler","Wall firing - front firing",162,1602,9.8888888888888893,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1970-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3393_1","coal",null,null,3393,"Allen Steam Plant","TN","1","1","Conventional Boiler","Cyclone firing",330,3064,9.2848484848484851,"coal - subbituminous, coal - bituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3393_2","coal",null,null,3393,"Allen Steam Plant","TN","2","2","Conventional Boiler","Cyclone firing",330,3064,9.2848484848484851,"coal - subbituminous, coal - bituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1971-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3399_2","coal",null,null,3399,"Cumberland","TN","2","2","Conventional Boiler","Wall firing - opposed firing",1300,14130,10.86923076923077,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","Other control","Other (specify): Hydrated Lime for opacity","2006-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-06-01","SO2 control","Wet FGD - Spray Type","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3403_1","coal",null,null,3403,"Gallatin","TN","1","1","Conventional Boiler","Tangential firing",300,2750,9.1666666666666661,"coal - subbituminous, coal - bituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3403_3","coal",null,null,3403,"Gallatin","TN","3","3","Conventional Boiler","Tangential firing",327.60000000000002,3032,9.2551892551892543,"coal - subbituminous, coal - bituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2713_3","coal",null,null,2713,"L.V. Sutton Electric Plant","NC","Sut_Cfg_3b","3","Conventional Boiler","Wall firing - rear firing",420,3695,8.7976190476190474,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2005-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2952_4","coal",null,null,2952,"Muskogee","OK","MK4 Config","4","Conventional Boiler","Tangential firing",391,5360.25,13.709079283887467,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2723_1","coal",null,null,2723,"Dan River","NC","1","1","Conventional Boiler","Tangential firing",71,1140,16.056338028169016,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2723_2","coal",null,null,2723,"Dan River","NC","2","2","Conventional Boiler","Tangential firing",70.400000000000006,1140,16.193181818181817,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2727_Unit 2","coal",null,null,2727,"Marshall","NC","U22007","Unit 2","Conventional Boiler","Tangential firing",400,3663.2,9.1579999999999995,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2007-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2002-01-01","SO2 control","Wet FGD - Spray Type","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2727_Unit 3","coal",null,null,2727,"Marshall","NC","U3","Unit 3","Conventional Boiler","Tangential firing",700,6103.1,8.7187142857142863,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2008-12-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2006-12-01","SO2 control","Wet FGD - Spray Type","2007-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E578&\"_\"&I578","v":"2732_10"},"coal",null,null,2732,"Riverbend","NC","10","10","Conventional Boiler","Tangential firing",141.1,1318,9.3408929836995043,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2006-10-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2716_3","coal",null,null,2716,"W.H. Weatherspoon Plant","NC","Wea_Cfg_3","3","Conventional Boiler","Tangential firing",79,962,12.177215189873417,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2713_2","coal",null,null,2713,"L.V. Sutton Electric Plant","NC","Sut_Cfg_1","2","Conventional Boiler","Wall firing - front firing",110,1081,9.827272727272728,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1975-05-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2718_ES-2","coal",null,null,2718,"G G Allen","NC","2-2009","ES-2","Conventional Boiler","Tangential firing",177,1509,8.5254237288135588,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2007-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1988-10-01","SO2 control","Wet FGD - Spray Type","2009-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2718_ES-5","coal",null,null,2718,"G G Allen","NC","5-2009","ES-5","Conventional Boiler","Tangential firing",285.3,2705,9.4812478093235182,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2008-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2000-06-01","SO2 control","Wet FGD - Spray Type","2009-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2720_Boiler 5","coal",null,null,2720,"Buck","NC","5","Boiler 5","Conventional Boiler","Tangential firing",40,619,15.475,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2720_Boiler 6","coal",null,null,2720,"Buck","NC","6","Boiler 6","Conventional Boiler","Tangential firing",40,619,15.475,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2720_Boiler 7","coal",null,null,2720,"Buck","NC","7","Boiler 7","Conventional Boiler","Tangential firing",40,619,15.475,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2723_3","coal",null,null,2723,"Dan River","NC","3","3","Conventional Boiler","Tangential firing",151,1710,11.324503311258278,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2713_1","coal",null,null,2713,"L.V. Sutton Electric Plant","NC","Sut_Cfg_1","1","Conventional Boiler","Tangential firing",103,1081,10.495145631067961,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1975-05-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2535_2","coal",null,null,2535,"AES Cayuga, LLC","NY","Unit_2","2","Conventional Boiler","Tangential firing",168,1450,8.6309523809523814,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning",null,"SO2 control","Wet FGD - Spray Type","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2718_ES-1","coal",null,null,2718,"G G Allen","NC","1-2009","ES-1","Conventional Boiler","Tangential firing",176.2,1738,9.8637911464245178,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1988-10-01","SO2 control","Wet FGD - Spray Type","2009-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2549_68","coal",null,null,2549,"CR Huntley Generating Station","NY","068","68","Conventional Boiler","Tangential firing",201,1836,9.1343283582089558,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction",null,"SO2 control","Dry FGD - Sorbent Injection",null,"Other control","Activated carbon injection",null,"PM control","Fabric Filter, unspecified","2008-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2732_8","coal",null,null,2732,"Riverbend","NC","8","8","Conventional Boiler","Tangential firing",100,1059,10.59,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2007-10-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2708_6","coal",null,null,2708,"Cape Fear Steam Electric Plant","NC","Cap_Cfg_6b","6","Conventional Boiler","Tangential firing",184,1752,9.5217391304347831,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2006-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2709_1","coal",null,null,2709,"H.F. Lee Plant","NC","Lee_Cfg_1","1","Conventional Boiler","Tangential firing",80,704,8.8000000000000007,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1974-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2709_2","coal",null,null,2709,"H.F. Lee Plant","NC","Lee_Cfg_1","2","Conventional Boiler","Wall firing - front firing",82,833,10.158536585365853,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1974-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2709_3","coal",null,null,2709,"H.F. Lee Plant","NC","Lee_Cfg_3b","3","Conventional Boiler","Wall firing - opposed firing",260,2412,9.2769230769230777,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2007-03-19","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2549_67","coal",null,null,2549,"CR Huntley Generating Station","NY","067","67","Conventional Boiler","Tangential firing",204,1836,9,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction",null,"SO2 control","Dry FGD - Sorbent Injection",null,"Other control","Activated carbon injection",null,"PM control","Fabric Filter, unspecified","2009-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2830_4","coal",null,null,2830,"Walter C Beckjord","OH","4","4","Conventional Boiler","Tangential firing",162,1423,8.783950617283951,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1974-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2830_5","coal",null,null,2830,"Walter C Beckjord","OH","5","5","Conventional Boiler","Tangential firing",255,2367,9.2823529411764714,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2830_6","coal",null,null,2830,"Walter C Beckjord","OH","6","6","Conventional Boiler","Tangential firing",443,3979,8.9819413092550793,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2836_10","coal",null,null,2836,"Avon Lake","OH","AL10","10","Conventional Boiler","Tangential firing",101,1447,14.326732673267326,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2836_12","coal",null,null,2836,"Avon Lake","OH","AL12-2","12","Conventional Boiler","Wall firing - opposed firing",680,6581,9.677941176470588,"","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2004-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1985-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2840_4","coal",null,null,2840,"Conesville","OH","CV-4","4","Conventional Boiler","Tangential firing",841.5,7960,9.4592988710635773,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2009-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-06-01","Other control","Dry sorbent injection","2009-06-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2009-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2840_5","coal",null,null,2840,"Conesville","OH","CV-5","5","Conventional Boiler","Tangential firing",443.9,4091,9.2160396485694989,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-09-01","SO2 control","Wet FGD - Spray Type","1977-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2727_Unit 1","coal",null,null,2727,"Marshall","NC","U12007","Unit 1","Conventional Boiler","Tangential firing",400,3658.2,9.1455000000000002,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2006-04-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1998-12-01","SO2 control","Wet FGD - Spray Type","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2848_H-4","coal",null,null,2848,"O H Hutchings","OH","H-4","H-4","Conventional Boiler","Tangential firing",64,696,10.875,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2824_10","coal",null,null,2824,"Stanton","ND","u10","10","Conventional Boiler","Tangential firing",60,642,10.7,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","2000-01-01","PM control","Fabric Filter, reverse air","2000-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2848_H-6","coal",null,null,2848,"O H Hutchings","OH","H-6","H-6","Conventional Boiler","Tangential firing",60.5,646,10.677685950413224,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2850_B003","coal",null,null,2850,"J M Stuart","OH","MS3W","B003","Conventional Boiler","Wall firing - opposed firing",623,5800,9.3097913322632415,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-02-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-05-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2008-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2850_B004","coal",null,null,2850,"J M Stuart","OH","MS4W","B004","Conventional Boiler","Wall firing - opposed firing",623,5800,9.3097913322632415,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-02-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1974-06-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2008-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2872_1","coal",null,null,2872,"Muskingum River","OH","MR-1","1","Conventional Boiler","Wall firing - front firing",219.6,2050,9.3351548269581066,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2872_2","coal",null,null,2872,"Muskingum River","OH","MR-2","2","Conventional Boiler","Wall firing - front firing",219.6,2050,9.3351548269581066,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2872_3","coal",null,null,2872,"Muskingum River","OH","MR-3","3","Conventional Boiler","Cyclone firing",237.5,2150,9.0526315789473681,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2876_3","coal",null,null,2876,"Kyger Creek","OH","Unit 3","3","Conventional Boiler","Wall firing - front firing",213,2138.1010000000001,10.038032863849766,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-02-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1980-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2876_4","coal",null,null,2876,"Kyger Creek","OH","Unit 4","4","Conventional Boiler","Wall firing - front firing",213,2158.7159999999999,10.134816901408451,"coal - bituminous, coal - subbituminous","bituminous, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-04-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1980-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3788_5","coal",null,null,3788,"Potomac River","VA","5","5","Conventional Boiler","Tangential firing",108,961,8.8981481481481488,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Sorbent Injection","2006-05-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-10-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1957-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2848_H-3","coal",null,null,2848,"O H Hutchings","OH","H-3","H-3","Conventional Boiler","Tangential firing",62.5,716,11.456,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2832_Unit 8","coal",null,null,2832,"Miami Fort","OH","U8","Unit 8","Conventional Boiler","Wall firing - opposed firing",550,5003,9.0963636363636358,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2001-01-01","SO2 control","Wet FGD - Spray Type","2007-01-01","Other control","Dry sorbent injection","2007-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2917_9","coal",null,null,2917,"Hamilton","OH","Unit 9","9","Conventional Boiler","Tangential firing",50.6,729,14.407114624505928,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1974-06-01","SO2 control","Dry FGD - Spray Dryer","2001-06-01","PM control","Single cyclone","1997-01-01","PM control","Fabric Filter, pulse","1997-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2732_9","coal",null,null,2732,"Riverbend","NC","9","9","Conventional Boiler","Tangential firing",141.69999999999999,1318,9.3013408609738892,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2006-11-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1995-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2790_B1","coal",null,null,2790,"R.M. Heskett Station","ND","B1","B1","Conventional Boiler","Stoker - traveling grate",22,320,14.545454545454545,"","Lignite, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2790_B2","coal",null,null,2790,"R.M. Heskett Station","ND","B2","B2","Fluidized bed firing","Fluidized bed firing",78,900,11.538461538461538,"","Lignite, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, unspecified","1976-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2828_2","coal",null,null,2828,"Cardinal","OH","CD-U2","2","Conventional Boiler","Wall firing - opposed firing",615.20000000000005,5275,8.5744473342002596,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-01-01","Other control","Dry sorbent injection","2007-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-05-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2007-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2830_1","coal",null,null,2830,"Walter C Beckjord","OH","1","1","Conventional Boiler","Tangential firing",100,971,9.7100000000000009,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2830_2","coal",null,null,2830,"Walter C Beckjord","OH","2","2","Conventional Boiler","Tangential firing",100,999,9.99,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2830_3","coal",null,null,2830,"Walter C Beckjord","OH","3","3","Conventional Boiler","Wall firing - opposed firing",135,1215,9,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1971-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2832_Unit 7","coal",null,null,2832,"Miami Fort","OH","U7","Unit 7","Conventional Boiler","Wall firing - opposed firing",550,4995,9.081818181818182,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2007-01-01","SO2 control","Wet FGD - Spray Type","2007-01-01","Other control","Dry sorbent injection","2007-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2828_1","coal",null,null,2828,"Cardinal","OH","CD-U1","1","Conventional Boiler","Wall firing - opposed firing",615.20000000000005,5275,8.5744473342002596,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-01-01","Other control","Dry sorbent injection","2008-03-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-05-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2008-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2840_6","coal",null,null,2840,"Conesville","OH","CV-6","6","Conventional Boiler","Tangential firing",443.9,4091,9.2160396485694989,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-03-01","SO2 control","Wet FGD - Spray Type","1977-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2843_9","coal",null,null,2843,"Picway","OH","PI","9","Conventional Boiler","Wall firing - front firing",106.2,1290,12.146892655367232,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2848_H-1","coal",null,null,2848,"O H Hutchings","OH","H-1","H-1","Conventional Boiler","Tangential firing",53,607,11.452830188679245,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2848_H-2","coal",null,null,2848,"O H Hutchings","OH","H-2","H-2","Conventional Boiler","Tangential firing",53,574,10.830188679245284,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2850_B001","coal",null,null,2850,"J M Stuart","OH","MS1W","B001","Conventional Boiler","Wall firing - opposed firing",623,5800,9.3097913322632415,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-02-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-05-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2850_B002","coal",null,null,2850,"J M Stuart","OH","MS2W","B002","Conventional Boiler","Wall firing - opposed firing",623,5800,9.3097913322632415,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-02-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1970-10-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2824_1","coal",null,null,2824,"Stanton","ND","u1","1","Conventional Boiler","Wall firing - front firing",132,1800,13.636363636363637,"subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2000-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","2000-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["2832_Unit 6","coal",null,null,2832,"Miami Fort","OH","U6","Unit 6","Conventional Boiler","Tangential firing",175,1253,7.16,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1960-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6166_MB2","coal",null,null,6166,"Rockport","IN","RP-2","MB2","Conventional Boiler","Wall firing - opposed firing",1320,12374,9.3742424242424249,"subbituminous","subbituminous",null,null,null,null,null,null,null,"Other control","Activated carbon injection","2009-09-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1989-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6177_U2B","coal",null,null,6177,"Coronado Generating Station","AZ","U2B","U2B","Conventional Boiler","Wall firing - unspecified",456.6,4719,10.33508541392904,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, unspecified","1980-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6113_5","coal",null,null,6113,"Gibson","IN","5","5","Conventional Boiler","Wall firing - opposed firing",661,6655,10.068078668683812,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"Other control","Other (specify): Soda Ash Injection for SO3 mitigation","2004-06-01","NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-01-01","SO2 control","Wet FGD - Spray Type","1982-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6124_1","coal",null,null,6124,"McIntosh","GA","Unit 1","1","Conventional Boiler","Wall firing - front firing",165,1598.3344999999999,9.6868757575757574,"oil - distillate","No.2 Fuel Oil (distillate)",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1981-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6139_2","coal",null,null,6139,"Welsh","TX","WE-2","2","Conventional Boiler","Wall firing - opposed firing",558,5156,9.2401433691756267,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1980-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6166_MB1","coal",null,null,6166,"Rockport","IN","RP-1","MB1","Conventional Boiler","Wall firing - opposed firing",1320,12374,9.3742424242424249,"","bituminous, subbituminous",null,null,null,null,null,null,null,"Other control","Activated carbon injection","2009-09-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E642&\"_\"&I642","v":"6170_1"},"coal",null,null,6170,"Pleasant Prairie","WI","PPPPB1","1","Conventional Boiler","Wall firing - opposed firing",655,6449,9.8458015267175565,"subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2006-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-06-01","SO2 control","Wet FGD - Spray Type","2006-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6204_1","coal",null,null,6204,"Laramie River Station","WY","1","1","Conventional Boiler","Wall firing - opposed firing",605,6420,10.611570247933884,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-07-01","SO2 control","Wet FGD - Tray Type","1980-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6204_2","coal",null,null,6204,"Laramie River Station","WY","2","2","Conventional Boiler","Wall firing - opposed firing",602,6420,10.664451827242525,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1981-07-01","SO2 control","Wet FGD - Tray Type","1981-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6204_3","coal",null,null,6204,"Laramie River Station","WY","3","3","Conventional Boiler","Wall firing - opposed firing",610,6600,10.819672131147541,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","1982-11-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6213_1SG1","coal",null,null,6213,"Merom","IN","1SG1conf1","1SG1","Conventional Boiler","Wall firing - opposed firing",515,5088,9.8796116504854368,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1983-11-01","SO2 control","Wet FGD - Packed Type","1983-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6213_2SG1","coal",null,null,6213,"Merom","IN","2SG1conf2","2SG1","Conventional Boiler","Wall firing - opposed firing",515,5088,9.8796116504854368,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1982-02-01","SO2 control","Wet FGD - Packed Type","1982-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6249_1","coal",null,null,6249,"Winyah","SC","W1","1","Conventional Boiler","Wall firing - rear firing",295,2904,9.8440677966101688,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-03-01","SO2 control","Wet FGD - Spray Type","2007-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6249_2","coal",null,null,6249,"Winyah","SC","W2","2","Conventional Boiler","Wall firing - opposed firing",305,2908,9.5344262295081972,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-07-01","SO2 control","Wet FGD - Spray Type","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6139_3","coal",null,null,6139,"Welsh","TX","WE-3","3","Conventional Boiler","Wall firing - opposed firing",558,5156,9.2401433691756267,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1982-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6090_1","coal",null,null,6090,"Sherburne County","MN","Unit 1","1","Conventional Boiler","Tangential firing",741,6909,9.3238866396761129,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","PM scrubber - Venturi","1976-05-01","SO2 control","Wet FGD - Spray Type","1976-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2001-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6061_1","coal",null,null,6061,"South Mississippi El Pwr Assn","MS","1","1","Conventional Boiler","Turbo",204,2600,12.745098039215685,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-04-01","SO2 control","Wet FGD - Venturi Type","1978-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6061_2","coal",null,null,6061,"South Mississippi El Pwr Assn","MS","2","2","Conventional Boiler","Turbo",204,2600,12.745098039215685,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-04-01","SO2 control","Wet FGD - Venturi Type","1978-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6068_3","coal",null,null,6068,"Jeffrey Energy Center","KS","3","3","Conventional Boiler","Tangential firing",783,7815,9.980842911877394,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1983-05-01","SO2 control","Wet FGD - Spray Type","1983-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6071_1","coal",null,null,6071,"Trimble Co.","KY","TC01","1","Conventional Boiler","Tangential firing",547,5602,10.241316270566728,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-12-01","Other control","Other (specify): Sorbent injection for SO3 reduction","2008-07-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1990-09-01","Other control","Other (specify): Sorbent injection for SO3 reduction","2008-07-01","SO2 control","Wet FGD - Spray Type","1990-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_1","coal",null,null,3407,"Kingston","TN","1","1","Conventional Boiler","Tangential firing",175,1641,9.3771428571428572,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6073_2","coal",null,null,6073,"Victor J. Daniel Jr","MS","Unit 2","2","Conventional Boiler","Tangential firing",536,5166.7280000000001,9.6394179104477615,"coal - subbituminous, coal - bituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1998-01-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1998-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6177_U1B","coal",null,null,6177,"Coronado Generating Station","AZ","U1B","U1B","Conventional Boiler","Wall firing - unspecified",456.6,4719,10.33508541392904,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, unspecified","1979-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6170_2","coal",null,null,6170,"Pleasant Prairie","WI","PPPPB2","2","Conventional Boiler","Wall firing - opposed firing",643,6449,10.029548989113531,"subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-04-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1985-05-01","SO2 control","Wet FGD - Spray Type","2007-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6090_2","coal",null,null,6090,"Sherburne County","MN","Unit 2","2","Conventional Boiler","Tangential firing",737,6770,9.1858887381275434,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","PM scrubber - Venturi","1977-04-01","SO2 control","Wet FGD - Spray Type","1977-04-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","2001-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6096_NC1","coal",null,null,6096,"Nebraska City","NE","NC1","NC1","Conventional Boiler","Wall firing - front firing",646,6554.9620000000004,10.147,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6138_1","coal",null,null,6138,"Flint Creek","AR","FC-1","1","Conventional Boiler","Wall firing - opposed firing",558,6324,11.333333333333334,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6082_1","coal",null,null,6082,"AES Somerset LLC","NY","001","1","Conventional Boiler","Wall firing - opposed firing",680.8,6280,9.2244418331374867,"","Bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","1999-01-01","Other control","Dry sorbent injection",null,"PM control","Electrostatic precipitator, unspecified","1984-01-01","SO2 control","Wet FGD - Spray Type","1984-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8223_1","coal",null,null,8223,"Springerville","AZ","1","1","Conventional Boiler","Tangential firing",427,3830,8.9695550351288063,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","1985-06-01","PM control","Fabric Filter, reverse air","1985-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7253_2","coal",null,null,7253,"Richard Gorsuch","OH","UNIT2","2","Conventional Boiler","Radiant",53.3,550.9,10.335834896810507,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7253_4","coal",null,null,7253,"Richard Gorsuch","OH","UNIT4","4","Conventional Boiler","Radiant",53.3,519,9.7373358348968111,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8042_Unit 2","coal",null,null,8042,"Belews Creek Steam Station","NC","2-2008","Unit 2","Conventional Boiler","Wall firing - opposed firing",1183,10800,9.1293322062552829,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-01-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1974-01-01","SO2 control","Wet FGD - Spray Type","2008-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6641_2","coal",null,null,6641,"Independence","AR","002","2","Conventional Boiler","Tangential firing",879,8700,9.8976109215017072,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1984-12-06","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8223_2","coal",null,null,8223,"Springerville","AZ","2","2","Conventional Boiler","Tangential firing",430,3830,8.9069767441860463,"bituminous","bituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","1990-06-01","PM control","Fabric Filter, reverse air","1990-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8226_1","coal",null,null,8226,"Cheswick Power Plant","PA","CH2","1","Conventional Boiler","Tangential firing",612,6000,9.8039215686274517,"coal - subbituminous, coal - bituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-04-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1970-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["10002_1","coal",null,null,10002,"ACE Cogeneration Company","CA","Config 1","1","Fluidized bed firing","Fluidized bed firing",117,1052,8.9914529914529915,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","1991-01-01","PM control","Fabric Filter, reverse air","1991-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8219_1","coal",null,null,8219,"Ray D Nixon","CO","Unit 1","1","Conventional Boiler","Wall firing - front firing",225,2095,9.3111111111111118,"subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1980-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7790_1-1","coal",null,null,7790,"Bonanza Power Plant","UT","1-1","1-1","Conventional Boiler","Wall firing - opposed firing",483,4899,10.142857142857142,"Bituminous","Bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1985-11-01","SO2 control","Wet FGD - Spray Type","1985-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6073_1","coal",null,null,6073,"Victor J. Daniel Jr","MS","Unit 1","1","Conventional Boiler","Tangential firing",537,5206.3059999999996,9.6951694599627558,"coal - subbituminous, coal - bituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1998-01-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1998-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6481_1SGA","coal",null,null,6481,"Intermountain Power Project","UT","U1","1SGA","Conventional Boiler","Wall firing - opposed firing",950,8180,8.6105263157894729,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1986-06-01","SO2 control","Wet FGD - Spray Type","1986-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6481_2SGA","coal",null,null,6481,"Intermountain Power Project","UT","U2","2SGA","Conventional Boiler","Wall firing - opposed firing",950,8220,8.6526315789473678,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Fabric Filter, reverse air","1987-05-01","SO2 control","Wet FGD - Spray Type","1987-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6768_1","coal",null,null,6768,"Sikeston Power Station","MO","1","1","Conventional Boiler","Wall firing - opposed firing",233,2780,11.931330472103005,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1981-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6772_1","coal",null,null,6772,"Hugo","OK","001","1","Conventional Boiler","Wall firing - unspecified",465,4567,9.8215053763440867,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1982-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6823_W1","coal",null,null,6823,"D B Wilson","KY","1","W1","Conventional Boiler","Wall firing - opposed firing",443,4477,10.106094808126411,"Bituminous","Bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-10-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-09-01","Other control","Dry sorbent injection","2006-03-01","SO2 control","Wet FGD - Spray Type","1984-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["8042_Unit 1","coal",null,null,8042,"Belews Creek Steam Station","NC","1-2008","Unit 1","Conventional Boiler","Wall firing - opposed firing",1185.8,10800,9.1077753415415756,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-06-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1973-01-01","SO2 control","Wet FGD - Spray Type","2008-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6249_3","coal",null,null,6249,"Winyah","SC","W3","3","Conventional Boiler","Wall firing - opposed firing",305,2877,9.4327868852459016,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2005-04-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1980-05-01","SO2 control","Wet FGD - Spray Type","1980-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6249_4","coal",null,null,6249,"Winyah","SC","W4","4","Conventional Boiler","Wall firing - opposed firing",305,3051,10.00327868852459,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1981-11-01","SO2 control","Wet FGD - Spray Type","1981-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6257_3","coal",null,null,6257,"Scherer","GA","Unit 3","3","Conventional Boiler","Tangential firing",880,9362.5,10.639204545454545,"subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1987-01-01","Other control","Activated carbon injection","2009-02-01","PM control","Fabric Filter, pulse","2009-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6257_4","coal",null,null,6257,"Scherer","GA","Unit 4","4","Conventional Boiler","Tangential firing",880,8821.5853999999999,10.024528863636364,"subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1989-02-01","Other control","Activated carbon injection",null,"PM control","Fabric Filter, pulse",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6264_1","coal",null,null,6264,"Mountaineer","WV","Mt-1","1","Conventional Boiler","Wall firing - opposed firing",1320,11960,9.0606060606060606,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-01-01","Other control","Dry sorbent injection","2007-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-09-01","SO2 control","Wet FGD - Spray Type","2007-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6639_G1","coal",null,null,6639,"R D Green","KY","1","G1","Conventional Boiler","Wall firing - opposed firing",250,2704.2,10.816799999999999,"coal - bituminous, petroleum coke","petroleum coke, bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-12-01","SO2 control","Wet FGD - Spray Type","1979-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6641_1","coal",null,null,6641,"Independence","AR","001","1","Conventional Boiler","Tangential firing",853,8700,10.199296600234467,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, unspecified","1983-01-18","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["7253_1","coal",null,null,7253,"Richard Gorsuch","OH","UNIT1","1","Conventional Boiler","Radiant",53.3,455.3,8.5422138836772987,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1972-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3944_2","coal",null,null,3944,"Harrison Power Station","WV","Boiler2","2","Conventional Boiler","Wall firing - unspecified",692,6042,8.7312138728323703,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, unspecified","1973-12-01","SO2 control","Wet FGD - Spray Type","1994-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4072_7","coal",null,null,4072,"Pulliam","WI","7","7","Conventional Boiler","Wall firing - rear firing",87.7,999,11.391106043329533,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1958-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4042_2","coal",null,null,4042,"Valley","WI","VAPP-B2","2","Conventional Boiler","Wall firing - front firing",72,868,12.055555555555555,"bituminous","bituminous",3.7607415051294743E-4,null,null,null,null,null,null,"PM control","Fabric Filter, pulse","1994-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4042_4","coal",null,null,4042,"Valley","WI","VAPP-B4","4","Conventional Boiler","Wall firing - front firing",72,868,12.055555555555555,"bituminous","bituminous",4.224502483624627E-4,null,null,null,null,null,null,"PM control","Fabric Filter, pulse","1995-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4054_2","coal",null,null,4054,"Nelson Dewey","WI","Unit 2","2","Conventional Boiler","Cyclone firing",117.1,1161,9.9146029035012813,"coal - subbituminous, petroleum coke","petroleum coke, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-01-01","PM control","Electrostatic precipitator, unspecified","1974-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4072_5","coal",null,null,4072,"Pulliam","WI","5","5","Conventional Boiler","Wall firing - rear firing",53.63,693,12.921872086518739,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1953-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4078_2","coal",null,null,4078,"Weston","WI","W2","2","Conventional Boiler","Wall firing - front firing",88.9,1000,11.248593925759279,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1972-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4041_8","coal",null,null,4041,"South Oak Creek","WI","OCPP-B8","8","Conventional Boiler","Tangential firing",336,3009,8.9553571428571423,"subbituminous","subbituminous",1.6794382840427404E-4,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1991-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4271_B1","coal",null,null,4271,"John P. Madgett","WI","001","B1","Conventional Boiler","Turbo",425.73,4029.5,9.4649190801681815,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, unspecified","1979-12-01","PM control","Fabric Filter, unspecified","2007-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3992_8","coal",null,null,3992,"Blount Street","WI","8B6T","8","Conventional Boiler","Wall firing - front firing",53.4,575,10.767790262172285,"coal - bituminous, other non-fossil fuel (specify)","natural gas, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1957-06-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3944_3","coal",null,null,3944,"Harrison Power Station","WV","Boiler3","3","Conventional Boiler","Wall firing - unspecified",692,5876,8.4913294797687868,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, unspecified","1972-12-01","SO2 control","Wet FGD - Spray Type","1994-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3948_1","coal",null,null,3948,"Mitchell","WV","MI-1","1","Conventional Boiler","Wall firing - opposed firing",816.3,7020,8.5997794928335178,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2007-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1977-02-01","SO2 control","Wet FGD - Tray Type","2007-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6031_2","coal",null,null,6031,"Killen Station","OH","2-Operation","2","Conventional Boiler","Wall firing - opposed firing",658,5928,9.009118541033434,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1982-06-01","NOx control","Selective Catalytic Reduction","2003-11-01","SO2 control","Wet FGD - Jet Bubbling Reactor","2007-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3992_9","coal",null,null,3992,"Blount Street","WI","9B7T","9","Conventional Boiler","Wall firing - front firing",53.2,575,10.808270676691729,"coal - bituminous, other non-fossil fuel (specify)","natural gas, bituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1961-07-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4041_5","coal",null,null,4041,"South Oak Creek","WI","OCPP-B5","5","Conventional Boiler","Wall firing - front firing",273,2488,9.1135531135531131,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4041_6","coal",null,null,4041,"South Oak Creek","WI","OCPP-B6","6","Conventional Boiler","Wall firing - front firing",278,2516,9.0503597122302164,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1972-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4054_1","coal",null,null,4054,"Nelson Dewey","WI","Unit 1","1","Conventional Boiler","Cyclone firing",120,1222,10.183333333333334,"coal - subbituminous, petroleum coke","petroleum coke, subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-01-01","PM control","Electrostatic precipitator, unspecified","1974-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
[{"$f":"E706&\"_\"&I706","v":"4072_6"},"coal",null,null,4072,"Pulliam","WI","6","6","Conventional Boiler","Wall firing - rear firing",73.7,875,11.872455902306648,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1951-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3936_1","coal",null,null,3936,"Kanawha River","WV","KR-1","1","Conventional Boiler","Vertical firing",219.6,1950,8.8797814207650276,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1969-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_6","coal",null,null,3407,"Kingston","TN","6","6","Conventional Boiler","Tangential firing",200,2056,10.28,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_7","coal",null,null,3407,"Kingston","TN","7","7","Conventional Boiler","Tangential firing",200,2056,10.28,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-07-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_8","coal",null,null,3407,"Kingston","TN","8","8","Conventional Boiler","Tangential firing",200,2056,10.28,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2004-07-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3407_9","coal",null,null,3407,"Kingston","TN","9","9","Conventional Boiler","Tangential firing",200,2056,10.28,"coal - bituminous, coal - subbituminous","subbituminous, bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2006-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1976-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3776_6","coal",null,null,3776,"Glen Lyn","VA","GL-6","6","Conventional Boiler","Wall firing - front firing",237.5,2040,8.5894736842105264,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3788_1","coal",null,null,3788,"Potomac River","VA","1","1","Conventional Boiler","Tangential firing",93,970,10.43010752688172,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Sorbent Injection","2006-05-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-10-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1949-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3788_2","coal",null,null,3788,"Potomac River","VA","2","2","Conventional Boiler","Tangential firing",93,970,10.43010752688172,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Sorbent Injection","2006-05-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-10-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1950-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3788_3","coal",null,null,3788,"Potomac River","VA","3","3","Conventional Boiler","Tangential firing",108,961,8.8981481481481488,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Sorbent Injection","2006-05-01","PM control","Electrostatic precipitator, hot side, w/o flue gas conditioning","1978-10-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1954-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3935_3","coal",null,null,3935,"John E. Amos","WV","AM-3","3","Conventional Boiler","Wall firing - opposed firing",1300,11936,9.1815384615384623,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2001-05-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1973-10-01","SO2 control","Wet FGD - Spray Type","2009-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3948_2","coal",null,null,3948,"Mitchell","WV","MI-2","2","Conventional Boiler","Wall firing - opposed firing",816.3,7020,8.5997794928335178,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2007-01-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-08-01","SO2 control","Wet FGD - Tray Type","2007-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3938_41","coal",null,null,3938,"Philip Sporn","WV","SP-4","41","Conventional Boiler","Vertical firing",152.5,1311,8.5967213114754095,"","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction","2009-01-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3938_51","coal",null,null,3938,"Philip Sporn","WV","SP-5","51","Conventional Boiler","Wall firing - opposed firing",495.5,3961,7.9939455095862764,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3944_1","coal",null,null,3944,"Harrison Power Station","WV","Boiler1","1","Conventional Boiler","Wall firing - unspecified",693,5779,8.3391053391053394,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2002-05-01","PM control","Electrostatic precipitator, cold side, unspecified","1974-12-01","SO2 control","Wet FGD - Spray Type","1994-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3947_1","coal",null,null,3947,"Kammer","WV","K-1","1","Conventional Boiler","Cyclone firing",237.5,2156,9.0778947368421061,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3947_2","coal",null,null,3947,"Kammer","WV","K-2","2","Conventional Boiler","Cyclone firing",237.5,2156,9.0778947368421061,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3982_5","coal",null,null,3982,"Bay Front","WI","5","5","Conventional Boiler","Cyclone firing",32,389,12.15625,"coal - subbituminous","natural gas, subbituminous",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1976-08-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3992_7","coal",null,null,3992,"Blount Street","WI","7B1345T","7","Conventional Boiler","Cell burner",22.4,310,13.839285714285715,"coal - bituminous","bituminous, natural gas",null,null,null,null,null,null,null,"PM control","Multiple cyclone","1949-12-01","PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1975-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3935_1","coal",null,null,3935,"John E. Amos","WV","AM-1","1","Conventional Boiler","Wall firing - opposed firing",816.3,7020,8.5997794928335178,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction",null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6021_C3","coal",null,null,6021,"Craig","CO","C3","C3","Conventional Boiler","Wall firing - opposed firing",478,4124,8.6276150627615067,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Spray Dryer","1984-10-01","PM control","Fabric Filter, reverse air","1984-10-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6034_1","coal",null,null,6034," Belle River","MI","BR1-Config","1","Conventional Boiler","Wall firing - opposed firing",674,6814,10.109792284866469,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1984-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6034_2","coal",null,null,6034," Belle River","MI","BR2-Config","2","Conventional Boiler","Wall firing - opposed firing",677.1,6814,10.063506129079899,"subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1985-07-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6052_2","coal",null,null,6052,"Wansley","GA","Unit 2","2","Conventional Boiler","Tangential firing",920,8554.2800000000007,9.2981304347826086,"bituminous","bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1978-04-01","SO2 control","Wet FGD - Spray Type","2009-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6064_N1","coal",null,null,6064,"Nearman Creek","KS","N1","N1","Conventional Boiler","Wall firing - front firing",257.39999999999998,2433,9.4522144522144522,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1988-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["3947_3","coal",null,null,3947,"Kammer","WV","K-3","3","Conventional Boiler","Cyclone firing",237.5,2156,9.0778947368421061,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6085_15","coal",null,null,6085,"R.M. Schahfer","IN","R.M.0015","15","Conventional Boiler","Wall firing - opposed firing",502,5100,10.159362549800797,"","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1979-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6085_17","coal",null,null,6085,"R.M. Schahfer","IN","R.M.0017","17","Conventional Boiler","Tangential firing",393,3967,10.0941475826972,"","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1983-04-01","SO2 control","Wet FGD - Spray Type","1983-04-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6085_18","coal",null,null,6085,"R.M. Schahfer","IN","R.M.0018","18","Conventional Boiler","Tangential firing",393,3967,10.0941475826972,"bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1986-01-01","SO2 control","Wet FGD - Spray Type","1986-02-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6095_1","coal",null,null,6095,"Sooner","OK","SO1 Config","1","Conventional Boiler","Tangential firing",401,5428.8091000000004,13.538177306733168,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-11-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6095_2","coal",null,null,6095,"Sooner","OK","SO2 Config","2","Conventional Boiler","Tangential firing",383,5661.8362000000006,14.782862140992169,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-12-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6068_1","coal",null,null,6068,"Jeffrey Energy Center","KS","1","1","Conventional Boiler","Tangential firing",790,8396,10.627848101265823,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1978-07-01","SO2 control","Wet FGD - Spray Type","1978-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4143_1","coal",null,null,4143,"Genoa","WI","001","1","Conventional Boiler","Tangential firing",373.5,3627.69,9.7126907630522084,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"SO2 control","Dry FGD - Unspecified",null,"PM control","Electrostatic precipitator, cold side, unspecified","1969-07-01","PM control","Fabric Filter, unspecified","2007-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6068_2","coal",null,null,6068,"Jeffrey Energy Center","KS","2","2","Conventional Boiler","Tangential firing",786,8124,10.335877862595419,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1980-05-01","SO2 control","Wet FGD - Spray Type","1980-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4140_B5","coal",null,null,4140,"Alma","WI","B5","B5","Conventional Boiler","Wall firing - unspecified",83.5,862.65,10.331137724550898,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Electrostatic precipitator, cold side, unspecified","1974-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4140_B4","coal",null,null,4140,"Alma","WI","B4","B4","Conventional Boiler","Wall firing - unspecified",53.63,557.20000000000005,10.389707253402946,"","Bituminous, Subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Noncatalytic Reduction",null,"PM control","Electrostatic precipitator, cold side, unspecified","1974-06-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4259_1","coal",null,null,4259,"Endicott Station","MI","1","1","Conventional Boiler","Wall firing - front firing",60,617,10.283333333333333,"coal - bituminous","bituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1979-09-01","SO2 control","Wet FGD - Tray Type","1979-09-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6002_1","coal",null,null,6002,"James H. Miller Jr.","AL","Unit 1","1","Conventional Boiler","Wall firing - front firing",725,7015.9856007600001,9.6772215182896559,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2005-05-01","PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1999-05-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6009_2","coal",null,null,6009,"White Bluff","AR","002","2","Conventional Boiler","Tangential firing",881,8700,9.8751418842224741,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1981-07-21","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6009_1","coal",null,null,6009,"White Bluff","AR","001","1","Conventional Boiler","Tangential firing",853,8700,10.199296600234467,"","Subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/o flue gas conditioning","1983-06-17","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["4078_1","coal",null,null,4078,"Weston","WI","W1","1","Conventional Boiler","Wall firing - front firing",63.6,858,13.490566037735849,"coal - subbituminous","subbituminous",null,null,null,null,null,null,null,"PM control","Electrostatic precipitator, cold side, w/ flue gas conditioning","1971-01-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]
["6004_1","coal",null,null,6004,"Pleasants Power Station","WV","001","1","Conventional Boiler","Wall firing - unspecified",700,5969,8.5271428571428576,"","Bituminous",null,null,null,null,null,null,null,"NOx control","Selective Catalytic Reduction","2003-05-01","PM control","Electrostatic precipitator, cold side, unspecified","1979-03-01","SO2 control","Wet FGD - Tray Type","1979-03-01","","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"","",null,"",""]

{"sheet":"Pb_Variability","index":1,"n_rows":306,"n_cols":15,"rows_kept":306,"cut":false,"hidden":false,"merged":[]}
["facility_name","facility_id","boiler_id","configuration_id","compound","Final_EF","Final_EF_Units","Final_Output_EF","Final_Output_EF_Units","From","Report_id","Pb_Min_lb_per_MWh_Rank","New Souce MACT Floor Test_ID","New Source MACT Floor QA Calc","New Source Floor Agreement of QA Calc"]
["Weston",4078,"4","W4","Lead",9.9561881881283049E-8,"lb/MMBtu",8.9650232254762201E-7,"lb/MW","ERT","",1]
["Weston",4078,"4","W4","Lead",1.5466666666666668E-6,"lb/MMBtu",1.3926918944009283E-5,"lb/MW","Part II","W4 Metals 2008",1]
["Reid Gardner",2324,"1","1","Lead",9.0550520926906308E-8,"lb/MMBtu",9.911611074431636E-7,"lb/MW","ERT","",2]
["Dallman",963,"34","34","Lead",1.36E-7,"lb/MMBtu",1.1411787271142112E-6,"lb/MW","Part II","Dallman 34 Test 1",3]
["Dallman",963,"34","34","Lead",1.3900000000000001E-7,"lb/MMBtu",1.1663517872711423E-6,"lb/MW","Part II","Dallman 34 Test 2",3]
["Dallman",963,"34","34","Lead",2.2999999999999999E-7,"lb/MMBtu",1.9299346120313865E-6,"lb/MW","ERT","",3]
["Rawhide",6761,"101","Rawhide101","Lead",1.3236249390726807E-7,"lb/MMBtu",1.2151310916077068E-6,"lb/MW","ERT","",4]
["Brandon Shores",602,"2","002","Lead",1.4170611592242315E-7,"lb/MMBtu",1.3759869227249785E-6,"lb/MW","ERT","",5]
["Logan Generating Plant",10043,"B01","Unit1","Lead",1.8498897230757785E-7,"lb/MMBtu",1.6195145444883523E-6,"lb/MW","ERT","",6]
["Logan Generating Plant",10043,"B01","Unit1","Lead",4.4100000000000008E-5,"lb/MMBtu",3.8608026479106339E-4,"lb/MW","Part II","2005 Annual Stack Test-4",6]
["Havana",891,"Boiler 9","Boiler 9","Lead",1.5554931996104345E-7,"lb/MMBtu",1.6266384187194357E-6,"lb/MW","ERT","",7]
["TransAlta Centralia Generation",3845,"BD21","BW21CONFIG","Lead",1.2895774185617486E-7,"lb/MMBtu",1.6559200583621261E-6,"lb/MW","ERT","",8]
["PSEG Mercer Generating Station",2408,"E1","MERU1E1PT1OS1-Coal","Lead",1.8878896062676965E-7,"lb/MMBtu",1.7062559123702212E-6,"lb/MW","ERT","",9]
["PSEG Mercer Generating Station",2408,"E1","MERU1E1PT1OS1-Coal","Lead",5.3333333333333334E-7,"lb/MMBtu",4.8202137998056365E-6,"lb/MW","Part II","MER1 2009 1YR ST Co NG",9]
["AES Hawaii",10673,"BLR B","002","Lead",1.8823205922902722E-7,"lb/MMBtu",1.7510217765916011E-6,"lb/MW","ERT","",10]
["Walter Scott Jr. Energy Center",1082,"4","4","Lead",1.9999999999999999E-7,"lb/MMBtu",1.8058823529411763E-6,"lb/MW","Part II","8/2007 PB",11]
["Walter Scott Jr. Energy Center",1082,"4","4","Lead",1.420508740800985E-6,"lb/MMBtu",1.2826358336055953E-5,"lb/MW","ERT","",11]
["Walter Scott Jr. Energy Center",1082,"4","4","Lead",3.0000000000000001E-6,"lb/MMBtu",2.7088235294117647E-5,"lb/MW","Part II","5/2007 PB",11]
["Cholla",113,"4","004","Lead",1.8284497621474502E-7,"lb/MMBtu",1.8361937846694866E-6,"lb/MW","ERT","",12]
["Chambers Cogeneration LP",10566,"Boil 2","Boil 2","Lead",1.997125060274261E-7,"lb/MMBtu",1.9438683920002806E-6,"lb/MW","ERT","",13]
["Asheville Steam Electric Plant",2706,"1","Ash_Cfg_1d","Lead",2.1842222222222225E-7,"lb/MMBtu",2.0196141706924317E-6,"lb/MW","Part II","Ash_Blr_1_Test_8t",14]
["Asheville Steam Electric Plant",2706,"1","Ash_Cfg_1d","Lead",7.0733333333333329E-7,"lb/MMBtu",6.5402705314009657E-6,"lb/MW","Part II","Ash_Blr_1_Test_10e",14]
["Asheville Steam Electric Plant",2706,"1","Ash_Cfg_1d","Lead",4.029236022004867E-6,"lb/MMBtu",3.7255834522305875E-5,"lb/MW","ERT","",14]
["Asheville Steam Electric Plant",2706,"2","Ash_Cfg_2","Lead",2.1983216160725487E-7,"lb/MMBtu",2.0496116243970527E-6,"lb/MW","ERT","",15]
["Asheville Steam Electric Plant",2706,"2","Ash_Cfg_2","Lead",4.3100000000000003E-7,"lb/MMBtu",4.0184411764705884E-6,"lb/MW","Part II","Ash_Blr_2_Test_8e",15]
["Asheville Steam Electric Plant",2706,"2","Ash_Cfg_2","Lead",6.2800000000000006E-7,"lb/MMBtu",5.8551764705882363E-6,"lb/MW","Part II","Ash_Blr_2_Test_7o",15]
["Cope",7210,"COP1","COP001","Lead",2.3286049698252503E-7,"lb/MMBtu",2.1433198260811051E-6,"lb/MW","ERT","",16]
["Craig",6021,"C2","C2","Lead",2.3490934304688269E-7,"lb/MMBtu",2.1991841786560135E-6,"lb/MW","ERT","",17]
["Northampton Generating Company, L.P.",50888,"BLR1","GEN1","Lead",2.4466524071860208E-7,"lb/MMBtu",2.3172426930869253E-6,"lb/MW","ERT","",18]
["Northampton Generating Company, L.P.",50888,"BLR1","GEN1","Lead",1.0549809744514062E-6,"lb/MMBtu",9.9918032786885252E-6,"lb/MW","Part II","TDF 2009 Stack Test - #226-013",18]
["AES Shady Point,LLC",10671,"2a","Unit 2","Lead",1.7941858859895406E-7,"lb/MMBtu",2.4904085859112952E-6,"lb/MW","ERT","",19]
["AES Shady Point,LLC",10671,"2b","Unit 2","Lead",1.7941858859895406E-7,"lb/MMBtu",2.4904085859112952E-6,"lb/MW","ERT","",20]
["AES Shady Point,LLC",10671,"1b","Unit 1","Lead",1.7941858859895406E-7,"lb/MMBtu",2.4904085859112952E-6,"lb/MW","ERT","",21]
["AES Shady Point,LLC",10671,"1A","Unit 1","Lead",1.7941858859895406E-7,"lb/MMBtu",2.4904085859112952E-6,"lb/MW","ERT","",22]
["H L Spurlock Station",6041,"4","Unit 04","Lead",2.67E-7,"lb/MMBtu",2.492E-6,"lb/MW","Part II","Compliance_metals_05/27/09",23]
["H L Spurlock Station",6041,"4","Unit 04","Lead",3.3250851180878836E-6,"lb/MMBtu",3.1034127768820251E-5,"lb/MW","ERT","",23]
["AES Thames",10675,"B","B","Lead",2.7066666666666666E-7,"lb/MMBtu",2.6077692307692307E-6,"lb/MW","Part II","8",24]
["AES Hawaii",10673,"BLR A","001","Lead",2.5955489457731445E-7,"lb/MMBtu",2.6119149686824532E-6,"lb/MW","ERT","",25]
["Gerald Gentleman",6077,"2","U2","Lead",2.6401850360332862E-7,"lb/MMBtu",2.6535619735491881E-6,"lb/MW","ERT","",26]
["Elm Road Generating Station",56068,"1","ERGS-B1","Lead",2.7918708784059832E-7,"lb/MMBtu",2.6867117832813857E-6,"lb/MW","ERT","",27]
["Chambers Cogeneration LP",10566,"Boil 1","Boil 1","Lead",2.7616506516602757E-7,"lb/MMBtu",2.6880066342826681E-6,"lb/MW","ERT","",28]
["R D Green",6639,"G2","2","Lead",2.3580828240058494E-7,"lb/MMBtu",2.6901877104327819E-6,"lb/MW","ERT","",29]
["Crist",641,"5","Unit 5","Lead",2.71535326023767E-7,"lb/MMBtu",2.7081675083172846E-6,"lb/MW","ERT","",30]
["Crist",641,"6","Unit 6","Lead",2.71535326023767E-7,"lb/MMBtu",2.7097087196479506E-6,"lb/MW","ERT","",31]
["PSEG Mercer Generating Station",2408,"E2","MERU2E2PT2OS1-Coal","Lead",3.0276816984340694E-7,"lb/MMBtu",2.7363887070395378E-6,"lb/MW","ERT","",32]
["PSEG Mercer Generating Station",2408,"E2","MERU2E2PT2OS1-Coal","Lead",5.3333333333333334E-7,"lb/MMBtu",4.8202137998056365E-6,"lb/MW","Part II","MER2 2009 1YR ST Co NG",32]
["Springerville",8223,"4","4","Lead",2.9999999999999999E-7,"lb/MMBtu",2.7999999999999999E-6,"lb/MW","Part II","U4 INITIAL PERF 09DEC13 (HG, PB)",33]
["Springerville",8223,"4","4","Lead",3.530335021164723E-7,"lb/MMBtu",3.2949793530870752E-6,"lb/MW","ERT","",33]
["Crist",641,"7","Unit 7","Lead",2.71535326023767E-7,"lb/MMBtu",2.867300084115354E-6,"lb/MW","ERT","",34]
["Crist",641,"4","Unit 4","Lead",2.71535326023767E-7,"lb/MMBtu",2.8770889723553877E-6,"lb/MW","ERT","",35]
["Welsh",6139,"1","WE-1","Lead",3.1190487213511184E-7,"lb/MMBtu",2.8820457360728253E-6,"lb/MW","ERT","",36]
["Cedar Bay Generating Company L.P.",10672,"CBC","CBC1","Lead",2.5177456597964593E-7,"lb/MMBtu",2.9090909090909093E-6,"lb/MW","Part II","CBCmetals2009",37]
["Cedar Bay Generating Company L.P.",10672,"CBC","CBC1","Lead",9.3139145545448613E-7,"lb/MMBtu",1.0761620838566509E-5,"lb/MW","ERT","",37]
["Springerville",8223,"3","3","Lead",3.15E-7,"lb/MMBtu",2.9400000000000002E-6,"lb/MW","Part II","U3 INITIAL PERF TESTS (PB, HG)",38]
["Springerville",8223,"3","3","Lead",3.8553089423616618E-7,"lb/MMBtu",3.5982883462042177E-6,"lb/MW","ERT","",38]
["Duck Creek",6016,"1","001","Lead",2.7008263987241221E-7,"lb/MMBtu",3.0384296985646372E-6,"lb/MW","ERT","",39]
["Duck Creek",6016,"1","001","Lead",4.7999999999999996E-7,"lb/MMBtu",5.3999999999999991E-6,"lb/MW","Part II","3",39]
["A. B. Brown Generating Station",6137,"1","1Config","Lead",3.2146677858945694E-7,"lb/MMBtu",3.0545409376915189E-6,"lb/MW","ERT","",40]
["Sheldon Station",2277,"1","U1","Lead",2.9118697256899844E-7,"lb/MMBtu",3.1257101586703425E-6,"lb/MW","ERT","",41]
["Stanton Energy Center",564,"2","2 coal","Lead",3.473728771952254E-7,"lb/MMBtu",3.1812823753391796E-6,"lb/MW","ERT","",42]
["Dunkirk Generating Plant",2554,"4","4","Lead",3.3841174719417797E-7,"lb/MMBtu",3.1862767581974913E-6,"lb/MW","ERT","",43]
["Clover",7213,"2","Unit 2","Lead",2.8178300385823836E-7,"lb/MMBtu",3.2729680240769113E-6,"lb/MW","ERT","",44]
["TransAlta Centralia Generation",3845,"BD22","BW22CONFIG","Lead",2.4106180302456554E-7,"lb/MMBtu",3.2919603894518711E-6,"lb/MW","ERT","",45]
["Wygen 1",55479,"3","WYG1Cfg","Lead",2.9382638826382022E-7,"lb/MMBtu",3.3999910641956339E-6,"lb/MW","ERT","",46]
["Dunkirk Generating Plant",2554,"1","1","Lead",3.1348032871416365E-7,"lb/MMBtu",3.4010771663553145E-6,"lb/MW","ERT","",47]
["San Juan",2451,"Unit 3","Unit 3","Lead",3.2298957698761062E-7,"lb/MMBtu",3.4187021770122461E-6,"lb/MW","ERT","",48]
["Sheldon Station",2277,"2","U2","Lead",3.2129184854115127E-7,"lb/MMBtu",3.4498997070305178E-6,"lb/MW","ERT","",49]
["J K Spruce",7097,"BLR1","1","Lead",3.1760939576808828E-7,"lb/MMBtu",3.4832989077255338E-6,"lb/MW","ERT","",50]
["J K Spruce",7097,"BLR1","1","Lead",1.6433333333333334E-6,"lb/MMBtu",1.8022833333333333E-5,"lb/MW","Part II","JKS Unit 1 Test Report June 2009",50]
["AES Warrior Run Cogeneration Facility",10678,"BLR1","BLR1","Lead",3.4524017330105741E-7,"lb/MMBtu",3.4985476967686365E-6,"lb/MW","ERT","",51]
["Wygen 2",56319,"0001","WYG2Cfg","Lead",2.606800826080892E-7,"lb/MMBtu",3.5300427853178743E-6,"lb/MW","ERT","",52]
["Bridgeport Station",568,"BHB3","BHSEMU3OS2-Coal","Lead",3.4743131686577831E-7,"lb/MMBtu",3.5346610400736753E-6,"lb/MW","ERT","",53]
["James H. Miller Jr.",6002,"4","Unit 4","Lead",3.7468048203368662E-7,"lb/MMBtu",3.6154485376271346E-6,"lb/MW","ERT","",54]
["AES Thames",10675,"A","A","Lead",3.8033333333333334E-7,"lb/MMBtu",3.6643653846153849E-6,"lb/MW","Part II","7",55]
["Sunnyside Cogen Associates",50951,"1","Config 1","Lead",3.1720547808747169E-7,"lb/MMBtu",3.7007305776871697E-6,"lb/MW","ERT","",56]
["Gibson",6113,"1","1-2007-FGDIN","Lead",3.910454337951777E-7,"lb/MMBtu",3.767287931025252E-6,"lb/MW","ERT","",57]
["San Juan",2451,"Unit 2","Unit 2","Lead",3.7875687510764029E-7,"lb/MMBtu",3.7752847443161549E-6,"lb/MW","ERT","",58]
["Cedar Bay Generating Company L.P.",10672,"CBA","CBA1","Lead",3.2950576498679844E-7,"lb/MMBtu",3.8072242193583343E-6,"lb/MW","ERT","",59]
["Cedar Bay Generating Company L.P.",10672,"CBA","CBA1","Lead",4.2365912544651964E-7,"lb/MMBtu",4.8951048951048953E-6,"lb/MW","Part II","CBA2009metals",59]
["Cedar Bay Generating Company L.P.",10672,"CBB","CBB1","Lead",3.3319381718707608E-7,"lb/MMBtu",3.8498372572811073E-6,"lb/MW","ERT","",60]
["Cedar Bay Generating Company L.P.",10672,"CBB","CBB1","Lead",5.3484414472502038E-7,"lb/MMBtu",6.1797752808988771E-6,"lb/MW","Part II","CBB2009metals",60]
["Cross",130,"3","C3","Lead",3.9976105448399837E-7,"lb/MMBtu",3.8748039489024993E-6,"lb/MW","ERT","",61]
["Cross",130,"3","C3","Lead",2.2333333333333333E-6,"lb/MMBtu",2.1647253333333333E-5,"lb/MW","Part II","C3TVM292007",61]
["Neil Simpson II",7504,"2","NS2Cfg","Lead",3.2935247281157227E-7,"lb/MMBtu",4.1169059101446537E-6,"lb/MW","ERT","",62]
["Clover",7213,"1","Unit 1","Lead",3.6458288517820677E-7,"lb/MMBtu",4.1643655307014199E-6,"lb/MW","ERT","",63]
["G G Allen",2718,"ES-3","3-2009","Lead",5.2982899323629236E-7,"lb/MMBtu",4.193460024619749E-6,"lb/MW","ERT","",64]
["G G Allen",2718,"ES-4","4-2009","Lead",5.2982899323629236E-7,"lb/MMBtu",4.2414833632774159E-6,"lb/MW","ERT","",65]
["Pulliam",4072,"8","8","Lead",3.9746681774666671E-7,"lb/MMBtu",4.3522472429112885E-6,"lb/MW","ERT","",66]
["J T Deely",6181,"1","1","Lead",4.6152500892852914E-7,"lb/MMBtu",4.3598729176781721E-6,"lb/MW","ERT","",67]
["J T Deely",6181,"2","2","Lead",4.6152500892852914E-7,"lb/MMBtu",4.3598729176781721E-6,"lb/MW","ERT","",68]
["TS Power Plant",56224,"BLR100","TSPower","Lead",5.0883333333333341E-7,"lb/MMBtu",4.440727272727273E-6,"lb/MW","Part II","Optimal 07/2009",69]
["TS Power Plant",56224,"BLR100","TSPower","Lead",7.5800000000000009E-7,"lb/MMBtu",6.6152727272727275E-6,"lb/MW","Part II","TRC 04/2008",69]
["TS Power Plant",56224,"BLR100","TSPower","Lead",8.426895592156651E-7,"lb/MMBtu",7.354381607700349E-6,"lb/MW","ERT","",69]
["Roxboro Steam Electric Plant",2712,"1","Rox_Cfg_1b","Lead",4.5783404722611437E-7,"lb/MMBtu",4.4653684346339204E-6,"lb/MW","ERT","",70]
["Roxboro Steam Electric Plant",2712,"1","Rox_Cfg_1b","Lead",9.8733333333333325E-7,"lb/MMBtu",9.6297056277056264E-6,"lb/MW","Part II","Rox_Blr_1_Test_8e",70]
["Roxboro Steam Electric Plant",2712,"1","Rox_Cfg_1b","Lead",6.3700000000000003E-5,"lb/MMBtu",6.212818181818182E-4,"lb/MW","Part II","Rox_Blr_1_Test_7e",70]
["INDIANTOWN COGENERATION L.P.",50976,"AABO1","001","Lead",4.8999999999999997E-7,"lb/MMBtu",4.6448199445983376E-6,"lb/MW","Part II","10669-3",71]
["INDIANTOWN COGENERATION L.P.",50976,"AABO1","001","Lead",3.5016904839537267E-6,"lb/MMBtu",3.3193309795262196E-5,"lb/MW","ERT","",71]
["RS Nelson",1393,"6","001","Lead",4.7786886608675327E-7,"lb/MMBtu",4.7465560991823896E-6,"lb/MW","ERT","",72]
["PPL Montour",3149,"2","U2","Lead",5.2017395077343294E-7,"lb/MMBtu",4.7544687243041429E-6,"lb/MW","ERT","",73]
["Sioux",2107,"2","002","Lead",5.1346293082042905E-7,"lb/MMBtu",4.8210641596116624E-6,"lb/MW","ERT","",74]
["Hatfield's Ferry Power Station",3179,"1","001","Lead",5.110430920239814E-7,"lb/MMBtu",4.9371959737910064E-6,"lb/MW","ERT","",75]
["Hatfield's Ferry Power Station",3179,"1","001","Lead",7.5999999999999992E-6,"lb/MMBtu",7.3423728813559313E-5,"lb/MW","Part II","Pb-11/09-1",75]
["Roxboro Steam Electric Plant",2712,"2","Rox_Cfg_2c","Lead",5.1169052635056232E-7,"lb/MMBtu",5.0171874795653293E-6,"lb/MW","ERT","",76]
["Roxboro Steam Electric Plant",2712,"2","Rox_Cfg_2c","Lead",5.4013333333333322E-7,"lb/MMBtu",5.2960726410621139E-6,"lb/MW","Part II","Rox_Blr_2_Test_8j",76]
["Roxboro Steam Electric Plant",2712,"2","Rox_Cfg_2c","Lead",1.0705E-6,"lb/MMBtu",1.0496381934566145E-5,"lb/MW","Part II","Rox_Blr_2_Test_10e",76]
["Roxboro Steam Electric Plant",2712,"2","Rox_Cfg_2c","Lead",2.3176666666666669E-6,"lb/MMBtu",2.2725001896633478E-5,"lb/MW","Part II","Rox_Blr_2_Test_9e",76]
["Gerald Gentleman",6077,"1","U1","Lead",4.7642562041801132E-7,"lb/MMBtu",5.0227920653300268E-6,"lb/MW","ERT","",77]
["Eastlake",2837,"3","Unit 3","Lead",6.390090307304471E-7,"lb/MMBtu",5.3472630696540884E-6,"lb/MW","ERT","",78]
["PPL Brunner Island",3140,"2","U2","Lead",5.5679645878876309E-7,"lb/MMBtu",5.3696147043496486E-6,"lb/MW","ERT","",79]
["Gibson",6113,"2","2-2007-FGDIN","Lead",5.6046079785526405E-7,"lb/MMBtu",5.4638568553393665E-6,"lb/MW","ERT","",80]
["PPL Brunner Island",3140,"1","U1","Lead",5.5679645878876309E-7,"lb/MMBtu",5.6438913777224622E-6,"lb/MW","ERT","",81]
["Cardinal",2828,"3","CD-U3","Lead",7.0213283868205319E-7,"lb/MMBtu",5.6980780369966622E-6,"lb/MW","ERT","",82]
["Newton",6017,"2","002","Lead",6.6673333457550882E-7,"lb/MMBtu",5.9145699034924174E-6,"lb/MW","ERT","",83]
["Salem Harbor",1626,"1","Unit 1","Lead",4.9694445248584524E-7,"lb/MMBtu",5.987576706771321E-6,"lb/MW","ERT","",84]
["Birchwood Power Facility",54304,"1A","1A","Lead",5.7815601570398997E-7,"lb/MMBtu",5.9899046672034998E-6,"lb/MW","ERT","",85]
["Gallatin",3403,"2","2","Lead",6.5946967917925029E-7,"lb/MMBtu",6.0451387258097937E-6,"lb/MW","ERT","",86]
["Marshall",2727,"Unit 4","U4","Lead",7.0460568059735639E-7,"lb/MMBtu",6.0694733326656285E-6,"lb/MW","Part II","U4032707",87]
["San Juan",2451,"Unit 4","Unit 4","Lead",5.8652114558428191E-7,"lb/MMBtu",6.0905477047897216E-6,"lb/MW","ERT","",88]
["Weston",4078,"3","W3","Lead",6.5151817328818633E-7,"lb/MMBtu",6.10081902595361E-6,"lb/MW","ERT","",89]
["PPL Montour",3149,"1","U1","Lead",6.7769292161147249E-7,"lb/MMBtu",6.1553564109729601E-6,"lb/MW","ERT","",90]
["Mayo Electric Generating Facility",6250,"1A","May_Cfg_1b","Lead",6.7800000000000001E-7,"lb/MMBtu",6.4084696969696976E-6,"lb/MW","Part II","May_Unit_1_Test_6e",91]
["Mayo Electric Generating Facility",6250,"1B","May_Cfg_1b","Lead",6.7800000000000001E-7,"lb/MMBtu",6.4084696969696976E-6,"lb/MW","Part II","May_Unit_1_Test_6e",92]
["Hammond",708,"2","Unit 2","Lead",6.4907153890291578E-7,"lb/MMBtu",6.4231667961805476E-6,"lb/MW","ERT","",93]
["Hammond",708,"3","Unit 3","Lead",6.4907153890291578E-7,"lb/MMBtu",6.4421309733171894E-6,"lb/MW","ERT","",94]
["Comanche",470,"2","Unit 2","Lead",6.8082890473674601E-7,"lb/MMBtu",6.4949212227215056E-6,"lb/MW","ERT","",95]
["Hammond",708,"1","Unit 1","Lead",6.4907153890291578E-7,"lb/MMBtu",6.5401125551898389E-6,"lb/MW","ERT","",96]
["AES Puerto Rico Cogeneration Facility",68029,"BLR1","Unit_1","Lead",6.7875889639059044E-7,"lb/MMBtu",6.5517535199050955E-6,"lb/MW","ERT","",97]
["Hammond",708,"4","Unit 4","Lead",6.4907153890291578E-7,"lb/MMBtu",6.8134162831687168E-6,"lb/MW","ERT","",98]
["Cambria Cogen",10641,"B1","001","Lead",6.0584906053239808E-7,"lb/MMBtu",6.923989263227407E-6,"lb/MW","ERT","",99]
["Spruance Genco, LLC",54081,"2A","GEN2","Lead",5.3829110552992893E-7,"lb/MMBtu",7.0334203684224158E-6,"lb/MW","ERT","",100]
["Spruance Genco, LLC",54081,"2B","GEN2","Lead",5.3829110552992893E-7,"lb/MMBtu",7.0334203684224158E-6,"lb/MW","ERT","",101]
["Herbert A. Wagner",1554,"2","002","Lead",7.3207396406551275E-7,"lb/MMBtu",7.5125935070998823E-6,"lb/MW","ERT","",102]
["Silver Bay Power",10849,"BLR1","GEN1","Lead",9.2109919298513827E-7,"lb/MMBtu",7.6126161122280024E-6,"lb/MW","ERT","",103]
["Iatan",6065,"1","1","Lead",7.1999999999999999E-7,"lb/MMBtu",7.7355371900826453E-6,"lb/MW","Part II","LeadTestOct2009",104]
["Piney Creek Project",54144,"BRBR1","BRBRI","Lead",6.2054054054054056E-7,"lb/MMBtu",7.7567567567567564E-6,"lb/MW","Part II","16-00127 Condition 4 & 12",105]
["Piney Creek Project",54144,"BRBR1","BRBRI","Lead",1.4284361374527188E-6,"lb/MMBtu",1.7855451718158986E-5,"lb/MW","ERT","",105]
["Whelan Energy Center Unit 1 (WEC1)",60,"1","1","Lead",7.7806250610520388E-7,"lb/MMBtu",7.8653184678170794E-6,"lb/MW","ERT","",106]
["Craig",6021,"C1","C1","Lead",9.2527968033395115E-7,"lb/MMBtu",8.1733038429499029E-6,"lb/MW","ERT","",107]
["McMeekin",3287,"MCM2","MCM002","Lead",1.019174697928726E-6,"lb/MMBtu",8.5031598093098942E-6,"lb/MW","ERT","",108]
["Cross",130,"4","C4","Lead",7.8335387757409349E-7,"lb/MMBtu",8.5203834555978998E-6,"lb/MW","ERT","",109]
["Cross",130,"4","C4","Lead",2.0666666666666666E-6,"lb/MMBtu",2.2478719999999997E-5,"lb/MW","Part II","C4TVICrpt2009",109]
["Cross",130,"4","C4","Lead",4.4633333333333332E-5,"lb/MMBtu",4.8546783999999996E-4,"lb/MW","Part II","C4TVIC2008",109]
["Roxboro Steam Electric Plant",2712,"3A","Rox_Cfg_3b","Lead",9.3899999999999992E-7,"lb/MMBtu",8.7690688259109301E-6,"lb/MW","Part II","Rox_Unit_3_Test_7m",110]
["Roxboro Steam Electric Plant",2712,"3B","Rox_Cfg_3b","Lead",9.3899999999999992E-7,"lb/MMBtu",8.7690688259109301E-6,"lb/MW","Part II","Rox_Unit_3_Test_7m",111]
["Roxboro Steam Electric Plant",2712,"4B","Rox_Cfg_4c","Lead",9.5933333333333348E-7,"lb/MMBtu",8.9340331096196885E-6,"lb/MW","Part II","Rox_Unit_4_Test_12e",112]
["Roxboro Steam Electric Plant",2712,"4A","Rox_Cfg_4c","Lead",9.5933333333333348E-7,"lb/MMBtu",8.9340331096196885E-6,"lb/MW","Part II","Rox_Unit_4_Test_12e",113]
["Southampton Power Station",10774,"2","Unit 1 & 2","Lead",6.9036769385771128E-7,"lb/MMBtu",9.0255423505809603E-6,"lb/MW","ERT","",114]
["Southampton Power Station",10774,"1","Unit 1 & 2","Lead",6.9036769385771128E-7,"lb/MMBtu",9.0255423505809603E-6,"lb/MW","ERT","",115]
["Hayden",525,"1","Unit 1","Lead",9.5925031741717829E-7,"lb/MMBtu",9.3218236291580253E-6,"lb/MW","ERT","",116]
["W H Zimmer",6019,"1","1","Lead",1.047136355655361E-6,"lb/MMBtu",9.4123279241294374E-6,"lb/MW","ERT","",117]
["East Bend Station",6018,"2","2","Lead",9.8002396679652739E-7,"lb/MMBtu",9.5076948742161902E-6,"lb/MW","ERT","",118]
["Cholla",113,"3","003","Lead",1.0103634506813589E-6,"lb/MMBtu",9.7028017935924586E-6,"lb/MW","ERT","",119]
["Eastlake",2837,"1","Unit 1","Lead",1.1756126235598438E-6,"lb/MMBtu",9.8375917457611926E-6,"lb/MW","ERT","",120]
["Nebraska City",6096,"NC2","NC2","Lead",9.7180856152046086E-7,"lb/MMBtu",9.8609414737481172E-6,"lb/MW","ERT","",121]
["Elmer Smith Station",1374,"1374-2","Unit001","Lead",1.1955054238653571E-6,"lb/MMBtu",9.9163745732093853E-6,"lb/MW","ERT","",122]
["Elmer Smith Station",1374,"1374","Unit001","Lead",1.1955054238653571E-6,"lb/MMBtu",9.9163745732093853E-6,"lb/MW","ERT","",123]
["Hayden",525,"2","Unit 2","Lead",1.0650137604971454E-6,"lb/MMBtu",1.0134446731467572E-5,"lb/MW","ERT","",124]
["AES Puerto Rico Cogeneration Facility",68029,"BLR2","Unit_2","Lead",1.0570025819818536E-6,"lb/MMBtu",1.02027692364319E-5,"lb/MW","ERT","",125]
["Spruance Genco, LLC",54081,"1A","GEN1","Lead",7.8881170481050949E-7,"lb/MMBtu",1.0306773146478782E-5,"lb/MW","ERT","",126]
["Spruance Genco, LLC",54081,"1B","GEN1","Lead",7.8881170481050949E-7,"lb/MMBtu",1.0306773146478782E-5,"lb/MW","ERT","",127]
["San Juan",2451,"Unit 1","Unit 1","Lead",1.050454516286137E-6,"lb/MMBtu",1.0524418626682999E-5,"lb/MW","ERT","",128]
["Muscatine #1",1167,"8","8","Lead",9.6745845370690893E-7,"lb/MMBtu",1.0616244098677147E-5,"lb/MW","ERT","",129]
["Cambria Cogen",10641,"B2","002","Lead",9.4512168009160147E-7,"lb/MMBtu",1.0801390629618303E-5,"lb/MW","ERT","",130]
["New Castle Plant",3138,"3","NC3-2","Lead",1.05275E-6,"lb/MMBtu",1.1010905612244898E-5,"lb/MW","Part II","NC-50",131]
["Lansing",1047,"4","Unit 4","Lead",1.11E-6,"lb/MMBtu",1.1032778198334594E-5,"lb/MW","Part II","LANS4-Metals-20060502",132]
["Martin Drake",492,"5","Unit 5 - Coal","Lead",1.0689663026403658E-6,"lb/MMBtu",1.1078378045545609E-5,"lb/MW","ERT","",133]
["McMeekin",3287,"MCM1","MCM001","Lead",1.3180789707597687E-6,"lb/MMBtu",1.1164617059731818E-5,"lb/MW","ERT","",134]
["Roanoke Valley II",54755,"BLR2","Boiler 2","Lead",1.0049072339287526E-6,"lb/MMBtu",1.1254961020002027E-5,"lb/MW","ERT","",135]
["Hardin Generator Project",55749,"PC1","PC1","Lead",1.0483657962510146E-6,"lb/MMBtu",1.1487974775725404E-5,"lb/MW","ERT","",136]
["W.H. Weatherspoon Plant",2716,"1","Wea_Cfg_1","Lead",1.309452517917355E-6,"lb/MMBtu",1.1661539404848898E-5,"lb/MW","ERT","",137]
["W.H. Weatherspoon Plant",2716,"2","Wea_Cfg_1","Lead",1.309452517917355E-6,"lb/MMBtu",1.1661539404848898E-5,"lb/MW","ERT","",138]
["Cross",130,"1","C1","Lead",1.1159465294259819E-6,"lb/MMBtu",1.1894892351356942E-5,"lb/MW","ERT","",139]
["Tanners Creek",988,"4","TC-4","Lead",1.4722685497631998E-6,"lb/MMBtu",1.2673141389198493E-5,"lb/MW","ERT","",140]
["Clinch River",3775,"1","CR-1","Lead",1.4002783098567695E-6,"lb/MMBtu",1.2790629135556902E-5,"lb/MW","ERT","",141]
["Scrubgrass Generating Company L.P.",50974,"#2 CFB Boiler","Gen 1","Lead",9.9999999999999995E-7,"lb/MMBtu",1.2886597938144331E-5,"lb/MW","Part II","12/13/2005 Waste Bituminous Coal Baseline Testing",142]
["Scrubgrass Generating Company L.P.",50974,"#2 CFB Boiler","Gen 1","Lead",3.0000000000000001E-6,"lb/MMBtu",3.8659793814432993E-5,"lb/MW","Part II","common stack test 3-2-2005",142]
["Scrubgrass Generating Company L.P.",50974,"#2 CFB Boiler","Gen 1","Lead",6.4562840428628393E-6,"lb/MMBtu",8.3199536634830405E-5,"lb/MW","ERT","",142]
["Scrubgrass Generating Company L.P.",50974,"#1 CFB boiler","Gen 1","Lead",9.9999999999999995E-7,"lb/MMBtu",1.2886597938144331E-5,"lb/MW","Part II","12/13/2005 Waste Bituminous Coal Baseline Testing",143]
["Scrubgrass Generating Company L.P.",50974,"#1 CFB boiler","Gen 1","Lead",3.0000000000000001E-6,"lb/MMBtu",3.8659793814432993E-5,"lb/MW","Part II","common stack test 3-2-2005",143]
["Scrubgrass Generating Company L.P.",50974,"#1 CFB boiler","Gen 1","Lead",6.4562840428628393E-6,"lb/MMBtu",8.3199536634830405E-5,"lb/MW","ERT","",143]
["Gibson",6113,"4","4","Lead",1.3776140099482376E-6,"lb/MMBtu",1.3057113120008636E-5,"lb/MW","Part II","U4010506",144]
["R. Gallagher",1008,"2","2-2007","Lead",1.3927829050448491E-6,"lb/MMBtu",1.3556420275769863E-5,"lb/MW","Part II","U2091409-BASE",145]
["Conemaugh",3118,"2","CON-2","Lead",1.4863333333333333E-6,"lb/MMBtu",1.4267847222222222E-5,"lb/MW","Part II","C-193",146]
["Nucla",527,"1","001","Lead",1.5908094863380294E-6,"lb/MMBtu",1.4924685362734965E-5,"lb/MW","ERT","",147]
["BL England",2378,"2","2 Coal w or w/o TDF","Lead",1.583297376866492E-6,"lb/MMBtu",1.514211478174768E-5,"lb/MW","Part II","CAM 238-012",148]
["BL England",2378,"2","2 Coal w or w/o TDF","Lead",1.6159659090909093E-5,"lb/MMBtu",1.5454545454545454E-4,"lb/MW","Part II","CAM 238-026",148]
["State Line",981,"3","Unit 3","Lead",1.4338753820887386E-6,"lb/MMBtu",1.5799182450792581E-5,"lb/MW","ERT","",149]
["Spruance Genco, LLC",54081,"4B","GEN4","Lead",1.2123341791702846E-6,"lb/MMBtu",1.5840603386371314E-5,"lb/MW","ERT","",150]
["Spruance Genco, LLC",54081,"4B","GEN4","Lead",2.4519555386500998E-6,"lb/MMBtu",3.2037746585149387E-5,"lb/MW","Part II","2006 Emissions Testing  at Boilers 4A and 4B",150]
["Spruance Genco, LLC",54081,"4A","GEN4","Lead",1.2123341791702846E-6,"lb/MMBtu",1.5840603386371314E-5,"lb/MW","ERT","",151]
["Spruance Genco, LLC",54081,"4A","GEN4","Lead",2.4519555386500998E-6,"lb/MMBtu",3.2037746585149387E-5,"lb/MW","Part II","2006 Emissions Testing  at Boilers 4A and 4B",151]
["Consumers Energy - J.H. Campbell",1710,"Unit 2","JHC2-Conf","Lead",1.8067271635940434E-6,"lb/MMBtu",1.6386145825965231E-5,"lb/MW","ERT","",152]
["Consumers Energy - J.H. Campbell",1710,"Unit 1","JHC1-Conf","Lead",1.8067271635940434E-6,"lb/MMBtu",1.6886964474322429E-5,"lb/MW","ERT","",153]
["New Castle Plant",3138,"5","NC5-2","Lead",1.7600000000000001E-6,"lb/MMBtu",1.7698255408234471E-5,"lb/MW","Part II","NC-48",154]
["Scholz",642,"1","Unit 1","Lead",1.5356232218508671E-6,"lb/MMBtu",1.8210955787929434E-5,"lb/MW","ERT","",155]
["Joppa Steam",887,"1","1","Lead",1.8555982397516794E-6,"lb/MMBtu",1.822191397464824E-5,"lb/MW","ERT","",156]
["Valley",4042,"3","VAPP-B3","Lead",1.6038555418423378E-6,"lb/MMBtu",1.933536958776596E-5,"lb/MW","ERT","",157]
["Scholz",642,"2","Unit 2","Lead",1.5356232218508671E-6,"lb/MMBtu",2.0205730353113708E-5,"lb/MW","ERT","",158]
["Taconite Harbor Energy Center",10075,"2","THEC2","Lead",1.7912658325922976E-6,"lb/MMBtu",2.0649314459050096E-5,"lb/MW","ERT","",159]
["Sibley",2094,"3","3","Lead",2.1273413422549101E-6,"lb/MMBtu",2.078651119170842E-5,"lb/MW","ERT","",160]
["Canadys Steam",3280,"CAN3","CAN003","Lead",2.1182549662128098E-6,"lb/MMBtu",2.0890573977596062E-5,"lb/MW","ERT","",161]
["Taconite Harbor Energy Center",10075,"1","THEC1","Lead",2.0593890833251133E-6,"lb/MMBtu",2.1015693416582784E-5,"lb/MW","ERT","",162]
["South Oak Creek",4041,"7","OCPP-B7","Lead",2.4226607006905536E-6,"lb/MMBtu",2.1622246753663195E-5,"lb/MW","ERT","",163]
["Will County",884,"4","WC4CONFIG","Lead",2.25319708890173E-6,"lb/MMBtu",2.1844080626470127E-5,"lb/MW","ERT","",164]
["Louisa",6664,"101","101","Lead",2.0583016067842347E-6,"lb/MMBtu",2.2050674604853716E-5,"lb/MW","ERT","",165]
["Louisa",6664,"101","101","Lead",1.06E-5,"lb/MMBtu",1.1355826086956522E-4,"lb/MW","Part II","1/19/2010-Lead",165]
["Colbert",47,"4","4","Lead",2.1675268213358195E-6,"lb/MMBtu",2.2986621940266367E-5,"lb/MW","ERT","",166]
["Sibley",2094,"1","1","Lead",2.1273413422549101E-6,"lb/MMBtu",2.3578677858883513E-5,"lb/MW","ERT","",167]
["Hawthorn",2079,"5A","5A","Lead",2.1790715658586759E-6,"lb/MMBtu",2.4211906287318621E-5,"lb/MW","ERT","",168]
["Albright Power Station",3942,"2","Unit_2","Lead",3.0663068802690411E-6,"lb/MMBtu",2.4341176839666584E-5,"lb/MW","ERT","",169]
["Spruance Genco, LLC",54081,"3B","GEN3","Lead",1.9920333437026558E-6,"lb/MMBtu",2.6028310240017279E-5,"lb/MW","ERT","",170]
["Spruance Genco, LLC",54081,"3A","GEN3","Lead",1.9920333437026558E-6,"lb/MMBtu",2.6028310240017279E-5,"lb/MW","ERT","",171]
["Sibley",2094,"2","2","Lead",2.1273413422549101E-6,"lb/MMBtu",2.6166298509735393E-5,"lb/MW","ERT","",172]
["Colbert",47,"3","3","Lead",2.4785016287040809E-6,"lb/MMBtu",2.628450977240678E-5,"lb/MW","ERT","",173]
["Conemaugh",3118,"1","CON-1","Lead",2.8066666666666663E-6,"lb/MMBtu",2.6942200854700853E-5,"lb/MW","Part II","C-190",174]
["Shawville",3131,"4","SHAW4-2","Lead",2.8700000000000001E-6,"lb/MMBtu",2.7387127659574467E-5,"lb/MW","Part II","SH-184 U3-4",175]
["Shawville",3131,"4","SHAW4-2","Lead",5.8664903656051964E-5,"lb/MMBtu",5.598129636114746E-4,"lb/MW","ERT","",175]
["Shawville",3131,"3","SHAW3-2","Lead",2.8700000000000001E-6,"lb/MMBtu",2.7387127659574467E-5,"lb/MW","Part II","SH-184 U3-4",176]
["Shawville",3131,"3","SHAW3-2","Lead",5.8664903656051964E-5,"lb/MMBtu",5.598129636114746E-4,"lb/MW","ERT","",176]
["Eddystone Generating Station",3161,"2","Unit 2","Lead",3.3133333333333331E-6,"lb/MMBtu",2.7444955752212389E-5,"lb/MW","Part II","Particulate Emissions Test - Unit 2",177]
["Eddystone Generating Station",3161,"2","Unit 2","Lead",3.6615082462631156E-6,"lb/MMBtu",3.0328953261082092E-5,"lb/MW","ERT","",177]
["Grant Town Power Plant",10151,"BLR1A","GEN1","Lead",2.062359144540091E-6,"lb/MMBtu",2.9307208896096031E-5,"lb/MW","ERT","",178]
["Grant Town Power Plant",10151,"BLR1B","GEN1","Lead",2.062359144540091E-6,"lb/MMBtu",2.9307208896096031E-5,"lb/MW","ERT","",179]
["Hennepin Power Station",892,"Unit 1","001","Lead",2.8624993210329861E-6,"lb/MMBtu",2.9617326308287961E-5,"lb/MW","ERT","",180]
["PANTHER CREEK ENERGY FACILITY",50776,"BLR2","BG2","Lead",2.3007973966742339E-6,"lb/MMBtu",2.9687708344183661E-5,"lb/MW","ERT","",181]
["PANTHER CREEK ENERGY FACILITY",50776,"BLR1","BG1","Lead",2.3007973966742339E-6,"lb/MMBtu",2.9687708344183661E-5,"lb/MW","ERT","",182]
["Martin Drake",492,"7","Unit 7 - Coal","Lead",2.8679845098899186E-6,"lb/MMBtu",3.0001965617642767E-5,"lb/MW","ERT","",183]
["PSEG Hudson Generating Station",2403,"U2","HUDU2E2PT2OS1-Coal","Lead",3.0333333333333337E-6,"lb/MMBtu",3.0347127482188877E-5,"lb/MW","Part II","EG08009",184]
["PSEG Hudson Generating Station",2403,"U2","HUDU2E2PT2OS1-Coal","Lead",4.3666666666666666E-6,"lb/MMBtu",4.3686524177656509E-5,"lb/MW","Part II","HUD2 2009 5YR ST CoNg",184]
["PSEG Hudson Generating Station",2403,"U2","HUDU2E2PT2OS1-Coal","Lead",4.555304706055685E-6,"lb/MMBtu",4.5573762407105532E-5,"lb/MW","Part II","EG07044",184]
["PSEG Hudson Generating Station",2403,"U2","HUDU2E2PT2OS1-Coal","Lead",5.4601356601092637E-6,"lb/MMBtu",5.4626186685949884E-5,"lb/MW","Part II","EG06031A",184]
["Hennepin Power Station",892,"Unit 2","002","Lead",2.8624993210329861E-6,"lb/MMBtu",3.0582257703343866E-5,"lb/MW","ERT","",185]
["Sunbury Generation LP",3152,"4","Boiler 4","Lead",2.9645248059149453E-6,"lb/MMBtu",3.1498076062846298E-5,"lb/MW","ERT","",186]
["Meredosia",864,"5","005","Lead",2.3292066533144144E-6,"lb/MMBtu",3.1786820209937888E-5,"lb/MW","ERT","",187]
["Ebensburg Power Company",10603,"031","EPC01","Lead",2.2699999999999999E-6,"lb/MMBtu",3.2484482758620686E-5,"lb/MW","Part II","2005 Emissions",188]
["Ebensburg Power Company",10603,"031","EPC01","Lead",7.259847987365687E-6,"lb/MMBtu",1.0389092809506069E-4,"lb/MW","ERT","",188]
["Mecklenburg Power Station",52007,"BLR1","Unit 1 & 2","Lead",2.8561467909399166E-6,"lb/MMBtu",3.4461665885419782E-5,"lb/MW","ERT","",189]
["Mecklenburg Power Station",52007,"BLR2","Unit 1 & 2","Lead",2.8561467909399166E-6,"lb/MMBtu",3.4461665885419782E-5,"lb/MW","ERT","",190]
["H L Spurlock Station",6041,"1","Unit 01","Lead",3.3462022493329321E-6,"lb/MMBtu",3.5417216249480254E-5,"lb/MW","ERT","",191]
["George Neal South",7343,"4","4","Lead",3.63E-6,"lb/MMBtu",3.6725806451612905E-5,"lb/MW","Part II","Lead-Jan 2010",192]
["Big Stone",6098,"001","001","Lead",3.4554553423216483E-6,"lb/MMBtu",3.7060631136132588E-5,"lb/MW","ERT","",193]
["Hopewell",10771,"10771-01","1 & 2","Lead",2.9669976307573095E-6,"lb/MMBtu",3.7305631974963229E-5,"lb/MW","ERT","",194]
["Hopewell",10771,"10771-02","1 & 2","Lead",2.9669976307573095E-6,"lb/MMBtu",3.7305631974963229E-5,"lb/MW","ERT","",195]
["Morgantown Energy Facility",10743,"CFB1","Unit 1&2","Lead",2.3840985353435697E-6,"lb/MMBtu",3.7405683916597392E-5,"lb/MW","ERT","",196]
["Morgantown Energy Facility",10743,"CFB2","Unit 1&2","Lead",2.3840985353435697E-6,"lb/MMBtu",3.7405683916597392E-5,"lb/MW","ERT","",197]
["Columbia",8023,"1","Unit 1","Lead",3.63E-6,"lb/MMBtu",3.7449940708114521E-5,"lb/MW","Part II","COL-1-Stack-Metals-20050810",198]
["Vermilion",897,"Unit 2","002","Lead",3.8822407629961354E-6,"lb/MMBtu",3.7975373281671288E-5,"lb/MW","ERT","",199]
["Shawville",3131,"2","SHAW2-2","Lead",3.6299999999999995E-6,"lb/MMBtu",3.9174959999999994E-5,"lb/MW","Part II","SH-184-U2",200]
["Burlington",1104,"1","Unit 1","Lead",3.7799999999999998E-6,"lb/MMBtu",3.9721913027072913E-5,"lb/MW","Part II","BGS1-Metals-Stack-2006517",201]
["HB Robinson / Darlington Electric Power Plant",3251,"1","Rob_Cfg_1","Lead",4.3432084446855689E-6,"lb/MMBtu",4.0250161682567334E-5,"lb/MW","ERT","",202]
["Waukegan",883,"8","WK8CONFIG","Lead",4.0178028391780748E-6,"lb/MMBtu",4.155113087017682E-5,"lb/MW","ERT","",203]
["La Cygne",1241,"2","2","Lead",3.7716108820817475E-6,"lb/MMBtu",4.2396209915371468E-5,"lb/MW","ERT","",204]
["Ottumwa",6254,"1","Unit 1","Lead",4.2200000000000003E-6,"lb/MMBtu",4.4069794798065613E-5,"lb/MW","Part II","OGS1-Metals-20060615",205]
["Vermilion",897,"Unit 1","001","Lead",3.8822407629961354E-6,"lb/MMBtu",4.4807528806247061E-5,"lb/MW","ERT","",206]
["Colstrip",6076,"3","Unit3","Lead",4.7693884159197935E-6,"lb/MMBtu",4.4867799346286451E-5,"lb/MW","ERT","",207]
["Roanoke Valley I",54035,"BLR1","Boiler 1","Lead",4.8313112516349732E-6,"lb/MMBtu",4.5127632570216785E-5,"lb/MW","ERT","",208]
["Quindaro",1295,"2","Unit 2","Lead",3.9253782581095174E-6,"lb/MMBtu",4.5675937327250978E-5,"lb/MW","ERT","",209]
["Cape Fear Steam Electric Plant",2708,"5","Cap_Cfg_5b","Lead",5.8286094317893928E-6,"lb/MMBtu",4.7314594210996246E-5,"lb/MW","ERT","",210]
["Hoot Lake",1943,"002","2","Lead",4.1259433369263917E-6,"lb/MMBtu",5.0789206941538718E-5,"lb/MW","ERT","",211]
["Lawrence Energy Center",1250,"3","3","Lead",4.5987053383581816E-6,"lb/MMBtu",5.1140774883465988E-5,"lb/MW","ERT","",212]
["Valley",4042,"1","VAPP-B1","Lead",4.4693143810003982E-6,"lb/MMBtu",5.3880067815393687E-5,"lb/MW","ERT","",213]
["Marion Generating Station",976,"123","123","Lead",5.3423748489929336E-6,"lb/MMBtu",5.5649738010343052E-5,"lb/MW","ERT","",214]
["ML Kapp",1048,"2","Unit 2","Lead",5.6799999999999998E-6,"lb/MMBtu",5.7841746724890821E-5,"lb/MW","Part II","KAPP2-Metals-20060608",215]
["Harding Street",990,"60","60s","Lead",6.9040925332370265E-6,"lb/MMBtu",6.2691625949125499E-5,"lb/MW","ERT","",216]
["Cane Run",1363,"4","CR4","Lead",4.7725956106824678E-6,"lb/MMBtu",6.5623189646883936E-5,"lb/MW","ERT","",217]
["Joliet 9",874,"5","JOL5 CONFIG","Lead",6.3055967418929415E-6,"lb/MMBtu",6.9098083060153436E-5,"lb/MW","ERT","",218]
["Merrimack Station",2364,"2","mk2","Lead",7.7833454714828164E-6,"lb/MMBtu",6.9680573553304619E-5,"lb/MW","ERT","",219]
["Eagle Valley",991,"6","6","Lead",7.2803140045094539E-6,"lb/MMBtu",7.0515041357962992E-5,"lb/MW","ERT","",220]
["Shawville",3131,"1","SHAW1-2","Lead",6.6000000000000003E-6,"lb/MMBtu",7.1227200000000001E-5,"lb/MW","Part II","SH-184-U1",221]
["Seward",3130,"1","SEW-1","Lead",6.9533030922302547E-6,"lb/MMBtu",7.3693126789448854E-5,"lb/MW","ERT","",222]
["Seward",3130,"2","SEW-1","Lead",6.9533030922302547E-6,"lb/MMBtu",7.3693126789448854E-5,"lb/MW","ERT","",223]
["George Neal North",1091,"2","2","Lead",7.8820000000000001E-6,"lb/MMBtu",7.4721360000000003E-5,"lb/MW","Part II","12/15/2008-Pb",224]
["Richard Gorsuch",7253,"3","UNIT3","Lead",7.2109415365698141E-6,"lb/MMBtu",7.4815209563285312E-5,"lb/MW","ERT","",225]
["Harding Street",990,"70","70ss","Lead",8.5785717832559354E-6,"lb/MMBtu",7.6391903806402204E-5,"lb/MW","ERT","",226]
["Wabash River",1010,"6","6","Lead",9.3567572274526789E-6,"lb/MMBtu",8.3692650416929853E-5,"lb/MW","ERT","",227]
["Crystal River Power Plant",628,"1","CryR_Cfg_1","Lead",9.6333375001473353E-6,"lb/MMBtu",9.2407789970163311E-5,"lb/MW","ERT","",228]
["Michigan City",997,"12","12","Lead",9.9384180481309079E-6,"lb/MMBtu",9.3360896815775207E-5,"lb/MW","ERT","",229]
["Dale Station",1385,"3","03","Lead",7.9858090548354225E-6,"lb/MMBtu",9.4232546847057994E-5,"lb/MW","ERT","",230]
["Wabash River",1010,"4","4","Lead",9.3567572274526789E-6,"lb/MMBtu",9.6030998524576703E-5,"lb/MW","ERT","",231]
["Cane Run",1363,"5","CR5","Lead",7.9696261345471283E-6,"lb/MMBtu",9.6075824450728367E-5,"lb/MW","ERT","",232]
["Conesville",2840,"3","CV-3","Lead",8.9236214152106476E-6,"lb/MMBtu",1.0070171560680137E-4,"lb/MW","ERT","",233]
["George Neal North",1091,"3","3","Lead",1.112E-5,"lb/MMBtu",1.0514787193973636E-4,"lb/MW","Part II","1/20/2009-Pb",234]
["Prairie Creek",1073,"4","Unit 4","Lead",1.0200000000000001E-5,"lb/MMBtu",1.108037761294673E-4,"lb/MW","Part II","PC4-Metals-20060822",235]
["James River Power Station",2161,"5","Unit_5_JRPS","Lead",1.1602750101604313E-5,"lb/MMBtu",1.1160740573924147E-4,"lb/MW","ERT","",236]
["Titus",3115,"2","TI-2","Lead",1.1583333333333333E-5,"lb/MMBtu",1.2093967517401391E-4,"lb/MW","Part II","T-57",237]
["Walter Scott Jr. Energy Center",1082,"3","3","Lead",1.2300000000000001E-5,"lb/MMBtu",1.2380392156862745E-4,"lb/MW","Part II","6/2009 PB",238]
["Muscatine #1",1167,"9","9","Lead",1.3732896876394519E-5,"lb/MMBtu",1.4374547898539448E-4,"lb/MW","Part II","Lead Emission Test - Unit 9",239]
["Fair Station",1218,"2","U2","Lead",1.406595960705729E-5,"lb/MMBtu",1.4865161857458272E-4,"lb/MW","ERT","",240]
["Colver Power Project",10143,"AAB01","AAB01","Lead",1.7142462641593176E-5,"lb/MMBtu",1.575536261105205E-4,"lb/MW","ERT","",241]
["H L Spurlock Station",6041,"3","Unit 03","Lead",1.9948050917260171E-5,"lb/MMBtu",1.6623375764383477E-4,"lb/MW","ERT","",242]
["George Neal North",1091,"1","1","Lead",1.8600000000000001E-5,"lb/MMBtu",1.7484000000000003E-4,"lb/MW","Part II","1/13/2010-PB",243]
["Albright Power Station",3942,"1","Unit_1","Lead",1.8070963647676376E-5,"lb/MMBtu",1.7535527687745226E-4,"lb/MW","ERT","",244]
["Riverbend",2732,"7","7","Lead",1.8077179878870228E-5,"lb/MMBtu",1.9239933157511125E-4,"lb/MW","ERT","",245]
["Urquhart",3295,"URQ3","URQ003","Lead",2.0752044690123493E-5,"lb/MMBtu",2.1114701781795557E-4,"lb/MW","ERT","",246]
["Lake Road",2098,"6","6","Lead",2.1752342087897486E-5,"lb/MMBtu",2.1532621460747009E-4,"lb/MW","ERT","",247]
["R.M. Schahfer",6085,"14","R.M.0014","Lead",2.268628043318657E-5,"lb/MMBtu",2.2540855558614861E-4,"lb/MW","ERT","",248]
["Elrama Power Plant",3098,"4","ELR4-2","Lead",3.700713554373244E-5,"lb/MMBtu",3.8427409394329741E-4,"lb/MW","ERT","",249]
["Elrama Power Plant",3098,"3","ELR3-2","Lead",3.700713554373244E-5,"lb/MMBtu",3.8576238090786693E-4,"lb/MW","ERT","",250]
["Fair Station",1218,"1","U1","Lead",2.9E-5,"lb/MMBtu",3.906122448979592E-4,"lb/MW","Part II","MET05U1",251]
["Fair Station",1218,"1","U1","Lead",9.6000000000000002E-5,"lb/MMBtu",1.293061224489796E-3,"lb/MW","Part II","MACT06U1",251]
["Elrama Power Plant",3098,"2","ELR2-2","Lead",3.700713554373244E-5,"lb/MMBtu",4.6406947971840476E-4,"lb/MW","ERT","",252]
["Elrama Power Plant",3098,"1","ELR1-2","Lead",3.700713554373244E-5,"lb/MMBtu",4.6406947971840476E-4,"lb/MW","ERT","",253]
["O H Hutchings",2848,"H-5","H-5","Lead",5.7199999999999994E-5,"lb/MMBtu",5.8198730158730153E-4,"lb/MW","Part II","2009 H-5 EF trail baseline metals",254]
["James River Power Station",2161,"4","Unit_4_JRPS","Lead",2.8104613840999014E-3,"lb/MMBtu",2.8104613840999014E-2,"lb/MW","ERT","",255]

{"sheet":"Pb_New_Sub1UPL Pooled Template ","index":2,"n_rows":116,"n_cols":12,"rows_kept":116,"cut":false,"hidden":false,"merged":[[0,1,0,11],[37,0,37,3]]}
[null,"Emissions (lb/MW)"]
["Runs","4078\nWeston\nBoiler 4"]
[1,1.9989931070496084E-5]
[2,1.5397649608355089E-5]
[3,6.3931761531766744E-6]
[4,7.9673601118429955E-7]
[5,9.150941351949091E-7]
[6,9.7767682126365728E-7]
[7]
[8]
[9]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]
[32]
[33]
[34]
[35]
["Use for large sample sets and small sample sets that are Normal."]
[]
["Testing Normality","Raw Data"]
["Sample Size",{"$f":"COUNT(B3:L37)","v":6}]
["Kurtosis",{"$f":"KURT(B3:L37)","v":-1.3309597584980875},null,"Because only had two test averages, used the run by run data from each test.  Changing m=1 to m=3."]
["SE Kurtosis",{"$f":"SQRT((B41^2-1)/((B41-3)*(B41+5)))","v":1.0298573010888745}]
["Result Kurtosis",{"$f":"IF(ABS(B42/B43)>NORMSINV(1-0.05/2),\"non normal\",\"normal\")","v":"normal"}]
["Skewness",{"$f":"SKEW(B3:L37)","v":0.8531465561900804}]
["SE Skewness",{"$f":"SQRT((6*B41*(B41-1))/((B41-2)*(B41+1)*(B41+3)))","v":0.84515425472851657}]
["Result Skewness",{"$f":"IF(ABS(B45/B46)>NORMSINV(1-0.05/2),\"non normal\",\"normal\")","v":"normal"}]
[]
[]
["ni = number test runs =",{"$f":"COUNT(B3:B37)","v":6},0,0,0,0,0,0,0,0,0,0]
[]
["Total Number of sources =",{"$f":"COUNTA(B2:L2)","v":1}]
[]
[]
["n =Total # test runs =",{"$f":"SUM(B50:L50)","v":6}]
[]
[]
[]
[]
[null,{"$f":"B55-1","v":5}]
[]
[]
[]
[]
["This step is for QC only:"]
[]
["means",{"$f":"AVERAGE(B3:B37)","v":7.4117106332784507E-6},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[]
[]
[]
[]
[]
[null,{"$f":"AVERAGE(B3:L37)","v":7.4117106332784507E-6}]
["Mean ="]
[]
[]
[]
["Pooled Variance = ",null,null,{"$f":"VAR(B3:L37)","v":7.0076993887262832E-11}]
[]
[]
[]
[]
[]
["m= number future runs =",3]
[]
[]
["Term1",{"$f":"1/B55+1/B85","v":0.5}]
[]
[]
[]
["Term2",{"$f":"D79*B88","v":3.5038496943631416E-11}]
[]
[]
[]
[]
[]
["Squared root Term2",null,{"$f":"SQRT(B92)","v":5.9193324744967163E-6}]
[]
[]
["NOTE: the pvalue for the t-statistic is calculated as: 2*alpha, where 1-alpha is desired confidence, so if 99% confidence is desired then alpha=0.01 and 2*alpha=2*(0.01)"]
[]
[]
["t-statistic","= quantile t-distribution with df degrees of freedom at .99 confidence level =",null,null,null,null,null,{"$f":"TINV(2*0.01,B60)","v":3.3649299989072183}]
[]
[]
["UPL  POOLED VARIANCE = ",null,null,null,null,{"$f":"B74+H104*C98","v":2.7329850050218148E-5},"lb/MW"]
[null,null,null,null,null,{"$f":"F107*1000","v":2.7329850050218148E-2},"lb/GW"]
[]
[]
[]
[]
[null,null,null,null,"3xRDL ",2E-3,"lb/GW"]
[]
[]
[null,null,null,null,"3xRDL compared to UPL",{"$f":"IF(F113<F108,F108,F113)","v":2.7329850050218148E-2}]

{"sheet":"Pb_QA_Calcs","index":3,"n_rows":114,"n_cols":101,"rows_kept":114,"cut":false,"hidden":false,"merged":[[8,0,8,4],[8,6,8,18],[8,20,8,26],[8,28,8,36],[8,38,8,45]]}
[null,null,null,null,null,null,null,null,"Anthracite",null,"Anthracite",null,null,"fPM","30B",null,"μg/dscm","No",null,"μg/dscm",{"$f":"1/453592370","v":2.2046226218487758E-9},"lbs/μg",2.8316846592000001E-2,null,null,null,"cm/cf",null,null,null,null,null,"lb/hr",null,null,"lb/MMBtu",null,null,null,null,null,null,null,"Round to",null,null,null,"From ",null,"original database export===>"]
[null,null,null,null,null,null,null,null,"Bituminous",null,"Bituminous",null,null,"Se","M5",null,"lb/dscf","Yes",null,"ppm",{"$f":"U1/1000","v":2.2046226218487757E-12},"lb/mg",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Same ",null,null,null,"Min ",null,"original database export===>"]
[null,null,null,null,null,null,null,null,"Lignite",null,"Lignite",null,null,"Pb","M5B",null,"ppm",null,null,null,null,"lb/scf",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sig Figs ",null,null,null,"Test",null,"original database export===>"]
[null,null,null,null,null,null,null,null,"Oil",null,"Oil",null,null,"Hg","M29",null,"ppm @ 3% O2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"as Submitted",null,null,null,"Sheet",null,"original database export===>"]
[null,null,null,null,null,null,null,null,"Pet Coke",null,"Pet Coke",null,null,"HCl","OTM27",null,"ppm @ 7% O2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"prior to ",null,null,null,null,null,"original database export===>"]
[null,null,null,null,null,null,null,null,"Subbituminous",null,"Sub Bituminous",null,null,"SO2","26A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Calc % Diff.",null,null,null,null,null,"original database export===>"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"M6C",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"original database export===>"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"original database export===>"]
["RTI",null,null,null,null,null,"As Submitted",null,null,null,null,null,null,null,null,null,null,null,null,null,"RTI-QA",null,null,null,null,null,null,null,"As Submitted",null,null,null,null,null,null,null,null,null,"RTI-QA",null,null,null,null,null,null,null,"Final for UPL",null,"Final for UPL","original database export===>","Key","RTI Calculated QA\nlb/MMBtu","Run Grade","Submitted Value","Submitted Value UOM","Use ?","Comment","facility_id","configuration_id","report_id","sampling_port_id","order","pollutant_id","pollutant_name","run_id","start_datetime","end_datetime","unit_load","fuel_flow_rate","fuel_heating_value","fg_moisture_content","fg_oxygen_content","fg_CO2_content","fg_temperature","test_method","conc","conc_units","conc_ND","conc_MDL","conc2","conc2_units","emission_rate","emission_rate_units","emission_rate_ND","emission_rate_MDL","Calculated conc lb/dscf","19-1\nlb/MMBtu","%Diff\n19-1","19-6\nlb/MMBtu","%Diff\n19-6","emission_factor","emission_factor_units","emission_factor_ND","emission_factor_MDL","run_pollutant_comment","Fuel1","Fuel1%Btu","Fuel2","Fuel2%Btu","QA Comment"]
["Comments",null,"Use Run in UPL Calc?","Grade","Key","Facility_Name","Facility_ID","Boiler_ID","Fuel1 Used","Fuel1 Fraction","Fuel2 Used","Fuel2 Fraction","\"Fuel Used/Fraction\" Data Source","Pollutant","Reference Method","Concentration","Concentration UOM","Non-Detect?","MDL","MDL UOM","HAP Conversion Value to lbs","HAP Conversion UOM","Volume Conversion Value to cubic feet","Reserve","Reserve","Reserve","Volume Conversion UOM","Submitted F Factor","Bws (percent)","%O2d","%CO2d","Emission Rate Value","Emission Rate UOM","Emission Rate MDL","Emission Factor Value","Emission Factor UOM","Emission Factor MDL","MDL UOM","Fd","Fw","Fc","Calculated conc lb/dscf","19-1\nlb/MMBtu","%diff\n19-1","19-6\nlb/MMBtu","%diff\n19-6","lb/MMBtu Value Used for UPL Calcs","Unit Heat Rate (MMBtu/MWh)","lb/MWh Value Used in UPL Calcs","original database export===>",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"average"]
[null,null,"Yes","A","1_Pb_T2_R1","Weston","4078","W4","Subbituminous",1,null,null,"Part II Submittal","Pb","M29",{"$f":"BX11","v":2.855},"μg/dscm","No",null,null,{"$f":"1/453592370","v":2.2046226218487758E-9},"lbs/μg",2.8316846592000001E-2,null,null,null,"cm/cf",null,{"$f":"BS11","v":15.6},{"$f":"BT11","v":4.7},{"$f":"BU11","v":16.600000000000001},{"$f":"CD11","v":0.01},"lb/hr",null,{"$f":"CM11","v":2.2200000000000003E-6},"lb/MMBtu",null,null,{"$f":"VLOOKUP(I11,$A$98:$E$114,3,FALSE)","v":9820},{"$f":"VLOOKUP(I11,$A$98:$E$114,4,FALSE)","v":0},{"$f":"VLOOKUP(I11,$A$97:$E$114,5,FALSE)","v":1840},{"$f":"P11*U11*W11","v":1.7823182744489288E-10},{"$f":"IF(AD11<>\"\",AP11*AM11*20.9/(20.9-AD11),\"no O2 data for run\")","v":2.2580212222922792E-6},{"$f":"(AQ11-$AI11)/$AI11","v":1.7126676708233729E-2},{"$f":"IF(AE11<>\"\",AP11*AO11*100/AE11,\"no CO2 data for run\")","v":1.9755817017988124E-6},{"$f":"(AS11-$AI11)/$AI11","v":-0.11009833252305762},{"$f":"AI11","v":2.2200000000000003E-6},9.0044734551784149,{"$f":"AU11*AV11","v":1.9989931070496084E-5},"original database export===>","1_Pb_T2_R1",{"$f":"CI14","v":"AvgOfStackTemp"},"A",{"$f":"CM11","v":2.2200000000000003E-6},{"$f":"CN11","v":"pound per million British Thermal Unit (lb/MMBtu)"},"Yes",null,4078,"W4","W4 Metals 2008","W4 Port",6,23,"Lead (Pb)","1","2008-07-11T07:40:00","2008-07-11T09:50:00",null,null,null,15.6,4.7,16.600000000000001,176.3,"29",2.855,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,"",0.01,"pound per hour (lb/hr)",false,null,null,null,null,null,null,2.2200000000000003E-6,"pound per million British Thermal Unit (lb/MMBtu)",false,null,"","coal - subbituminous",100,null,null,null,{"$f":"AVERAGE(AW11:AW13)","v":1.3926918944009281E-5}]
[null,null,"Yes","A","1_Pb_T2_R2","Weston","4078","W4","Subbituminous",1,null,null,"Part II Submittal","Pb","M29",{"$f":"BX12","v":2.1960000000000002},"μg/dscm","No",null,null,2.2046226218487758E-9,"lbs/μg",2.8316846592000001E-2,null,null,null,"cm/cf",null,{"$f":"BS12","v":15.8},{"$f":"BT12","v":4.7},{"$f":"BU12","v":14.6},{"$f":"CD12","v":0.01},"lb/hr",null,{"$f":"CM12","v":1.7099999999999999E-6},"lb/MMBtu",null,null,{"$f":"VLOOKUP(I12,$A$98:$E$114,3,FALSE)","v":9820},{"$f":"VLOOKUP(I12,$A$98:$E$114,4,FALSE)","v":0},{"$f":"VLOOKUP(I12,$A$97:$E$114,5,FALSE)","v":1840},1.3709180142521358E-10,1.7368177247474066E-6,{"$f":"(AQ12-$AI12)/$AI12","v":1.5682879969243658E-2},1.7277322919341983E-6,{"$f":"(AS12-$AI12)/$AI12","v":1.036976136502827E-2},{"$f":"AI12","v":1.7099999999999999E-6},9.0044734551784149,1.5397649608355089E-5,"original database export===>","1_Pb_T2_R2",{"$f":"#REF!","v":{"$error":"#REF!"}},"A",{"$f":"CM12","v":1.7099999999999999E-6},"pound per million British Thermal Unit (lb/MMBtu)","Yes",null,4078,"W4","W4 Metals 2008","W4 Port",6,23,"Lead (Pb)","2","2008-07-11T10:07:00","2008-07-11T12:16:00",null,null,null,15.8,4.7,14.6,178.1,"29",2.1960000000000002,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,"",0.01,"pound per hour (lb/hr)",false,null,null,null,null,null,null,1.7099999999999999E-6,"pound per million British Thermal Unit (lb/MMBtu)",false,null,"","coal - subbituminous",100]
[null,null,"Yes","A","1_Pb_T2_R3","Weston","4078","W4","Subbituminous",1,null,null,"Part II Submittal","Pb","M29",0.91600000000000004,"μg/dscm","No",null,null,2.2046226218487758E-9,"lbs/μg",2.8316846592000001E-2,null,null,null,"cm/cf",null,15.2,4.7,14.6,null,null,null,{"$f":"CM13","v":7.0999999999999998E-7},"lb/MMBtu",null,null,9820,0,1840,5.7184011887748469E-11,7.2446495258134077E-7,2.0373172649775759E-2,7.2067521831135061E-7,1.5035518748381167E-2,7.0999999999999998E-7,9.0044734551784149,6.3931761531766744E-6,"original database export===>","1_Pb_T2_R3",{"$f":"CI15","v":0},"A",7.0999999999999998E-7,"pound per million British Thermal Unit (lb/MMBtu)","Yes",null,4078,"W4","W4 Metals 2008","W4 Port",6,23,"Lead (Pb)","3","2008-07-11T12:25:00","2008-07-11T14:35:00",null,null,null,15.2,4.7,14.6,178.6,"29",0.91600000000000004,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,"",0,"pound per hour (lb/hr)",false,null,null,null,null,null,null,7.0999999999999998E-7,"pound per million British Thermal Unit (lb/MMBtu)",false,null,"","coal - subbituminous",100]
[null,null,null,null,null,"Weston",null,"W4",null,null,null,null,null,null,"M27",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,9.0044734551784149,null,"original database export===>","Key","RTI Calculated QA\nlb/MMBtu","Run Grade","Submitted Value","Submitted Value UOM","Use ?","Comment","facility_id","configuration_id","submittal_id","Compound","RunDate","Method","RunNumber","RunStartTime","RunEndTime","NetTravPts","Mass_TOOL","mass","units","Vmstd","Cd","Vwstd","PercH20","PercCO2","PercO2","Fd","19-1","19-5","Fc","19-6","19-9","Fw","FuelType","lb/mmBtuO2","CountOfComments","AvgOfStackTemp","AvgOfDryGasInlet","AvgOfDryGasOutlet","AvgOfOrificePresDesired","AvgOfOrificePresActual","AvgOfProbeTemp","AvgOfFilterTemp","AvgOfImpingTemp","CountOfNotes","M29 Isokinetic (+/- 10%)","OTM27 includes all fractions?","QA Comment","Questions for EPA"]
[null,null,null,null,null,"Weston",null,"W4",null,null,null,null,null,null,"M28",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,9.0044734551784149,null,"original database export===>",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DSCF","lb/dscf"]
[null,null,"Yes","A",{"$f":"AY16","v":"1_Pb_T1_R1"},"Weston",4078,"W4","Subbituminous",null,null,null,"ERT","Pb","M29",{"$f":"BT16","v":6.8903068165930623E-12},"lb/dscf",null,null,null,null,null,null,null,null,null,null,{"$f":"BY16","v":9423},{"$f":"BV16","v":"15.69"},{"$f":"BX16","v":5.55},{"$f":"BW16","v":13.75},null,null,null,{"$f":"CG16","v":8.8482243314971603E-8},"lb/MMBtu",null,null,9820,0,1840,{"$f":"P16","v":6.8903068165930623E-12},{"$f":"IF(AD16<>\"\",AP16*AM16*20.9/(20.9-AD16),\"no O2 data for run\")","v":9.2127217617193927E-8},{"$f":"(AQ16-$AI16)/$AI16","v":4.1194415576097598E-2},{"$f":"IF(AE16<>\"\",AP16*AO16*100/AE16,\"no CO2 data for run\")","v":9.2204833036590791E-8},{"$f":"(AS16-$AI16)/$AI16","v":4.2071601963885895E-2},{"$f":"AI16","v":8.8482243314971603E-8},9.0044734551784149,{"$f":"AU16*AV16","v":7.9673601118429955E-7},"original database export===>","1_Pb_T1_R1",8.8402726232873577E-8,"A",8.8482243314971603E-8,"lb/mmBtuO2","Yes",null,4078,"W4",1611,"Lead","2010-05-11","Method 29","M5/29-1","08:30","15:52",48,5.5000000000000003E-4,0.55000000000000004,"ug","175.820",6.8903068165930623E-12,"32.72","15.69",13.75,5.55,9423,8.8402726232873577E-8,7.45323384869357E-8,0,0,0,0,"",8.8482243314971603E-8,52,177.47916666666666,68.5625,61.208333333333336,1.7950640989015376,1.8208333333333331,237.125,249.79166666666666,51.729166666666664,52,101,null,null,null,null,{"$f":"AVERAGE(AW16:AW18)","v":8.9650232254762201E-7}]
[null,null,"Yes","A",{"$f":"AY17","v":"1_Pb_T1_R2"},"Weston",4078,"W4","Subbituminous",null,null,null,"ERT","Pb","M29",{"$f":"BT17","v":7.6246641699751544E-12},"lb/dscf",null,null,null,null,null,null,null,null,null,null,{"$f":"BY17","v":9430},{"$f":"BV17","v":"15.73"},{"$f":"BX17","v":6.1},{"$f":"BW17","v":13.4},null,null,null,{"$f":"CG17","v":1.0162661256651763E-7},"lb/MMBtu",null,null,9820,0,1840,{"$f":"P17","v":7.6246641699751544E-12},{"$f":"IF(AD17<>\"\",AP17*AM17*20.9/(20.9-AD17),\"no O2 data for run\")","v":1.0573451519711897E-7},4.0421524705574495E-2,{"$f":"IF(AE17<>\"\",AP17*AO17*100/AE17,\"no CO2 data for run\")","v":1.0469688113995734E-7},3.0211265493377815E-2,{"$f":"AI17","v":1.0162661256651763E-7},9.0044734551784149,9.150941351949091E-7,"original database export===>","1_Pb_T1_R2",1.015352829235063E-7,"A",1.0162661256651763E-7,"lb/mmBtuO2","Yes",null,4078,"W4",1611,"Lead","2010-05-12","Method 29","M5/29-2","08:00","13:30",48,5.8600000000000004E-4,0.58599999999999997,"ug","169.286",7.6246641699751544E-12,"31.59","15.73",13.4,6.1,9430,1.015352829235063E-7,8.556378291963876E-8,0,0,0,0,"",1.0162661256651763E-7,52,177.72916666666666,68.458333333333329,60.125,1.6701706873282498,1.6729166666666673,245.89583333333334,250.33333333333334,48.208333333333336,52,100.3]
[null,null,"Yes","A","1_Pb_T1_R3","Weston",4078,"W4","Subbituminous",null,null,null,"ERT","Pb","M29",8.2485924942470549E-12,"lb/dscf",null,null,null,null,null,null,null,null,null,null,9596,"16.06",5.65,13.65,null,null,null,1.085767897623599E-7,"lb/MMBtu",null,null,9820,0,1840,8.2485924942470549E-12,1.1101145090716571E-7,2.2423403290284326E-2,1.1118981823746947E-7,2.4066179160653497E-2,1.085767897623599E-7,9.0044734551784149,{"$f":"AU18*AV18","v":9.7767682126365728E-7},"original database export===>","1_Pb_T1_R3",1.0847921414512853E-7,"A",1.085767897623599E-7,"lb/mmBtuO2","Yes",null,4078,"W4",1611,"Lead","2010-05-13","Method 29","M5/29-3","07:55","13:15",48,6.4400000000000004E-4,0.64400000000000002,"ug","171.969",8.2485924942470549E-12,"32.90","16.06",13.65,5.65,9596,1.0847921414512853E-7,9.1057452353420902E-8,0,0,0,0,"",1.085767897623599E-7,52,178.22916666666666,72.3125,65.0625,1.7330845712404599,1.7375,249.875,250.04166666666666,48.625,52,100.8]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Conversions"]
[1,null,"ppm SO2=",1.66E-7,"lb/scf"]
[1,null,"ppm Hg=",{"$f":"D98*A104/A105","v":5.1979300655635339E-7},"lb/scf"]
[1000,null,"mg=",1,"g"]
[1000000,null,"ug=",1,"g"]
[454,null,"g=",1,"lb"]
[1,null,"m^3=",35.314500000000002,"ft^3"]
[200.59,null,"Hg molecular weight"]
[64.06,null,"SO2 molecular weight"]
[]
["Table 19-2",null,"Fd","Fw","Fc"]
["Fuel Type",null,"dscf/MMBtu","wscf/MMBtu","scf/MMBtu"]
["Coal"]
["Anthracite",null,10100,10540,1970]
["Bituminous",null,9780,10640,1800]
["Lignite",null,9860,11950,1910]
["Oil",null,9190,10320,1420]
["Subbituminous",null,9820,null,1840]

{"sheet":"ERT","index":4,"n_rows":11,"n_cols":49,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Key","RTI Calculated QA\nlb/MMBtu","Run Grade","Submitted Value","Submitted Value UOM","Use ?","Comment","facility_id","configuration_id","submittal_id","Compound","RunDate","Method","RunNumber","RunStartTime","RunEndTime","NetTravPts","Mass_TOOL","mass","units","Vmstd","Cd","Vwstd","PercH20","PercCO2","PercO2","Fd","19-1","19-5","Fc","19-6","19-9","Fw","FuelType","lb/mmBtuO2","CountOfComments","AvgOfStackTemp","AvgOfDryGasInlet","AvgOfDryGasOutlet","AvgOfOrificePresDesired","AvgOfOrificePresActual","AvgOfProbeTemp","AvgOfFilterTemp","AvgOfImpingTemp","CountOfNotes","M29 Isokinetic (+/- 10%)","OTM27 includes all fractions?","QA Comment","Questions for EPA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DSCF","lb/dscf"]
["1_Pb_T1_R1",{"$f":"AB3","v":8.8402726232873577E-8},"A",{"$f":"AI3","v":8.8482243314971603E-8},{"$f":"$AI$1","v":"lb/mmBtuO2"},"Yes",null,4078,"W4",1611,"Lead","2010-05-11","Method 29","M5/29-1","08:30","15:52",48,5.5000000000000003E-4,0.55000000000000004,"ug","175.820",{"$f":"S3/$H$10/$H$11/U3","v":6.8903068165930623E-12},"32.72","15.69",13.75,5.55,9423,{"$f":"V3*AA3*20.9/((20.9-Z3))","v":8.8402726232873577E-8},{"$f":"V3*AA3*20.9/((20.9-Z3)/(1-X3/100))","v":7.45323384869357E-8},0,{"$f":"V3*AD3/Y3","v":0},{"$f":"V3*AD3*(1-X3/100)*100/Y3","v":0},0,"",8.8482243314971603E-8,52,177.47916666666666,68.5625,61.208333333333336,1.7950640989015376,1.8208333333333331,237.125,249.79166666666666,51.729166666666664,52,101]
["1_Pb_T1_R2",{"$f":"AB4","v":1.015352829235063E-7},"A",{"$f":"AI4","v":1.0162661256651763E-7},{"$f":"$AI$1","v":"lb/mmBtuO2"},"Yes",null,4078,"W4",1611,"Lead","2010-05-12","Method 29","M5/29-2","08:00","13:30",48,5.8600000000000004E-4,0.58599999999999997,"ug","169.286",{"$f":"S4/$H$10/$H$11/U4","v":7.6246641699751544E-12},"31.59","15.73",13.4,6.1,9430,1.015352829235063E-7,8.556378291963876E-8,0,0,0,0,"",1.0162661256651763E-7,52,177.72916666666666,68.458333333333329,60.125,1.6701706873282498,1.6729166666666673,245.89583333333334,250.33333333333334,48.208333333333336,52,100.3]
["1_Pb_T1_R3",1.0847921414512853E-7,"A",1.085767897623599E-7,"lb/mmBtuO2","Yes",null,4078,"W4",1611,"Lead","2010-05-13","Method 29","M5/29-3","07:55","13:15",48,6.4400000000000004E-4,0.64400000000000002,"ug","171.969",{"$f":"S5/$H$10/$H$11/U5","v":8.2485924942470549E-12},"32.90","16.06",13.65,5.65,9596,1.0847921414512853E-7,9.1057452353420902E-8,0,0,0,0,"",1.085767897623599E-7,52,178.22916666666666,72.3125,65.0625,1.7330845712404599,1.7375,249.875,250.04166666666666,48.625,52,100.8]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Header tab comments",null,null,null,null,null,null,null,null,"Point tab notes"]
[null,null,null,null,null,null,null,"Conversions Used"]
[null,null,null,null,null,null,null,1000,"mg=",1,"g"]
[null,null,null,null,null,null,null,1000000,"ug=",1,"g"]
[null,null,null,null,null,null,null,454,"g=",1,"lb"]

{"sheet":"4078_PartII","index":5,"n_rows":28,"n_cols":50,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["Key","RTI Calculated QA\nlb/MMBtu","Run Grade","Submitted Value","Submitted Value UOM","Use ?","Comment","facility_id","configuration_id","report_id","sampling_port_id","order","pollutant_id","pollutant_name","run_id","start_datetime","end_datetime","unit_load","fuel_flow_rate","fuel_heating_value","fg_moisture_content","fg_oxygen_content","fg_CO2_content","fg_temperature","test_method","conc","conc_units","conc_ND","conc_MDL","conc2","conc2_units","emission_rate","emission_rate_units","emission_rate_ND","emission_rate_MDL","Calculated conc lb/dscf","19-1\nlb/MMBtu","%Diff\n19-1","19-6\nlb/MMBtu","%Diff\n19-6","emission_factor","emission_factor_units","emission_factor_ND","emission_factor_MDL","run_pollutant_comment","Fuel1","Fuel1%Btu","Fuel2","Fuel2%Btu","QA Comment"]
["1_Pb_T2_R1",{"$f":"AK5","v":2.2468150506464255E-6},"A",{"$f":"AO2","v":2.2200000000000003E-6},{"$f":"AP2","v":"pound per million British Thermal Unit (lb/MMBtu)"},"Yes",null,4078,"W4","W4 Metals 2008","W4 Port",6,23,"Lead (Pb)","1","2008-07-11T07:40:00","2008-07-11T09:50:00",null,null,null,15.6,4.7,16.600000000000001,176.3,"29",2.855,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,"",0.01,"pound per hour (lb/hr)",false,null,null,null,null,null,null,2.2200000000000003E-6,"pound per million British Thermal Unit (lb/MMBtu)",false,null,""]
["1_Pb_T2_R2",{"$f":"AK6","v":1.7281981965742734E-6},"A",{"$f":"AO3","v":1.7099999999999999E-6},{"$f":"AP3","v":"pound per million British Thermal Unit (lb/MMBtu)"},"Yes",null,4078,"W4","W4 Metals 2008","W4 Port",6,23,"Lead (Pb)","2","2008-07-11T10:07:00","2008-07-11T12:16:00",null,null,null,15.8,4.7,14.6,178.1,"29",2.1960000000000002,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,"",0.01,"pound per hour (lb/hr)",false,null,null,null,null,null,null,1.7099999999999999E-6,"pound per million British Thermal Unit (lb/MMBtu)",false,null,""]
["1_Pb_T2_R3",7.208695574052978E-7,"A",7.0999999999999998E-7,"pound per million British Thermal Unit (lb/MMBtu)","Yes",null,4078,"W4","W4 Metals 2008","W4 Port",6,23,"Lead (Pb)","3","2008-07-11T12:25:00","2008-07-11T14:35:00",null,null,null,15.2,4.7,14.6,178.6,"29",0.91600000000000004,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,"",0,"pound per hour (lb/hr)",false,null,null,null,null,null,null,7.0999999999999998E-7,"pound per million British Thermal Unit (lb/MMBtu)",false,null,""]
[null,null,null,null,null,null,null,4078,"W4","W4 Metals 2008","W4 Port",null,null,"Lead (Pb)","1","2008-07-11T07:40:00","2008-07-11T09:50:00",null,null,null,15.6,4.7,16.600000000000001,176.3,"29",2.855,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,null,null,null,null,null,{"$f":"Z2/$H$16/$H$17/$J$18","v":1.7807264028958666E-10},{"$f":"AJ5*$I$26*20.9/(20.9-V5)","v":2.2468150506464255E-6},{"$f":"($AO2-AK5)/$AO2","v":-1.2078851642533837E-2},{"$f":"AJ5*$K$26*100/W2","v":1.9309081477184093E-6},{"$f":"(AO2-AM5)/AO2","v":0.13022155508179772},2.2200000000000002,"pound per trillion British Thermal Unit (lb/1012Btu)",false,null,null,"coal - subbituminous",100,null,null,"lb/10^12Btu conversion"]
[null,null,null,null,null,null,null,4078,"W4","W4 Metals 2008","W4 Port",null,null,"Lead (Pb)","2","2008-07-11T10:07:00","2008-07-11T12:16:00",null,null,null,15.8,4.7,14.6,178.1,"29",2.1960000000000002,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,null,null,null,null,null,{"$f":"Z3/$H$16/$H$17/$J$18","v":1.3696935834533531E-10},{"$f":"AJ6*$I$26*20.9/(20.9-V6)","v":1.7281981965742734E-6},{"$f":"($AO3-AK6)/$AO3","v":-1.0642220218873346E-2},{"$f":"AJ6*$K$26*100/W3","v":1.6886633220657778E-6},{"$f":"(AO3-AM6)/AO3","v":1.247758943521763E-2},1.71,"pound per trillion British Thermal Unit (lb/1012Btu)",false,null,null,"coal - subbituminous",100,null,null,"lb/10^12Btu conversion"]
[null,null,null,null,null,null,null,4078,"W4","W4 Metals 2008","W4 Port",null,null,"Lead (Pb)","3","2008-07-11T12:25:00","2008-07-11T14:35:00",null,null,null,15.2,4.7,14.6,178.6,"29",0.91600000000000004,"microgram per dry standard cubic meter (μg/dscm)",false,null,null,null,null,null,null,null,{"$f":"Z4/$H$16/$H$17/$J$18","v":5.7132938180476835E-11},{"$f":"AJ7*$I$26*20.9/(20.9-V7)","v":7.208695574052978E-7},{"$f":"($AO4-AK7)/$AO4","v":-1.5309235782109614E-2},{"$f":"AJ7*$K$26*100/W4","v":7.0437868989628968E-7},{"$f":"(AO4-AM7)/AO4","v":7.9173381742398564E-3},0.71,"pound per trillion British Thermal Unit (lb/1012Btu)",false,null,null,"coal - subbituminous",100,null,null,"lb/10^12Btu conversion"]
[]
[]
[null,null,null,null,null,null,null,"Data from eICR.  No test report provided."]
[]
[null,null,null,null,null,null,null,"Conversions"]
[null,null,null,null,null,null,null,1,"ppm SO2=",1.66E-7,"lb/scf"]
[null,null,null,null,null,null,null,1,"ppm Hg=",{"$f":"J13*H19/H20","v":5.1979300655635339E-7},"lb/scf"]
[null,null,null,null,null,null,null,1000,"mg=",1,"g"]
[null,null,null,null,null,null,null,1000000,"ug=",1,"g"]
[null,null,null,null,null,null,null,454,"g=",1,"lb"]
[null,null,null,null,null,null,null,1,"m^3=",35.314500000000002,"ft^3"]
[null,null,null,null,null,null,null,200.59,"Hg molecular weight"]
[null,null,null,null,null,null,null,64.06,"SO2 molecular weight"]
[]
[null,null,null,null,null,null,null,"Table 19-2","Fd","Fw","Fc"]
[null,null,null,null,null,null,null,"Fuel Type","dscf/MMBtu","wscf/MMBtu","scf/MMBtu"]
[null,null,null,null,null,null,null,"Coal"]
[null,null,null,null,null,null,null,"Anthracite",10100,10540,1970]
[null,null,null,null,null,null,null,"Bituminous",9780,40640,1800]
[null,null,null,null,null,null,null,"Lignite",9860,11950,1910]
[null,null,null,null,null,null,null,"Oil",9190,10320,1420]